Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 1 of 4
11/3/2010
Code Change Cycle:
2010 Triennial Original Modification 3/1/2010 ‑ 4/2/2010
Total Mods for this TAC:
Fire
TAC:
 10 
SubCode:
Building
9‑Fire Protection Systems
916
 3853 
Changes to Carbon Monoxide Protection
Steven Bassett
9
Comment
Commission Action: AM (Consent)*
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
X⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G2    ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Modified
10‑Means of Egress
1011.1
 3995 
Adopts the exit sign requirements of the base code (IBC).
J Glenn‑BASF
10
Comment
Commission Action: AM (Consent)*
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [A1/Y1 – N5     ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Modified
SubCode:
Residential
3‑Building Planning
311.7.9.1
 4123 
Retain base code (IRC) language
J Glenn‑BASF
3
Comment
Commission Action: AS (Consent)*
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [ test  ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
X⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [     ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
Consent  (*) = Mod taken under consent with vote of 23-0
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 2 of 4
11/3/2010
Total Mods for this TAC:
Fire
TAC:
 10 
R302.2
 4087 
The 2009 IRC assumes all townhomes are sprinklered. However, in cases where fire sprinklers are removed from the text the townhome common wall must be upgraded back to the 2 hr requirement (R317.2 ‑ 2006 IRC).
jeffrey collins
3
Comment
Commission Action: AM(A1) (23Y-0N)
X⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [A1/ Y6 – N2     ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
SubCode:
Building
6‑Types of Construction
602.2 &amp; 602.3
 3655 
The FBC conflicts with the Florida Fire Prevetion and Life Safety Code (FFPC) because it does not include &quot;limited‑combustible&quot; materials. The FBC must be modified to comform with the FFPC
Michael Wolfe
6
Comment
Commission Action: NAR (Consent)*
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G3  /Y1 – N6     ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
603
 3435 
The purpose of this code change is to add materials, as defined in Florida Fire Prevention Code (FFPC) (NFPA‑1/101), limited‑ combustible material, which includes gypsum wall board, to be used in Type II Non‑combustible Building.
Wenyi Zhang
6
Comment
Commission Action: NAR (Consent)*
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ A3/ Y1 – N6    ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
7‑Fire and Smoke Protection Features
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
Consent  (*) = Mod taken under consent with vote of 23-0
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 3 of 4
11/3/2010
Total Mods for this TAC:
Fire
TAC:
 10 
703.4
 3656 
The FBC conflicts with the Florida Fire Prevetion and Life Safety Code (FFPC) because it does not include &quot;limited‑combustible&quot; materials. The FBC must be modified to comform with the FFPC
Michael Wolfe
7
Comment
Commission Action: NAR (Consent)*
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G1/ Y-1 N6   ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
10‑Means of Egress
Section 1008
 3598 
Exempts lawn storage buildings and storage sheds not exceeding 400 square feet from minimum and maximum height and width requirements.
Kevin Crowley
10
Comment
Commission Action: NAR (Consent)*
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [A4-G2/Y 3- N4     ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
2711‑Administrative Provisions (Reserved)
New appendix
 4391 
Add a new Appendix “XX” (Designation to be assigned)
Doug Harvey
2711
Comment
Commission Action: NAR Consent)*
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G3-G4/Y0 – N7    ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
SubCode:
Residential
3‑Building Planning
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
Consent  (*) = Mod taken under consent with vote of 23-0
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 4 of 4
11/3/2010
Total Mods for this TAC:
Fire
TAC:
 10 
R305
 3662 
Exempts lawn storage buildings and storage sheds not exceeding 400 square feet from ceiling height requirements.
Kevin Crowley
3
Comment
Commission action: NAR (1Y-22N)
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]
⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [A2 – G3/ Y3 – N4      ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
Modification #:
Code Change Cycle:
Chapter & Topic:
Date Submitted From:
TAC:
Proponent Last Name:
Affects HVHZ:
Sub Code:
Code Version:
Commission Action:
Text of Modification:
Section:
Related Modifications:
TAC Recommendation:
Date Submitted To:
Proponent First Name:
2010
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
Search Criteria
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations