Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 1 of 11
11/3/2010
Code Change Cycle:
2010 Triennial Original Modification 3/1/2010 ‑ 4/2/2010
Total Mods for this TAC:
Energy
TAC:
 37 
SubCode:
Energy Conservation
2‑Definitions
202
 3714 
Add definitions for Absorptance, Multi‑Scene Control and Normative.
Ann Stanton
2
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G-1 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [  G1/  0-10  ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Modified
4‑Residential Energy Efficiency
403.2.1
 4197 
Needs to be in residential code because Manual D applies to Residential and Light commercial duct systems
Robert Volin
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G2 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G2 / 0-11    ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Modified
405.6
 4457 
This modification introduces the option for approved computing software energy compliance
Jack Glenn
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ A3, A1 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ A3  3-8, A1 8-3 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Modified
5‑Commercial Energy Efficiency
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 2 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
503
 4061 
Modification to reference (baseline) building HVAC equipment suppy and return fan power calculation
Mangesh Basarkar
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G2 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G2 /1-10 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Modified
505.6
 4467 
This modification introduces the option for approved computing software energy compliance
Jack Glenn
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ A4, A6 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ A4/ 8-3  A6/ 3-8 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Modified
10‑Appendix D
FL Std 3
 4077 
Provides criteria on how to comply w/ s. 403.9.5 of the FECC; the mandatory requirement for portable spas, per legislative directive. This document is the APSP‑14 draft Standard for Portable Spa Energy Efficiency that provides the test protocol manufacturers must use when determining standby power.
Jennifer Hatfield
10
Comment
X⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [ A2 ]	 ⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ A2/ 11-0 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Modified
SubCode:
Energy Conservation
1‑Administration
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 3 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
101.5.1
 3847 
Reserve code section that would allow the code official to accept software and other materials for code compliance that are not specified in the code.
Ann Stanton
1
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [  G1   ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G1/ 1-10     ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
3‑Design Criteria
303.2
 4433 
Add criteria for insulation installation from the appendices of the present Florida energy code that were inadvertently omitted from the Florida‑specific criteria included in the base code.
Ann Stanton
3
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [  G1   ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [  G1/ 0-11   ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
304
 4438 
Add criteria for determining thermal properties of building materials and assemblies.
Ann Stanton
3
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G1    ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [  G1/ 1-10   ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
4‑Residential Energy Efficiency
402.1.1
 4258 
Removing footnote From Table 402.1.1, language that does not apply to FL requirements.
Amy Schmidt
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G1    ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G1/ 0-11   ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 4 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
402.2.5
 3943 
Establishes equivalency table for steel framed wall assemblies with stud spacing at 24 inches.
Joe Nebbia
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G1    ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [  G1/ 0-11   ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
403.6, 403.6.1, 403.6.1.1
 4058 
None
Robert Volin
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	⁭x2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G1    ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [  G1 /0-11   ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
405
 4322 
Makes two section 405 EnergyGauge USA FlaRes water heater changes: 
1) Allow primary heat pump water heater entries and energy factor (EF) entries for primary and add‑on heat pump water heaters.  2) Internally modify water heater energy factors based on typical residential water draw profiles.
Jeff Sonne
4
Comment

⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [ ]  X⁭2. Do not support comment.  Comment does not address TAC's concerns(s) [ G1, G3, G4 G5, G6, G7, G8 ]
⁭x3. No comment is needed.     [G2 , G9 ]						⁭4. Straw poll:     [G1/ 4-7  G2, G3 /2-9  G4/ 0-11  G5/ 1-10  G6/ 4-7  G7/ 3-8   G8 /4-7 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
405
 4382 
Relaxes the window area‑weighed average maximum fenestration SHGC requirement for section 405 (performance) code compliance calculations in cases where the window area‑weighted average overhang depth for the entire dwelling unit is 4.0 feet or greater.
Jeff Sonne
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G2 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G2 / 0-10 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
5‑Commercial Energy Efficiency
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 5 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
502
 4060 
Propose new envelope prescriptive requirements for alterations and renovations
Mangesh Basarkar
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G2  ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G2 /0-11 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
503.2.3(10)
 3675 
Add performance requirements for heat rejection equipment back into the code that were not included in the IECC.
Ann Stanton
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [  G1   ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G1 / 0-11]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
503.2.3
 3673 
Add room air conditioners and room air conditioner heat pump requirements to Table 503.2.3(3).
Ann Stanton
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G1    ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G1/ 0-11 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
505.5.1.2.3
 3864 
Add Florida‑specific criteria for calculating luminaire wattage. Correct from Addenda i to ASHRAE 90.1‑04.
Ann Stanton
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [G1 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G1 / 0-11   ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
10‑Appendix D
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 6 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
FL Std 2
 4072 
Provides criteria on how to comply with section 403.9 of the FECC; parts of which are legislative directive.  This document is the APSP‑15 Draft Standard for Energy Efficiency for Residential Inground Swimming Pools &amp; Spas that the FBC Energy Workgroup recommended for adoption into the 2010 code
Jennifer Hatfield
10
Comment
x⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [A-1  ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [A1 /11-0 ]

Proponent
Summary
Mod #
Section
Chapter
Approved as Submitted
SubCode:
Building
2711‑Administrative Provisions (Reserved)
New appendix
 4391 
Add a new Appendix “XX” (Designation to be assigned)
Doug Harvey
2711
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G3, G4 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G3/ 0-11 , G4 /0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
SubCode:
Energy Conservation
2‑Definitions
Definitions
 4307 
Add permanent shading to chapter 2 definitions
Amanda Hickman
2
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [G7 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G7/ 0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
4‑Residential Energy Efficiency
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 7 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
402.1.1
 3956 
This proposal creates a second option for builders to install roofing materials with a solar reflectance over 0.10, as long as the area‑weighted average fenestration SHGC does not exceed 0.25.
Eric Lacey
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ A4 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ A4/ 0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
402.1.1
 3957 
This proposal increases energy efficiency, reduces peak demand and sizing of cooling systems, and improves comfort for building occupants by lowering the prescriptive fenestration SHGC value to 0.25.
Eric Lacey
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ A3 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ A3/ 0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
402.3.2.1 (NEW)
 4309 
Adds compliance paths for meeting SHGC values in table 402.1.1.
Amanda Hickman
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G7, G8  ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G7/ 0-11 G8 /0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
402.3.6
 4317 
The SHGC requirements for replacement fenestration in section 402.3.6 can be satisfied by new section 402.3.2.1 on Permanent Shading.
Amanda Hickman
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G8, G9 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G8/ 0-11 , G9/ 0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 8 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
402.5
 4320 
Delete entire section: 402.5 Maximum fenestration U‑factor and SHGC (Mandatory).
Amanda Hickman
4
Comment
x⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [ G7 ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [    ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G7/ 9-2 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
402
 4080 
Eliminate the “Total UA Alternative” residential energy code compliance method described in section 402.1.1.3.
Jeff Sonne
4
Comment
X⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [ G-5 ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G5/ 9-2 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
403.2.2.1
 3892 
Add exception per compliance with section 405
Roger Sanders
4
Comment
X⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G2 - G3  - G4 -  G5  - G6  - G7-G8-G9/ 9-2 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
403.2.2.1
 4463 
This modification reinstates the original air duct tightness provisions in the IECC.
Jack Glenn
4
Comment
⁭ 1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [   ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [A5, A1 ]

X⁭3. No comment is needed.     [ G1 ]						⁭4. Straw poll:     [A5/ 5-6 , A1/ 4-7 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 9 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
403.5.1
 4458 
This restores original IECC language for ventilation.
Jack Glenn
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [G1 ]

⁭3. No comment is needed.     [    ]						⁭4. Straw poll:     [G1/ 2-8]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
405.6, Table B‑1.1.2(1)
 3947 
This proposal removes trade‑offs that are not allowed under the 2009 IECC performance path, including the programmable thermostat credit, the cross‑ventilation and whole house fan options, and an oversimplified credit for thermal storage mass.
Eric Lacey
4
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [  G1   ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G3/ 3-8 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
5‑Commercial Energy Efficiency
502.1.1.1(1)&amp;(2)
 3919 
Coordinate Skylight U‑Factor and SHGC requirements with ASHRAE 90.1‑2007, in general.
Roger LeBrun
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [A1 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ A1 /0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
502.2.5.1.3 (New)
 4327 
Adds a new section: 502.2.5.1.3 on Permanent Shading through different compliance paths on how to meet the requirements of Table 502.1.1.1.
Amanda Hickman
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [ G7 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G7/ 0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 10 of 11
11/3/2010
Total Mods for this TAC:
Energy
TAC:
 37 
502.2.5
 4329 
502.2.5.1 Shell buildings, renovations and alterations can comply with related modifcation new section 502.2.5.1.3.
Amanda Hickman
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [  G7   ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [ G7 /0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
503.2.6
 4042 
Change outside air supply from 70% to 30%
Amanda Hickman
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	X⁭2 Do not support comment.  Comment does not address TAC's concerns(s)     [G1 ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G1 / 0-11  ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
503.2.7.1.1
 3717 
Eliminates the reduced insulation levels being introduced into the code.
Darrell Winters
5
Comment
⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [     ]	x⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [  G1   ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [G1 /0-11 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
506.3
 4293 
Addition of credit for use of Energy Ventilation (ERV) Systems in performance method
Mangesh Basarkar
5
Comment
X⁭1. Support comment.  Comment sufficiently addresses the TAC's concern(s).    [ A1  ]	⁭2. Do not support comment.  Comment does not address TAC's concerns(s)     [     ]

⁭3. No comment is needed.     [     ]						⁭4. Straw poll:     [A1/ 11-0 ]

Proponent
Summary
Mod #
Section
Chapter
No Affirmative Recommendation with a Second
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 11 of 11
11/3/2010
Modification #:
Code Change Cycle:
Chapter & Topic:
Date Submitted From:
TAC:
Proponent Last Name:
Affects HVHZ:
Sub Code:
Code Version:
Commission Action:
Text of Modification:
Section:
Related Modifications:
TAC Recommendation:
Date Submitted To:
Proponent First Name:
2010
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
Search Criteria
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations