Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 1 of 64
6/28/2010
Code Change Cycle:
2010 Triennial Original Modification 3/1/2010 ‑ 4/2/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
202
 3873 
Florida‑specific mod to IBC flood provisions. Sec. 1612 and CCCL Sec 3109 use “substantial improvement” with different dfns. . FL Div Emerg Mgnt will coordinate a group with FBC and DEP to consider changes for future cycle.
Rebecca Quinn
2
Comment

Proponent
Summary
Mod #
Section
Chapter
202
 3874 
Retain base code (IBC) language as it provides better direction.
J Glenn‑BASF
2
Comment

Proponent
Summary
Mod #
Section
Chapter
202
 4314 
Updates the definition of Habitable Space to include revised information from AAMA/NPEA/NSA 2100‑10 for sunrooms.  This document now defines a Category IV sunroom as a non‑habitable space.
Daniel Walker
2
Comment

Proponent
Summary
Mod #
Section
Chapter
202
 4332 
Includes Tubular Daylighting Devices in definition of unit skylights
Chuck Anderson
2
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 2 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
801.5
 3882 
Florida‑specific modifications to Chapter 8, related to retaining flood provisions of the I‑Codes which require materials below the DFE to be flood damage‑resistant materials specified in 1612.4 by reference to ASCE 24.
Rebecca Quinn
8
Comment

Proponent
Summary
Mod #
Section
Chapter
801.5
 4398 
Clarify the elevation below which flood damage‑resistant materials are required is the elevation specified in 1612.4.
Christopher Jones
8
Comment

Proponent
Summary
Mod #
Section
Chapter
1202.1
 4109 
The modifications clarify that roofs of sunrooms without sloped glazing are solid roofs and clarifies open areas are areas with operable windows or fixed glass or glass doors . The clarifications are needed to address confusion demonstrated during the permitting phase for sunroom projects.
Joseph Belcher
12
Comment

Proponent
Summary
Mod #
Section
Chapter
1203.3.2
 3986 
1. Delete Florida Specific amendment to 1203.3.2 and retain IBC language.
2. Change code reference to Chapter 13 of the Florida Building Code, Building
3. Retain exception #5 and renumber to #6.
J Glenn‑BASF
12
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 3 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1210.3
 3989 
Delete Florida Code language to 1210.2 and retain IBC language with the accessibility requirement in exception #2.
J Glenn‑BASF
12
Comment

Proponent
Summary
Mod #
Section
Chapter
1403.2
 3909 
Delete Florida Code language to 1403.2 and retain IBC language.
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1403.5
 3883 
Florida‑specific modifications to 1403.5, related to retaining flood provisions of the I‑Codes which require materials below the DFE to be flood damage‑resistant materials specified in 1612.4 by reference to ASCE 24.
Rebecca Quinn
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1403.5
 4399 
Clarify the elevation below which flood damage‑resistant materials are required is the elevation specified in 1612.4.
Christopher Jones
14
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 4 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1403.7
 3998 
Retain Florida Specific language
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1404
 3856 
Adds reference to new section on labeling of soffits.
Joseph Belcher
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1404.10
 3914 
Change 1404.10 to correct terminology and reference the proper type of material.
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1404.2
 3912 
Change 1404.2 to include language from IBC and add “Florida Specific language. Retain Florida Specific Language in Section 1404.2.1
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 5 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1404.9
 3913 
Change 1404.9 title to include soffit and to include language from IBC and add “Florida Specific language.” Retain Florida Specific Language in Section 1404.9.1
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1405
 4215 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition and introduces new ultimate design wind speed maps in the code.
T Stafford
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1405.1
 4466 
Proosal eliminates wind load provisions of AAMA 1402 which are contrary to the wind load provisions of the code.
Joseph Belcher
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1405.10
 4002 
Change 1405.10 to retain base code (IBC) language.
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 6 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1405.11.4
 4003 
Change 1405.11.4 to retain base code (IBC) language.
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1405.14.1
 4004 
Change 1405.14.1 to retain base code (IBC) language.
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1405.3.2
 3999 
Change 1405.3.2 to retain IBC language
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
1405.4
 4000 
Change 1405.4 to retain IBC language.
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 7 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1405.8
 4001 
Change 1405.8 to retain IBC language.
J Glenn‑BASF
14
Comment

Proponent
Summary
Mod #
Section
Chapter
New 1504.9
 4374 
The code currently requires that garden and lanscaped roofs be evlauated for wind resistance. This new section proposes a design guide to be used for this purpose.
Mike Ennis
15
Comment

Proponent
Summary
Mod #
Section
Chapter
1601.1, 1612
 3885 
Florida‑specific mods to Chpt 16, retain I‑Code flood provisions. Defines ‘local floodplain management ordinance’ where communities will adopt FIRMs and higher stnds for NFIP Community Rating System. FBC requested statutory authority so that local higher stnds do not sunset every 3 years.
Rebecca Quinn
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1602, 1603, 1605, 1609, 1620
 4214 
This proposal updates ASCE 7 to the 2010 Edition and introduces new ultimate design wind speed maps in the code.
T Stafford
16
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 8 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1602.1 Definitions
 3687 
Add the requirement that exterior mounted cooling towers, fluid coolers, and evaporative condensers, which are subjected to wind forces be designed as a structure, to the FBC Building Code, volume.
Mark Speckin
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1603.1.4 Wind design data
 3688 
Add the requirement that the wind load requirement of Other Structures in terms of psf be shown on the Construction Documents
Mark Speckin
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1609.1
 3857 
Adds reference to new section on Soffit labeling.
Joseph Belcher
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1609.1.1
 4177 
This modification deletes language that, due to a glitch in ASCE 7, could result in low and erroneous roof uplift pressures for higher sloped roofs.
T Stafford
16
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 9 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1609.1.2
 3677 
This section is modified to imply that all openings into a roof structure, whether vertical or horizontal, need to be protected in the event of a hurricane or high event from debris as well as wind and rain. This will reduce structural, wind, water, and personal belonging damage in such an event.
Michael Hemmer
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1609.1.2
 4232 
The proposal adds and Exception from impact protection for screen or removable vinyl and acrylic wind panels on exterior balconies and porches.
Joseph Belcher
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1609.1.2.1
 4033 
Adds to standard to section 1609.1.2.1 Louvers. Louvers protecting intake and exhaust ventilation
Amanda Hickman
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1609.1.3
 4447 
Delete section 1609.1.3 in its entirety without substitution.
Kurt Roeper
16
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 10 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1609.4.3
 3665 
Clarify the intent of Section 1609.4.3 with regard to the 20% increase in uplift load regarding roof‑to‑wall connection.
Mo Madani
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1612
 3891 
Florida‑specific modifications to Chapter 16, related to retaining flood provisions of the I‑Codes.  The Flood Resistant Standards Workgroup recommended a table to show where all flood provisions are located.
Rebecca Quinn
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1612.5
 4397 
Modifies a provision to be consistent with NFIP, ASCE 7, and ASCE 24, to use language that is consistent with structural design and loads.
Christopher Jones
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1618.4.6.1 and 1618.4.6.2
 3664 
Coordinate structural design criteria for pedestrian guards and handrails between HVHZ and non‑HVHZ for non‑wind related loading.
Thomas Sputo
16
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 11 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1618.4.6.3
 3725 
Correlates the HVHZ requirements on use of laminated glazing for glass railings used in the wind borne debris region with those of the 2009 IBC.
Jaime Gascon
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1618.9
 3841 
Clarification of required design Flood Loads of ASCE 7
Mohammed Shaikh
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1620
 4143 
ASCE 7‑05 commentary states that high uplift may exist on rooftop equipment, but no methodology is given. Load calculations may vary by a large factor based on two methods given. This modification is to eliminate such differences and include uplift and revised lateral forces based on FIU research.
Arindam Gan Chowdhury
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1622
 4331 
The modification adds design wind pressures for aluminum screened enclosures developed from wind tunnel testing sponsored by the Aluminum Association of Florida.
Joseph Belcher
16
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 12 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1622.1
 4296 
Modification proposes use of AAF Guide to Aluminum Construction in High Wind Areas by designers in the HVHZ.
Joseph Belcher
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1626.1
 4347 
Adds provisions allowing the enclosure of balconies or porches with screen or removable vinyl or acrylic panels with invoking opening protection requirments.
Joseph Belcher
16
Comment

Proponent
Summary
Mod #
Section
Chapter
Table 1609.7(1)
 3650 
Wind load values have been revised based on ASCE 7‑10 provisions.
Joseph Hetzel
16
Comment

Proponent
Summary
Mod #
Section
Chapter
1714.5.3.3.2
 4448 
Delete section 1714.5.3.3.2 in its entirety without substitution.
Kurt Roeper
17
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 13 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1715.5.3
 3631 
Moves section 1715.5.3.3.1 on glazed curtain wall, window wall and storfront systems to a new section 1715.5.6; moves remaining 'exception' in 1715.5.3.3.1 to 1715.5.3 Exterior Door Assemblies.
Jaime Gascon
17
Comment

Proponent
Summary
Mod #
Section
Chapter
1715.5.3.3.1
 4179 
This section deals with glazed curtain walls, window wall and storefront systems; it is currently hidden as a subsection of a section on door components.  This modification is simply to move it.
Chuck Anderson
17
Comment

Proponent
Summary
Mod #
Section
Chapter
1715.9
 3231 
Establishes installation criteria (manufacturer's installation instructions), requires instructions available for inspector, provides for interchangeability of components, fastners, etc., specifies C&amp;C loads in accordance with 1609.1.1, and specifies factor of safety for testing.
Joseph Belcher
17
Comment

Proponent
Summary
Mod #
Section
Chapter
1715.9
 3689 
This modification is designed for the language set forth in Section 1715.8 to be consistant with regards to opening protection on soffit vents in Hurricane Prone Areas.
Michael Hemmer
17
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 14 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1715.9
 3855 
Adds labeling requirements for soffits.
Joseph Belcher
17
Comment

Proponent
Summary
Mod #
Section
Chapter
1716.1
 4411 
Delete sec. 1716.1 in its entirety since referenced standard, D1761, is not relevant to joist hangers &amp; content is in ASTM D 7147‑05 so that should be referenced in sec. 2303.5.
Stuart Lewis
17
Comment

Proponent
Summary
Mod #
Section
Chapter
1801.1
 3457 
Exception in 1801.1 Scope is proposed to revise as follows
Exception: Buildings and and structures located within the high‑velocity hurricane zone shall comply with the provisions of Sections 1816 through 1834 and 1805
Mohammed Shaikh
18
Comment

Proponent
Summary
Mod #
Section
Chapter
1801.1, 1804.4
 3887 
Florida‑specific modifications to Chapter 18, related to retaining flood provisions of the I‑Codes.
Rebecca Quinn
18
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 15 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1808.2 Design for capacity and settlement
 3606 
Upon identification of weak soils or soils having the possibility of differential settlement, require a design statement regarding either the remediation of the soils or indication within the building plan that the foundation system is designed with the understanding of the geologically hazard.
timothy moore
18
Comment

Proponent
Summary
Mod #
Section
Chapter
1816.1.7
 3872 
Modify 1816.1.7 regarding the use of approved termite baits for new construction termite control to agree with FSS Chapter 482 which establishes requirements for new construction termite control contracts.  Modification would change requirement for 5 year contract to 1 year plus 4 renewal years.
Sid Funk
18
Comment

Proponent
Summary
Mod #
Section
Chapter
1910.2
 4469 
Proposal adds additiona fiber materials and adopts a new Acceptance Criteria.
Joseph Belcher
19
Comment

Proponent
Summary
Mod #
Section
Chapter
2002.2
 3467 
This change updates the aluminum construction standard referenced to 2010.
John Kissell
20
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 16 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2002.4
 4216 
Proposal reduces concentrated load on purlins from 300 # to the OSHA required load for fixed ladders, 200#. The reduction applies to purlins only.
Joseph Belcher
20
Comment

Proponent
Summary
Mod #
Section
Chapter
2002.6
 4279 
Proposal to clarify wind load design criteria for sunrooms and to clarify intent of inclusion of AAMA Categories for sunrooms in code.
Joseph Belcher
20
Comment

Proponent
Summary
Mod #
Section
Chapter
2002.6
 4312 
This code change proposal updates the sunroom categories to be consistent with the revised edition of AAMA/NPEA/NSA 2100‑10.
Daniel Walker
20
Comment

Proponent
Summary
Mod #
Section
Chapter
2003.1, 2003.2, 2003.3
 3455 
This proposed modification updates the references for HVHZ aluminum construction to the 2010 Aluminum Design Manual.
John Kissell
20
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 17 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2003.9
 4345 
The proposal adds provisions for sunrooms in the HVHZ section of the code.
Joseph Belcher
20
Comment

Proponent
Summary
Mod #
Section
Chapter
2107.1
 4063 
Further modifies Florida Specific Amendment related to inspection and lap splice provisions of TMS 402/ACI 530/ ASCE 5 and TMS 602/ACI 530.1/ ASCE 6 to make them current with 2008 Editions of the documents.
Joseph Belcher
21
Comment

Proponent
Summary
Mod #
Section
Chapter
2107.5
 4064 
Updates existing Florida Specific Amendment to incorporate section and equation number changes of TMS 402/ACI 530/ASCE 5‑2008.
Joseph Belcher
21
Comment

Proponent
Summary
Mod #
Section
Chapter
2108.1
 4065 
Updates references in an existing Florida Specific Amendment to account for changes in the referenced document.
Joseph Belcher
21
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 18 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2109
 4218 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition and introduces new ultimate design wind speed maps in the code.
T Stafford
21
Comment

Proponent
Summary
Mod #
Section
Chapter
2114.2
 4066 
Changes the order of the organizations developing the masonry standards to agree with the foundation code.
Joseph Belcher
21
Comment

Proponent
Summary
Mod #
Section
Chapter
2122
 4135 
The modification updates the HVHZ provisions for the design and construction of reinforced unit masonry.
Joseph Belcher
21
Comment

Proponent
Summary
Mod #
Section
Chapter
1615.3, 2222.4.4
 4370 
The proposal revises the requirements for the deflection of structural roofing and siding made of formed metal sheets to be more consistent with current testing requirements in the Florida Building Code.  The proposal also removes a reference to this requirement that is redundant in Chapter 22.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 19 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2209.2.1
 3459 
Add additional current reference standard for composite steel deck design.
Thomas Sputo
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2214 and 2222
 3460 
Update versions of design references for HVHZ within Sections 2214 and 2222.
Thomas Sputo
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2214.3
 3633 
Section 2214.3 requiires modification due to adoption of Manual of Steel Construction Thirteenth edition
Mohammed Shaikh
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2218.3
 3365 
2218.3 Welding in the shop or field may only be done by AWS certified welders.
The code should read “AWS qualified” or “a welder whom has successfully performed a qualification test, per AWS D1.1 protocol and administered by an AWS certified welding inspector (CWI).
scott wilson
22
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 20 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2218.3
 4248 
The proposal cleans up vague code language and more appropriately references the welder qualification requirements of the AWS Code rather than AWS certification of welders.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2222.3.3
 4241 
The proposal deletes a subsection in the cold‑formed steel construction section that belongs only in Section 2223.10 with respect to metal building systems.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2222.3.3 and 2223.10.1
 3597 
Cables and Rods shall not be used as bracing in Cold ‑Formed and Pre‑Engineered steel buildings. This proposal is to delete the word &quot;habitable&quot; from these two sections of the code.
Mohammed Shaikh
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2222.3.4
 4251 
The proposal deletes a subsection in the cold‑formed steel construction section that belongs only in Section 2223.10 with respect to metal building systems.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 21 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2223.1, 2223.2, 2223.3, 2223.4, 2223.5, 2223.6
 4290 
The proposal updates responsibilities and document requirements for metal building systems to match the FL Board of Professional Engineers updated regulations with respect to engineers of record and delegated engineers.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2223.10.1
 4274 
This proposal seeks to clarify the intent of the applicability of the restriction on cables and rod bracing in metal buildings.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2223.10.2; 2223.10.5
 4276 
This proposal removes outdated terminology with respect to this form of construction.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2223.10.4
 4278 
This proposal deletes a redundant section that is already covered elsewhere in the code.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 22 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2223.11
 4246 
This proposal updates the certification requirement in Section 2223.11.2 to the new IAS AC472 accreditation program that replaced the discontinued AISC, Category MB Program.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2223.11.1
 4243 
This proposal would eliminate the requirements for inspections of metal building systems.  While inspections can serve a useful purpose, it is  inconsistent to require special inspections of metal building systems when other construction types are not subjected to this same scrutiny.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2223.8.2
 4282 
This proposal deletes an unnecessary requirement that is covered by other required design standards.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2223.8.3
 4284 
This proposal deletes an unnecessary requirement that is covered by other required design standards.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 23 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2223.8.4
 4288 
This proposal deletes redundant requirements that are covered by other sections in the code.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
Ch. 17 and 2223.11
 4244 
This proposal seeks to put more specificity into what the inspection requirements are in Section 2223.11.1 by invoking the appropriate inspection requirements of Chapter 17 of the IBC.
William Shoemaker
22
Comment

Proponent
Summary
Mod #
Section
Chapter
2303.5
 4414 
Replace reference to section 1716.1 with reference to ASTM D7147, which replaces all content of section 1716.1.
Stuart Lewis
23
Comment

Proponent
Summary
Mod #
Section
Chapter
2304, 2308
 4219 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition and introduces new ultimate design wind speed maps in the code.
T Stafford
23
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 24 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2304.11.6
 3931 
Using base code language for termite protection.
J Glenn‑BASF
23
Comment

Proponent
Summary
Mod #
Section
Chapter
2314.0
 4107 
This proposal updates the currently referenced standards to their current editions.  In addition, it adds the ANSI/AF&amp;PA Special Design Provisions for Wind and Seismic (SDPWS‑2008).
Paul Coats
23
Comment

Proponent
Summary
Mod #
Section
Chapter
2404.1
 3928 
Using base code language for Loads on vertical glass.
J Glenn‑BASF
24
Comment

Proponent
Summary
Mod #
Section
Chapter
2411.1
 3580 
This modification moves section 2411.3.3.7 on the requirements for 'exterior safety glazed lite', to a new section ‑ 2411.1 General.
Jaime Gascon
24
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 25 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
2411.1.10
 3470 
Delete Section 2411.1.10
William Dumbaugh
24
Comment

Proponent
Summary
Mod #
Section
Chapter
2411.1.11
 3668 
The modification clarifies that 'comparative' analysis is allowed, as opposed to the used term 'rational' analysis when the fixed glazing product differs from the one approved.
Jaime Gascon
24
Comment

Proponent
Summary
Mod #
Section
Chapter
2603.8
 3930 
Using base code language for termite protection for foam plastic.
J Glenn‑BASF
26
Comment

Proponent
Summary
Mod #
Section
Chapter
2603.8
 3962 
Using base code language for termite protection for foam plastic.
J Glenn‑BASF
26
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 26 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
3105.1
 3961 
Use base code language for awning provisions
J Glenn‑BASF
31
Comment

Proponent
Summary
Mod #
Section
Chapter
3109
 4416 
Change language in the Code in relation to working within the CCCL.
James Battaglia
31
Comment

Proponent
Summary
Mod #
Section
Chapter
3109
 4434 
Clarifies language regarding exceptions to 100 year storm event design standards.
George Merlin
31
Comment

Proponent
Summary
Mod #
Section
Chapter
3109.1.1
 4203 
Modification corrects a formatting error in the 2007 Florida Building Code relating to construction of structures seaward of the coastal construction control line (CCCL).
Jack Glenn
31
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 27 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
3109.2
 4234 
Add statutory definition for &quot;Substantial improvement&quot; to the code.
Jack Glenn
31
Comment

Proponent
Summary
Mod #
Section
Chapter
3113.1
 3574 
When required by local government to reduce noise attenuation in new structure or addition to existing structure near an airport, applicant must provide documentation that structure meets the reduction requirement.
Kevin Gartland
31
Comment

Proponent
Summary
Mod #
Section
Chapter
3113.1 and R325.1
 3511 
When required by local government to reduce noise attenuation in new structure or addition to existing structure near an airport, applicant must provide documentation that structure meets the reduction requirement.
Kevin Gartland
31
Comment

Proponent
Summary
Mod #
Section
Chapter
3304.1.4
 3959 
Restore reference to 1804.5 as the correct reference. Section 1803.5 Deals with soil investigation while Section 1804.5 deals with compacted fill. Delete the special inspector language.
J Glenn‑BASF
33
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 28 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
1.0
 4099 
This proposed modification updates the referenced standards to the latest versions referenced in the 2009 IBC, and corrects some out of date references.
Paul Coats
35
Comment

Proponent
Summary
Mod #
Section
Chapter
2002.4.1
 4285 
change AAF Guide to Construction in High Wind Areas from 2007 edition to 2010 edition
David Miller
35
Comment

Proponent
Summary
Mod #
Section
Chapter
35
 4264 
Updates AAMA referenced standards, ASTM glass and impact standards.
Chuck Anderson
35
Comment

Proponent
Summary
Mod #
Section
Chapter
3501
 3890 
Modification to correct citations to Code of Federal Regulations.
Rebecca Quinn
35
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 29 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
3501
 4220 
This modification updates ASCE 7 to the 2010 Edition.
T Stafford
35
Comment

Proponent
Summary
Mod #
Section
Chapter
AA
 3458 
This proposed modification updates the references for aluminum construction from the 2005 Aluminum Design Manual to the 2010 Aluminum Design Manual.
John Kissell
35
Comment

Proponent
Summary
Mod #
Section
Chapter
AAMA
 4310 
This code change proposal updates the reference to AAMA/NPEA/NSA 2100 from 2002 to 2010.
Daniel Walker
35
Comment

Proponent
Summary
Mod #
Section
Chapter
AISC
 3638 
Chapter 35 AISC requires modification due to adoption of Manual of steel construction Thirteenth edition
Mohammed Shaikh
35
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 30 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
ASTM
 4417 
Add ASTM D 7147‑05, update D1761‑06 line.
Stuart Lewis
35
Comment

Proponent
Summary
Mod #
Section
Chapter
Referenced Standards
 4034 
Add AMCA 540 to Chapter 35 ‑ Referenced Standards
Amanda Hickman
35
Comment

Proponent
Summary
Mod #
Section
Chapter
Referenced Standards
 4341 
Adds a reference to a new section addressing the use of the AAF Guide to Aluminum Construction in High Wind Areas in the HVHZ.
Joseph Belcher
35
Comment

Proponent
Summary
Mod #
Section
Chapter
Referenced Standards
 4350 
Delete organization.
Joseph Belcher
35
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 31 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Building
SDI ANSI A250.13
 4449 
Delete ANSI A250.13 as a referenced standard
Kurt Roeper
35
Comment

Proponent
Summary
Mod #
Section
Chapter
New appendix
 4391 
Add a new Appendix “XX” (Designation to be assigned)
Doug Harvey
2711
Comment

Proponent
Summary
Mod #
Section
Chapter
SubCode:
Existing Building
202
 3901 
Florida‑specific mods to retain I‑Code flood provisions. Defines ‘local floodplain management ordinance’ where communities will adopt FIRMs and higher stnds for NFIP Community Rating System. FBC requested statutory authority so that local higher stnds do not sunset every 3 years.
Rebecca Quinn
2
Comment

Proponent
Summary
Mod #
Section
Chapter
506.2
 4419 
Adds clarity about non‑structural damage repairs.
James Battaglia
5
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 32 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Existing Building
606.5
 4233 
The proposal adds and Exception from impact protection for screen or removable vinyl and acrylic wind panels on exterior balconies and porches and relocates the HVHZ provision as an Exception.
Joseph Belcher
6
Comment

Proponent
Summary
Mod #
Section
Chapter
611.8.1.
 3512 
Notes are taken from Table R802.2.9.1 and are necessary to determine the actual uplift based on the roof span and overhang.
Jack Glenn
6
Comment

Proponent
Summary
Mod #
Section
Chapter
611.8.1.4
 4470 
Changes fastener specification for connector to that recommended by the manufacturer.
Randall Shackelford
6
Comment

Proponent
Summary
Mod #
Section
Chapter
611.8.1.6
 4471 
Changes fastener specification for connector to that recommended by the manufacturer.
Randall Shackelford
6
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 33 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Existing Building
1605
 4444 
New provisions are added to specify uplift loads for gable rake overhang outlookers.
T Stafford
16
Comment

Proponent
Summary
Mod #
Section
Chapter
SubCode:
Mechanical
401.5
 4035 
Adds new standard: AMCA 550 to section 401.5
Amanda Hickman
4
Comment

Proponent
Summary
Mod #
Section
Chapter
501.2.2
 4037 
Add AMCA 550 to section 501.2.2
Amanda Hickman
5
Comment

Proponent
Summary
Mod #
Section
Chapter
Referenced Standards
 4036 
Add AMCA 550 to Referenced Standards
Amanda Hickman
15
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 34 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
202
 3895 
Florida‑specific mods to retain I‑Code flood provisions. Defines ‘local floodplain management ordinance’ where communities will adopt FIRMs and higher stnds for NFIP Community Rating System. FBC requested statutory authority so that local higher stnds do not sunset every 3 years.
Rebecca Quinn
2
Comment

Proponent
Summary
Mod #
Section
Chapter
202 Accessible
 4014 
Retain base code (IRC) language as it provides better direction
J Glenn‑BASF
2
Comment

Proponent
Summary
Mod #
Section
Chapter
202 Basic wind speed
 4015 
Retain base code (IRC) language as it provides better direction.
J Glenn‑BASF
2
Comment

Proponent
Summary
Mod #
Section
Chapter
202 Live load.
 4016 
Retain base code (IRC) language as it provides better direction.
J Glenn‑BASF
2
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 35 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
202 Shear Wall
 4019 
Retain base code (IRC) language.
J Glenn‑BASF
2
Comment

Proponent
Summary
Mod #
Section
Chapter
R202
 4110 
Clarifies terms related to roofs and to open areas. Current language has caused confusion at the permitting phase of sunroom construction projects.
Joseph Belcher
2
Comment

Proponent
Summary
Mod #
Section
Chapter
R202
 4221 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition.
T Stafford
2
Comment

Proponent
Summary
Mod #
Section
Chapter
R202
 4313 
Updates the definition of Habitable Space to include revised information from AAMA/NPEA/NSA 2100‑10 for sunrooms.  This document now defines a Category IV sunroom as a non‑habitable space.
Daniel Walker
2
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 36 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
301.2
 4199 
This proposal updates the component and cladding loads table for consistency with ASCE 7‑05.
T Stafford
3
Comment

Proponent
Summary
Mod #
Section
Chapter
301.2.1.1
 4198 
Retain base code (IRC) language
J Glenn‑BASF
3
Comment

Proponent
Summary
Mod #
Section
Chapter
301.2.1.4.3
 4196 
Language is redundant as the exposure categories are previously defined
J Glenn‑BASF
3
Comment

Proponent
Summary
Mod #
Section
Chapter
301.2.2.4.2
 4194 
Add base code (IRC) language for clarity
J Glenn‑BASF
3
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 37 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
301.3
 4097 
Retain the base code (IRC) language.
J Glenn‑BASF
3
Comment

Proponent
Summary
Mod #
Section
Chapter
308.6.1
 4336 
Includes Tubular Daylighting Devices in definition of unit skylights
Chuck Anderson
3
Comment

Proponent
Summary
Mod #
Section
Chapter
308.6.9
 4192 
Retain base code (IRC) language
J Glenn‑BASF
3
Comment

Proponent
Summary
Mod #
Section
Chapter
316.5.12
 4118 
Retain base code (IRC) language
J Glenn‑BASF
3
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 38 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
318.4
 4106 
Retain base code (IRC) language
J Glenn‑BASF
3
Comment

Proponent
Summary
Mod #
Section
Chapter
318.4
 4116 
Retain base code (IRC) language.
J Glenn‑BASF
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301
 4222 
This modification updates ASCE 7 to the 2010 Edition and introduces an ultimate design wind speed map.
T Stafford
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.1
 3863 
Exception in section  R301.1 is proposed to be revised  to include Section R406 Foundation Dampproofing and Waterproofing  of Non – HVHZ, since there is no provision in HVHZ.
Mohammed Shaikh
3
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 39 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R301.1, 322.1.4, 322.1.7 &amp; 322.1.9
 3896 
Florida‑specific modifications to Chapter 3, related to retaining flood provisions of the I‑Codes.  Clarifies that structures seaward of the CCCL must also comply with R322 if also located in a flood hazard area.
Rebecca Quinn
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.2.1.1
 4108 
This modification replaces the outdated WPPC Guide to Wood Construction in High Wind Areas with the similar AF&amp;PA WFCM Guide to Wood Construction in High Wind Areas.
Paul Coats
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.2.1.1
 4348 
Updates the name of the organization responsible for the document.
Joseph Belcher
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.2.1.1.2
 4298 
This code change proposal updates the sunroom categories to be consistent with the revised edition of AAMA/NPEA/NSA 2100‑10.
Daniel Walker
3
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 40 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R301.2.1.1.2
 4346 
Clarifies the application of AAMA 2100 and that the design is in accordance with the wind speeds and wind loads of the Florida Building Code.
Joseph Belcher
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.2.1.2
 3667 
This section is modified to imply that all openings into a roof structure whether vertical or horizontal need to be protected in the event of a hurricane or high wind event from debris as well as wind and rain. This will reduce structrual, wind, water, and personal belonging damage in such an event.
Michael Hemmer
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.2.1.4
 3666 
Clarify the intent of Section R301.2.1.4 with regard to the 20% increase in uplift load regarding roof‑to‑wall connection.
Mo Madani
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.2.4.1, R322.1.1
 4404 
Allow use of ASCE 24 as an alternative in any flood hazard area, including A zones (see R322.2).
Christopher Jones
3
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 41 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R301.2.4.1, R322.1.1
 4406 
Allow use of ASCE 24 as an alternative in Coastal A zones (where such areas are delineated, see R322.2).
Christopher Jones
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.3, R301.5
 4204 
This modification deletes the prescriptive construction requirements in the code that do not apply to the design of buildings in Florida.
T Stafford
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R322.2.4 and R322.3.3.1 (new)
 3897 
Florida‑specific modifications to the flood provisions retained in the residential code, to add provisions for pools that are found in Appendix G of the IRC.  The Workgroup recommended moving the provisions into the body of the code.
Rebecca Quinn
3
Comment

Proponent
Summary
Mod #
Section
Chapter
R322.3.3
 4395 
Add NFIP‑requirement that elevated buildings in V zones are to have the area underneath “free of obstruction.”
Christopher Jones
3
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 42 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R325.1
 3575 
When required by local government to reduce noise attenuation in new structure or addition to existing structure near an airport, applicant must provide documentation that structure meets the reduction requirement.
Kevin Gartland
3
Comment

Proponent
Summary
Mod #
Section
Chapter
Table R301.2(3)
 3651 
Wind load values have been revised based on ASCE 7‑10 provisions.
Joseph Hetzel
3
Comment

Proponent
Summary
Mod #
Section
Chapter
401.1
 4093 
Retain base code (IRC) language
J Glenn‑BASF
4
Comment

Proponent
Summary
Mod #
Section
Chapter
401.2
 4094 
Retain base code (IRC) language
J Glenn‑BASF
4
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 43 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
403.1
 4095 
Retain base code (IRC) language
J Glenn‑BASF
4
Comment

Proponent
Summary
Mod #
Section
Chapter
R401, R404
 4223 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition.
T Stafford
4
Comment

Proponent
Summary
Mod #
Section
Chapter
R401.1
 3898 
Second sentence in R401.1 requires foundations to meet the rqmts of R322 in addition to Chpt 4; thus #2 in the exception is not necessary.  Other proposals for Chpt 44 will require meeting the rqmts of R322 if structures in HVHZ are also in flood hazard areas.
Rebecca Quinn
4
Comment

Proponent
Summary
Mod #
Section
Chapter
R402.4.2 Compressible or shifting soil
 4280 
Upon identification of weak soils or soils having the possibility of differential settlement, require a design statement regarding either the remediation of the soils or indication within the building plan that the foundation system is designed with the understanding of the geologically hazard.
timothy moore
4
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 44 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R404
 4205 
This modification is a correlation with the proposed modifcation that deletes the prescriptive construction requirements in the code that do not apply to the design of buildings in Florida.
T Stafford
4
Comment

Proponent
Summary
Mod #
Section
Chapter
501 and 502
 3904 
Removes section which is applicable to areas with wind speeds less than 100 mph. Also reinstate I‑code format and reserve sections which are not applicable to FL. This will eliminate confusion and misuse of the code sections which are not applicable.
Jon Caudill
5
Comment

Proponent
Summary
Mod #
Section
Chapter
R502
 4224 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition.
T Stafford
5
Comment

Proponent
Summary
Mod #
Section
Chapter
R502, R503, R505
 4206 
This modification deletes the prescriptive construction requirements in the code that do not apply to the design of buildings in Florida.
T Stafford
5
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 45 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R506.2.5
 4472 
Updates referenced organization and adds new ICC Acceptance Criteris.
Joseph Belcher
5
Comment

Proponent
Summary
Mod #
Section
Chapter
602
 4032 
Removes section which is applicable to areas with wind speeds less than 100 mph. Also reinstate I‑code format and reserve sections which are not applicable to FL. This will eliminate confusion and misuse of the code sections which are not applicable.
Jon Caudill
6
Comment

Proponent
Summary
Mod #
Section
Chapter
606.14.1
 4103 
Retain base code (IRC) language
J Glenn‑BASF
6
Comment

Proponent
Summary
Mod #
Section
Chapter
606.8.1
 4102 
Retain base code (IRC) language
J Glenn‑BASF
6
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 46 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
609.1.2
 4098 
Retain base code (IRC) language
J Glenn‑BASF
6
Comment

Proponent
Summary
Mod #
Section
Chapter
609.1.4
 4104 
Retain base code (IRC) language
J Glenn‑BASF
6
Comment

Proponent
Summary
Mod #
Section
Chapter
609.1.5
 4105 
Retain base code (IRC) language
J Glenn‑BASF
6
Comment

Proponent
Summary
Mod #
Section
Chapter
612.6.1
 4193 
Retain base code (IRC) language
J Glenn‑BASF
6
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 47 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R602, R603, R604, R605, R611
 4207 
This modification deletes the prescriptive construction requirements in the code that do not apply to the design of buildings in Florida.
T Stafford
6
Comment

Proponent
Summary
Mod #
Section
Chapter
R602, R603, R606, R607, R608, R609, R611
 4225 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition.
T Stafford
6
Comment

Proponent
Summary
Mod #
Section
Chapter
R612.1
 3578 
Clarifies that the structural installation of windows and doors is part of the structural design and construction of walls and partitions as provided for in Chapter 6 of the FBC and IRC.
Dick Wilhelm
6
Comment

Proponent
Summary
Mod #
Section
Chapter
R612.11.4 [was FL613.7.5] Installation instruction
 3579 
ASTME2112 does not address Florida Specific CMU/stucco walls. Language is permissive.
Dick Wilhelm
6
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 48 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R616
 3582 
Strikes prescriptive language which will be contained in its entirety in FMA/AAMA 100‑07, Standard Practice for the Installation of Windows with Flanges or Mounting Fins in Wood Frame Construction.
Dick Wilhelm
6
Comment

Proponent
Summary
Mod #
Section
Chapter
R617
 3858 
Adds labeling requirements for manufactured soffit sytems.
Joseph Belcher
6
Comment

Proponent
Summary
Mod #
Section
Chapter
R617.4
 3860 
Adds installation criteria, addresses permited substitution of components, parts, or fasteners, specifies factor of safety for testing.
Joseph Belcher
6
Comment

Proponent
Summary
Mod #
Section
Chapter
702.3.4
 4038 
Retain base code (IRC) language as it provides better direction
J Glenn‑BASF
7
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 49 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
703.1
 4040 
Retain the base code (IRC) language while delteing the Florida Specific Amendment.
J Glenn‑BASF
7
Comment

Proponent
Summary
Mod #
Section
Chapter
703.10
 4044 
Retain the base code (IRC) language.
J Glenn‑BASF
7
Comment

Proponent
Summary
Mod #
Section
Chapter
703.10
 4124 
Retain base code (IRC) language
J Glenn‑BASF
7
Comment

Proponent
Summary
Mod #
Section
Chapter
703.11
 4045 
Retain base code (IRC) language.
J Glenn‑BASF
7
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 50 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
703.11
 4200 
This proposal establishes a proper basis for vinyl siding applications with foam sheathing by applying appropriate adjustment factors to vinyl siding wind pressure rating.
T Stafford
7
Comment

Proponent
Summary
Mod #
Section
Chapter
703.4
 4041 
Retain base code (IRC) language as it provides better direction.
J Glenn‑BASF
7
Comment

Proponent
Summary
Mod #
Section
Chapter
R702
 4208 
This modification is a correlation with the modification that deletes the prescriptive construction requirements in the code that do not apply to the design of buildings in Florida.
T Stafford
7
Comment

Proponent
Summary
Mod #
Section
Chapter
R703
 4226 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition.
T Stafford
7
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 51 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R703.1.1
 3859 
Provids reference to new labeling requirements.
Joseph Belcher
7
Comment

Proponent
Summary
Mod #
Section
Chapter
R703.12.3
 4468 
Proosal eliminates wind load provisions of AAMA 1402 which are contrary to the wind load provisions of the code.
Joseph Belcher
7
Comment

Proponent
Summary
Mod #
Section
Chapter
R703.8 Flashing
 3584 
Defines who is responsible for flashing instructions while also clarifying that door and window installation be in accordance with manufacturer's instructions and window and door flashing in accordance to R703.8 adds by reference, FMA/AAMA and FMA/WDMA installation protocols.
Dick Wilhelm
7
Comment

Proponent
Summary
Mod #
Section
Chapter
802
 4165 
Revise Sec. 802 to reserve roof/ceiling design and construction criteria for wind loads less than 100 mph and return section numbering to that used in the IRC.
Ann Stanton
8
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 52 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
802.1.6.3
 4046 
Retain the base code (IRC) language.
J Glenn‑BASF
8
Comment

Proponent
Summary
Mod #
Section
Chapter
802.1.6.5
 4047 
Retain base code (IRC) language
J Glenn‑BASF
8
Comment

Proponent
Summary
Mod #
Section
Chapter
802.2
 4048 
Retain base code (IRC) language
J Glenn‑BASF
8
Comment

Proponent
Summary
Mod #
Section
Chapter
802.2.9.1
 4473 
Deletes prescriptive roof tiedown requirements for windspeeds higher than 100 mph.
Randall Shackelford
8
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 53 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
804.1.1
 4050 
Retain base code (IRC) language.
J Glenn‑BASF
8
Comment

Proponent
Summary
Mod #
Section
Chapter
806.4
 4051 
Retain base code (IRC) language.
J Glenn‑BASF
8
Comment

Proponent
Summary
Mod #
Section
Chapter
R802, R803, R804
 4209 
This modification deletes the prescriptive construction requirements in the code that do not apply to the design of buildings in Florida.
T Stafford
8
Comment

Proponent
Summary
Mod #
Section
Chapter
R802, R803, R804
 4227 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition.
T Stafford
8
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 54 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R4403
 4229 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition.
T Stafford
9
Comment

Proponent
Summary
Mod #
Section
Chapter
1307.2.1
 3869 
Add prescriptive for ground mounted units
Robert Cochell
13
Comment

Proponent
Summary
Mod #
Section
Chapter
1.0
 4155 
This proposal updates referenced AF&amp;PA standards to their current editions.
Paul Coats
43
Comment

Proponent
Summary
Mod #
Section
Chapter
4301
 3900 
Florida‑specific modifications related to retaining flood provisions of the I‑Codes.  This mod updates a reference to a FEMA publication and conforms the form of the references to the I‑Codes.
Rebecca Quinn
43
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 55 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
4301
 4392 
Correct and update references to FEMA technical bulletins.
Christopher Jones
43
Comment

Proponent
Summary
Mod #
Section
Chapter
4301
 4393 
Correct and update references to FEMA technical bulletins.
Christopher Jones
43
Comment

Proponent
Summary
Mod #
Section
Chapter
AAMA
 4301 
Updates reference from AAMA/NPEA/NSA 2100‑02 to AAMA/NPEA/NSA 2100‑10.
Daniel Walker
43
Comment

Proponent
Summary
Mod #
Section
Chapter
AAMA
 4306 
Updates reference from AAMA/NPEA/NSA 2100‑02 to AAMA/NPEA/NSA 2100‑10.
Daniel Walker
43
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 56 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
AISC
 3671 
New AISC reference standard is adopted tHirteenth edition manual ‑2005.
This mod. is proposed to delete old manual references
Mohammed Shaikh
43
Comment

Proponent
Summary
Mod #
Section
Chapter
Chapter 43
 3586 
Adds FMA/AAMA 100‑07, FMA/AAMA 200‑09 and FMA/WDMA 250‑10 installation protocols to Chapter 43, Referenced Standards.
Dick Wilhelm
43
Comment

Proponent
Summary
Mod #
Section
Chapter
NA
 4342 
Updates AAMA standards and ASTM impact standards
Chuck Anderson
43
Comment

Proponent
Summary
Mod #
Section
Chapter
R301.2.1.1
 4291 
Updating the 2007 edition of the AAF Guide to Aluminum Construction in High Wind Areas to the 2010 edition
David Miller
43
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 57 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R4301
 4231 
This modification updates ASCE 7 to the 2010 Edition.
T Stafford
43
Comment

Proponent
Summary
Mod #
Section
Chapter
Referenced Standards
 4340 
Corrects incorrect code citation and adds new reference to new section addressing the use of the AAF Guide to Aluminum Construction in High Wind Areas in the HVHZ.
Joseph Belcher
43
Comment

Proponent
Summary
Mod #
Section
Chapter
Referenced Standards
 4349 
Update organization.
Joseph Belcher
43
Comment

Proponent
Summary
Mod #
Section
Chapter
4403.7.8
 3843 
Clarification of required design Flood Loads for ASCE 7 in HVHZ
Mohammed Shaikh
44
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 58 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
4408.1.3
 3670 
This section requires modification due to adoption of ‑2005 Manual of Steel Construction, Thirteenth edition
Mohammed Shaikh
44
Comment

Proponent
Summary
Mod #
Section
Chapter
4409.1.4.7
 4157 
This proposal updates the currently referenced standards to their current editions.
Paul Coats
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4402.10.21, R4402.13.1.7
 3701 
Clarification
chris schulte
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4403
 4230 
This modification is a correlation to the modification that updates ASCE 7 to the 2010 Edition.
T Stafford
44
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 59 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R4403.12
 4305 
Proposal deletes an obsolete table no longer contained in ASCE 7 and permits the use of the AAF Guide to design screen enclosures.
Joseph Belcher
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4403.12
 4333 
Adds aluminim screen enclosure design pressure table from Chapter 22. Add windbreaker provisions from Chapter 16, Section 1622.
Joseph Belcher
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4403.13
 3903 
Florida‑specific modifications related to retaining flood provisions of the I‑Codes.  These mod clarifies that structures and foundations seaward of the CCCL must also comply with R322 if also located in a flood hazard area.
Rebecca Quinn
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4403.13
 4344 
The proposal adds provisions for sunrooms in the HVHZ section of the code.
Joseph Belcher
44
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 60 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R4403.16.1
 3802 
This code modification is meant to standardize a form of testing which is extremely necessesary for soffit vents, soffit systems, and ridge vents in hurricane prone areas. This mod only revise Exception (b), the remaining text &quot;unchanged&quot;
Michael Hemmer
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4403.7.3.6.3
 3730 
Correlates the HVHZ requirements on use of laminated glazing for glass railings used in the wind borne debris region with those of the 2009 IBC.
Jaime Gascon
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4403.9
 4146 
ASCE 7‑05 commentary states that high uplift may exist on rooftop equipment, but no methodology is given. Load calculations may vary by a large factor based on two methods given. This modification is to eliminate such differences and include uplift and revised lateral forces based on FIU research.
Arindam Gan Chowdhury
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4407
 4137 
The modification brings the section on reinforced unit masonry up to date with the national masonry standards.
Joseph Belcher
44
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 61 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Residential
R4408.9.3.3 and R4408.10.10.1
 3866 
Cables and rods shall not be used to brace Cold‑Formed (R4408.9.3.3) and Pre‑Engineered (R4408.10.10.1) steel buildings.
This proposal is to delete the word “habitable” from these two sections.
Mohammed Shaikh
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4410.2.1.11
 3669 
The modification clarifies that 'comparative' analysis is allowed, as opposed to the used term 'rational' analysis when the fixed glazing product differs from the one approved.
Jaime Gascon
44
Comment

Proponent
Summary
Mod #
Section
Chapter
R4410.4
 3529 
As per the General portion of this section. We are requesting that the Soffit Vents and Gable Vents on Structures either have Specific Product Approvals or be protected with an Product Approved Shutter to prevent wind and water damage in that structure.
Michael Hemmer
44
Comment

Proponent
Summary
Mod #
Section
Chapter
New Appendix
 4405 
Add a new Appendix “XX” (Designation to be assigned)
Doug Harvey
3316
Comment

Proponent
Summary
Mod #
Section
Chapter
SubCode:
Test Protocols
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 62 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Test Protocols
1.3, 8.5, 12.1.2
 3535 
Clarifications of terms
chris schulte
1
Comment

Proponent
Summary
Mod #
Section
Chapter
10.4.8
 3528 
Deletion of reference to a nonexistent protocol ‑ TAS100(B), and clarifying the section.
Jaime Gascon
1
Comment

Proponent
Summary
Mod #
Section
Chapter
1.2
 3542 
Clarification
chris schulte
1
Comment

Proponent
Summary
Mod #
Section
Chapter
12
 3446 
Adds requirement for additional testing when original test is older than 10 years.
Jaime Gascon
1
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 63 of 64
6/28/2010
Total Mods for this TAC:
Structural
TAC:
 252 
SubCode:
Test Protocols
6.3.1.1
 3571 
Clarification
chris schulte
1
Comment

Proponent
Summary
Mod #
Section
Chapter
12
 3461 
Adds requirement for additional testing when original test is older than 10 years.
Jaime Gascon
1
Comment

Proponent
Summary
Mod #
Section
Chapter
5.2.7
 3464 
Deletion of ASTM E283's standard year in the text of the protocol.  Year of standard is already in chapter 35.
Jaime Gascon
1
Comment

Proponent
Summary
Mod #
Section
Chapter
13
 3462 
Adds requirement for additional testing when original test is older than 10 years.
Jaime Gascon
1
Comment

Proponent
Summary
Mod #
Section
Chapter
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations

Florida Department of Community Affairs
Building Codes and Standards
TAC & Commission Tracking Chart
Page 64 of 64
6/28/2010
Modification #:
Code Change Cycle:
Chapter & Topic:
Date Submitted From:
TAC:
Proponent Last Name:
Affects HVHZ:
Sub Code:
Code Version:
Commission Action:
Text of Modification:
Section:
Related Modifications:
TAC Recommendation:
Date Submitted To:
Proponent First Name:
2010
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
ALL
Search Criteria
AS = Approved as Submitted
AM = Approved as Modified
NAR = No Affirmative Recommendation
W = Withdrawn
I = Insufficient (incomplete or does not meet criteria)
TAC Recommendations