|  |  |  |  |
| --- | --- | --- | --- |
| **ROOFING**  TAC ACTION VOTES  Local Technical Amendments to the  2020 7th Edition Florida Building Code | | | |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with**  **TECHNICAL AMENDMENT** | **TEXT OF TECHNICAL AMENDMENT** | **TAC ACTION** |
|  |  |  |  |
| Pinellas County Construction Industry Licensing Board  (PCCLB | FBC – Building  Sec 1510.10 | Section 1510.10 – amendment to require that all roof mounted mechanical units comply with the code section upon reroofing the building. | VOTE: |
|  |  |  |  |
|  |  |  |  |
|  |  | 1510.10 Mechanical Units.  Roof mounted mechanical units shall be mounted on curbs raised a minimum of 8 inches (203 mm) above the roof surface, or where roofing materials extend beneath the unit, on raised equipment supports providing a minimum clearance height in accordance with Table 1510.10.  Exception: In buildings where the existing rooftop equipment, in the opinion of the building official, provides sufficient clearance to repair, recover, replace and/or maintain the roofing system or any of its components, such existing equipment need not comply with Table 1510.10. |  |