**Options for Changes to Rule 61G20-2.001 Based on Comments from DBPR Staff and the Public**

Election of Chairman

1. Annually (Recommended by the Commission’s legal counsel based on Section 553.75, F.S.)
2. Approximately, every three years coinciding with the Florida Building Code’s triennial update process (Current Draft)
	1. Every three years or coinciding with the Florida Building Code’s triennial update process depending on whichever is shorter. (Proposed by DBPR)
	2. The first chair’s term shall run from their election to the next edition of the code. Future chairman’s terms shall run concurrently with the update of the code to subsequent new editions. (FHBA)

 Experience Requirement for Chairman

1. One year (Proposed by DBPR and FHBA)
2. Two years
3. Three years (Current Draft)

Voting Requirement for Election of Chairman

1. 51% (Current Draft)
2. 75% (Proposed by FHBA)

Chairman’s Power to Appoint Vice Chairman and TAC Chairman

1. Chairman may appoint a vice chairman and TAC chairs. (Current Draft)
2. Chairman shall appoint a vice chairman and TAC chairman. (FHBA)