|  |  |  |  |
| --- | --- | --- | --- |
| **Mechanical**  **Local Technical Amendments to the**  **2017 6th Edition Florida Building Code** | | | |
| **JURISDICTION** | **DOCUMENT**  **with**  **TECHNICAL AMENDMENT** | **TEXT OF TECHNICAL AMENDMENT** | **TAC REVEW** |
|  | 2017 Florida Building Code, Mechanical Ch. 3  Dies for lack of 2nd NAR |  | Mechanical TAC |
|  | 2017 Florida Building Code, Mechanical Ch. 9  Dies for lack of 2nd NAR |  | Mechanical TAC |
| **Pinellas County Construction Licensing Board** | 2017 Florida Building Code, Residential Ch. 14 | **M1411.3 Condensate disposal.** Condensate from cooling coils and evaporators shall be conveyed from the drain pan outlet to an *approved* place of disposal. Such piping shall maintain a minimum horizontal slope in the direction of discharge of not less than 1/8 unit vertical in 12 units horizontal (1-percent slope). Condensate shall not discharge into a street, alley or other areas where it would cause a nuisance. Pipe Insulation: All primary condensate drain within unconditioned areas shall be insulated. | Mechanical TAC |
|  |  |  |  |
|  |  |  |  |