**Revise Section 157.1.1.1 (1) to read as follows:**

**1507.1.1.1 Underlayment for asphalt, metal, mineral surfaced, slate and slate-type roof coverings.** Underlayment for asphalt shingles, metal roof shingles, mineral surfaced roll roofing, slate and slate-type shingles, ~~wood shingles, wood shakes~~ and metal roof panels shall comply with one of the following methods:

1. The entire roof deck shall be covered with an approved self-adhering polymer modified bitumen underlayment complying with ASTM D1970 installed in accordance with both the underlayment manufacturer’s and roof covering manufacturer’s installation instructions for the deck material, roof ventilation configuration and climate exposure for the roof covering to be installed.

Exception: An existing self-adhering modified bitumen underlayment ~~complying with Underlayment Attachment~~ *~~3~~* ~~1. above~~ which has been previously installed over the roof decking and where it is required, re-nailing off the roof sheathing in accordance with 706.7.1 of the Florida Building Code, Existing Building can be confirmed or verified. An approved underlayment in accordance with Table 1507.1.1.1 for the applicable roof covering shall be applied over the entire roof over the existing self-adhered modified bitumen underlayment.

(R7580)