**Roofing Technical Advisory Committee – Errata**

**8th Edition (2023) Florida Building Code, Building**

**CHAPTER 35 REFERENCED STANDARDS**

R-FBC-B -Ch. 35 – Errata #1

John W. Knezevich, Knezevich Consulting, LLC

Mo,

Busy time for this, but if you have a place to mark up corrections for the next cycle of the code, put this in that pile.

From Chapter 35, 2023 code.  This should be 1507.12.2.  1507.13.2 is "reserved".  Thanks to your reviewers, they noted us referencing this incorrect section.

D6878/D6878M—21 Standard Specification for Thermoplastic Polyolefin Based Sheet Roofing . . . . . . . . . . . . . . . . . .1507.~~13~~12.2

**TAC Recommendation**:

**Commission Action:**

**Comment –**

**BOAF Building Officials Association of Florida CDC Code Development Committee**

**Proposal: Reference Chapter 35 fix reference number related to ASTM, correct reference is 1507.12.2, 1507.13.2 is reserved. ASTM D6878/D6878M-21 Standard Spec for Thermoplastic Polyolefin based sheet roofing should be 1507.12.2 not 1507.13.2**

**Comment: This is correct 1507.13 is reserved and 1507.12.2 is the correct reference**

**Approve/Oppose: Approve**

R-FBC-B -Ch. 35 – Errata #2

Isaac Rodriguez – NEMO

Greetings ,

I am Isaac Rodriguez with Nemo|etc. and I am reviewing the 2023 Florida Building Code, 8th edition draft to collate the standard changes.

In the 2023 Florida Building Code, 8th edition draft, Chapter 35, page 732

ASTM D5665/D5665M-17 is referenced as the updated standard version. But a 2017 version of the standard does not exist.

All the D5665/D5665M versions are listed below:

* 99a(2021)
* 99a(2014)e01
	+ [2014 was the version used in the 2020 FBC]
* 99a(2016)
* 99a

Which D5665/D5665M standard version should be used?

**Staff – Fix**

Use - 99a(2021) – latest edition.

**TAC Recommendation**:

**Commission Action:**

**Comment –**

**BOAF Building Officials Association of Florida CDC Code Development Committee**

**Proposal: Reference Chapter 35 fix ASTM reference year, ASTM D5665/D5665M-17 should be per Staff fix 99a(2021)-Latest Edition**

**Comment: correct reference year needed for this standard**

**Approve/Oppose: Approve**

**8th Edition (2023) Florida Building Code, Existing Building**

**CHAPTER 7 ALTERATIONS—LEVEL 1**

R-FBC-EB - Ch. 7 – Errata #1

Claude Navennec - Aluminart Corp. d/b/a Qualitair

Good morning,

I found an error in the code.

Could you forward this email to whoever could make an addendum to clarify.

Thanks.

2023 Florida Building code, Existing Building, Eight edition

Section 706.8.1.3, .4, .5 & .6

It reads “ 500 pounds (740 kg)”

500 lbs is actually 226.8 KG

740 KG is 1631.4 lbs

Hopefully the 500 lbs is right!

Thanks and have a great day!

**TAC Recommendation**:

**Commission Action:**

**Comment –**

**BOAF Building Officials Association of Florida CDC Code Development Committee**

**Proposal: Chapter 7 section 706.8.1.3, .4, .5, & .6 need correct lbs conversion to Kg. Currently reads 500 lbs =(740 kg) should be 500lbs= (226.8 kg). 740kg actually equals 1631.4 lbs.**

**Comment: agreed need correct conversion**

**Approve/Oppose: Approve**