|  |  |  |  |
| --- | --- | --- | --- |
| **PLUMBING / FUEL GAS**  **TAC ACTION/Votes**  **Local Technical amendments**  **to the**  **2020 7th Edition Florida Building Code** | | | |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with TECHNICAL AMENDMENT** | **SUMMARY OF TECHNICAL AMENDMENT** | **TAC ACTION/VOTE** |
|  |  |  |  |
| Pinellas County  Construction Industry Licensing Board  (PCCLB) | FBC –  Residential  P2906.9.1.4  P2903.2.1  P2903.1  P2705.1  FBC- Plumbing  Sec 705.10.2  Sec. 610.2  Sec 605.21.3 | AMEND EXISTING SECTION  **Section P2906.9.1.4 PVC plastic pipe**. A purple primer that conforms to ASTM F656 shall be applied to PVC solvent-cemented joints. Solvent cement for PVC plastic pipe conforming to ASTM D 2564 shall be applied to all joint surfaces.  Exception: Clear Primer conforming to ASTM F656 may be used on any exposed PVC pipe or fittings on trim/finish work.  **Section P2903.2.1** – amendment to add provisions pertaining to minimum water service size.  **Section P2903.1** – amendment to clarify that disinfection is not required every time work is performed on a plumbing system.  **Section P2705.1** – amendment to bring awareness to the plumbing fixture spacing requirements located in both sections of the code.  **Section 705.10.2** – amendment to permit the use of clear primer instead of purple primer when used on exposed PVC pipe or fittings on trim/finish work.  **Section 610.2** - amendment to clarify that disinfection is not required every time work is performed on a plumbing system.  **Section 65.21.3** – amendment to permit the use of clear primer instead of purple primer when used on exposed PVC pipe or fittings or trim/finish work. | VOTE: |
|  |  |  |  |
| County of Palm Beach | FBC – Plumbing  Appendix F | Amendment to adopt Appendix F “Proposed Construction Building Codes for Turf and Landscape Irrigation System” | VOTE: |
|  |  |  |  |
| County of Miami-Dade | FBC – Plumbing  Sec 604.4  Table 604.4  FBC - Residential  P2903.2 and Table P2903.2 | Sections 604.4/P2903.2 – amendments to meet the water conservation goals provided in the County’s Water Efficiency Plan. | Vote: |
|  |  |  |  |
| County of Broward | FBC – Residential Table P2903.2 | Table P2903.2 – amendment revising the maximum flow rates and consumption for plumbing fixture, fixture fittings and appliances. | VOTE: |
|  |  |  |  |
| County of Broward | FBC – Pluming  Sec 314.2.1 | Section 314.2.1 – amendment to require the collection of condensate from all cooling coils and evaporators of equipment serviced by on- site cooling tower in a building or structure wherein the aggregate cooling capacity of the equipment exceeds 65,000 BTU/HR. | VOTE: |
|  |  |  |  |
| County of Miami-Dade | FBC – Plumbing  Sec 604.4 | Section 604.4 – amendment reducing plumbing fixture water flow rates currently required by the FBC – Plumbing thereby increasing water conservation standards. |  |
|  |  |  |  |
|  |  |  |  |
| County of Broward | FBC – Plumbing  Appendix F | Amendment to adopt Appendix F “Proposed Construction Building Codes for Turf and Landscape Irrigation System” | VOTE: |
|  |  |  |  |
| County of Broward | FBC – Plumbing  Sec 307.2.1 | Section 307.2.1- amendment to require the collection of condensate from all cooling coils and evaporators of equipment serviced by on- site cooling tower in a building or structure wherein the aggregate cooling capacity of the equipment exceeds 65,000 BTU/HR. | VOTE: |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **FUEL GAS**  **TAC Action Votes to the**  **Local Technical Amendments**  **2020 7th Building Code** | | | |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with**  **TECHNICAL**  **AMENDMENT** | **TEXT OF TECHNICAL AMENDMENT** | **TAC REVIEW** |
|  |  |  |  |
| Pinellas County Construction Industry Licensing Board  (PCCLB) | FBC –  Residential  G2415.15  FBC – Fuel Gas  Sec 404.15 | Section G2415.15 - amendment to add limitations to control future connections to gas outlets.  Section 404.15 – amendment to add limitations to control future connections to gas outlets. | VOTE: |
|  |  |  |  |