454.1

Add as new definition

|  |
| --- |
| **“Swim-up Bar” means a public pool used for the consumption of food and beverages by people, that may include a permanent bar or counter from which food and beverages are served to people in the pool.**  **…**  **454.1.3.1.7 Food or drink service facilities shall not be located within 12 feet (3658 mm) of the water’s edge.****Any pool with food or drink service within 12 feet (3658 mm) of the water’s edge must comply with 454.1.9.9 for Swim Up Bars.**  **…**  **454.1.9.9 Swim Up Bars**  **454.1.9.9.1 A swim-up bar shall be constructed within the limits of sound engineering practice. The maximum pool depth shall not exceed 5 feet (1524 mm) and the recirculation turnover time shall be 2 hours or less.The disinfection equipment shall be capable of feeding 12 mg/L of halogen to the continuous recirculation flow of the filtration system. Attendants or lifeguards shall be provided in accordance with a safety/lifeguard plan approved by the Department of Health.**  **454.1.9.9.2A rules sign complying with 454.1.2.3.5 shall be provided, except, the first rule shall read:**  **Food and Drink are consumed in this pool. All drinks shall be in plastic or aluminum containers.**  **454.1.9.9.3If the bar or counter is built into the edge of the pool, pool access complying with 454.1.2.5 shall be provided at both ends of the bar. Deck complying with 454.1.3.1 shall be provided, except, up to 50% of the pool perimeter may be obstructed by the bar. Gutters or skimmers are not required at or under the bar counter, however, they are required at the rest of the pool. An automatic water level controller shall be provided, and an overfill waste line with air gap shall be provided.**  **454.1.9.9.4 A swim up bar may be physically combined or connected with other pool types, however, food and drink must be permitted over the entire body of water and the requirements of 454.1.9.9.1 shall apply to the entire water volume. A swim up bar’s water must not mix with any body of water that is not a swim up bar and does not allow the consumption of food and beverages.**  **454.1.9.9.5 A swim up bar may include obstructions intended for seating. Any structure intended for seating in the pool shall have 2 inch (51 mm) horizontal and 2 inch (51 mm) vertical markings in contrasting color on every edge, and be structurally rigid, impervious, non-toxic, smooth, and slip resistant. The edges of such obstructions shall not overhang into the water by more than 1.5 inches (38 mm).** |
|  |

**(SW10382 AM A1)**