|  |
| --- |
| **ROOFING**TAC ACTION VOTES Local Technical Amendments to the2020 7th Edition Florida Building Code |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with****TECHNICAL AMENDMENT** | **TEXT OF TECHNICAL AMENDMENT** | **TAC ACTION** |
|  |  |  |  |
| Pinellas County Construction Industry Licensing Board(PCCLB | FBC – BuildingSec 1510.10 | Section 1510.10 – amendment to require that all roof mounted mechanical units comply with the code section upon reroofing the building. | Batts to Deny 2nd Oyola VOTE:10 Yes – 0 No |
|  |  |  |  |
|  |  |  |  |
|  |  | 1510.10 Mechanical Units. Roof mounted mechanical units shall be mounted on curbs raised a minimum of 8 inches (203 mm) above the roof surface, or where roofing materials extend beneath the unit, on raised equipment supports providing a minimum clearance height in accordance with Table 1510.10. Exception: In buildings where the existing rooftop equipment, in the opinion of the building official, provides sufficient clearance to repair, recover, replace and/or maintain the roofing system or any of its components, such existing equipment need not comply with Table 1510.10. |  |