CHAPTER 35
REFERENCED STANDARDS
This chapter lists the standards that are referenced in various sections of this document. The standards are listed herein by the promulgating agency of the standard, the standard identification, the effective date and title, and the section or sections of this document that reference the standard. The application of the referenced standards shall be as specified in Section 102.4.

 Aluminum Association
900 - 19th Street N.W., Suite 300
Washington, DC 20006
 AA
 Standard						Referenced
reference						in code
number		Title					section number
 ADM 1—00	Aluminum Design Manual: Part 1-A Aluminum Structures, Allowable Stress Design; and Part 1-B—Aluminum Structures, Load and Resistance Factor Design of Buildings and Similar Type Structures	1604.3.5, 2002.1
 ASM 35—80	Aluminum Sheet Metal Work in Building Construction	2002.1
 American Architectural Manufacturers Association
1827 Waldon Office Square, Suite 104
Schaumburg, IL 60173
 AAMA
Standard							Referenced
reference						in code
number		Title					section number
 1402—86	Standard Specifications for Aluminum Siding, Soffit and Fascia	1404.5.1
 101/I.S.2—97	Voluntary Specifications for Aluminum, Vinyl (PVC) and Wood Windows and Glass Doors	1714.5.1
 101/I.S.2/NAFS—02	Voluntary Performance Specification for Window, Skylights and Glass Doors	1714.5.1, 2405.5
 American Concrete Institute
P.O. Box 9094
Farmington Hills, MI 48333-9094
 ACI
Standard							Referenced
reference						in code
number		Title					section number
 216.1—97	Standard Method for Determining Fire Resistance of Concrete and
Masonry Construction Assemblies	Table 721.1(2), 721.1
 318—02	Building Code Requirements for Structural Concrete	1604.3.2, Table 1617.6, 1617.6.2.4.3, Table 1704.3, 1704.4.1,
 Table 1704.4, 1708.3, 1805.4.2.6, 1805.9, 1808.2.23.1.1, 1808.2.23.2,
1808.2.23.2.1, 1808.2.23.2.2, 1809.2.3.2, 1809.2.3.2.2, 1810.1.2.2, 1812.8,
1901.2, 1901.3, 1901.4, 1902, 1903.1, 1903.2, 1903.3, 1903.4, 1903.5.1,1903.6, 1904.4.2, 1905.1.4, 1905.3, 1905.4, 1905.5, 1905.6.5.5, 1905.8.3, 1905.11.3,
1906.1.5, 1906.3, 1906.4.3, 1907.1, 1907.2, 1907.4.1, 1907.6, 1907.7.2, 1907.7.3, 
907.7.4, 1907.7.5, 1907.8, 1907.9, 1907.10, 1907.11, 1907.12, 1907.13, 1908 ,1908.1.1,
1908.1.2, 1908.1.3, 1908.1.4, 1908.1.5, 1908.1.6, 1908.1.7, 1908.1.8, 1908.1.9,
1909.1, 1909.3, 1909.4, 1909.5, 1909.6, 1910, 1910.2.1, 1910.2.2, 1910.2.3, 1910.2.4,
1910.3.1, 1910.4.1, 1910.4.2, 1910.4.3, 1910.4.3.1, 1910.5.2, 1913.1, 2108.3, 2205.3
 530—02	Building Code Requirements for Masonry Structures	1405.5, 1405.5.3, 1405.9, 1604.3.4, 1704.5, 1704.5.1, Table 1704.5.1, 1704.5.2, Table 1703.3.1, 1708.1.1, 1708.1.2, 1708.1.3,
1805.5.2, 1812.7, 2101.2.3, 2101.2.4, 2101.2.5, 2103.11.6, 2106.1,
 2106.1.1.1, 2106.1.1.2, 2106.1.1.3, 2106.3, 2106.4, 2106.5, 2106.6,
2107.1, 2107.2, 2107.2.1, 2107.2.2, 2107.2.4, 2107.2.5, 2107.2.6, 2108.1, 
2108.2, 2108.4, 2109.1, 2109.2.3.1, 2109.2.3.2
 530.1—02	Specifications for Masonry Structures	1405.5.1, 1405.9.1, Table1704.5.1, Table 1704.5.3, 1805.5.2,
 2103.11.7, 2104.1, 2104.1.1, 2104.3,
 TG/T1.1—01	Acceptance Criteria for Moment Frames Based on Testing	1908.1.3
 American Forest & Paper Association
1111 19th St, NW Suite 800
Washington, DC 20036
 AF&PA
Standard							Referenced
reference						in code
number		Title					section number
 AF&PA/ASCE 16—95	Standard for Load and Resistance Factor Design (LRFD) for Engineered Wood Construction	2307.1
 WCD No. 4—89	Plank and Beam Framing for Residential Buildings	2306.1.2
 WFCM—01	Wood Frame Construction Manual for One-and Two-family Dwellings	2301.2.3, 2308.1, 2308.2.1
 T.R. No. 7—87	Basic Requirements for Permanent Wood Foundation System	1805.4.6, 1807.2, 2304.9.5
 NDS—01	National Design Specification (NDS) for Wood Construction
with 2001Supplement	721.6.3.2, 1715.1.1, 1715.1.4, 1805.4.5, 1808.1, 2306.1, 2306.2.1,
 2306.3.2, Table 2306.3.1, Table 2306.4.1, 2306.3.4, 2306.3.5, 2306.4.1, Table 2308.9.3(4)
 AF&PA—93	Span Tables for Joists and Rafters	2306.1.1, 2308.8, 2308.10.2, 2308.10.3
 American Hardwood Association
1210 West N.W. Highway
Palatine, IL 60067
 AHA
Standard							Referenced
reference						in code
number		Title					section number
 A135.4—95	Basic Hardboard	1404.3.1, 2303.1.6
 A135.5—95	Prefinished Hardboard Paneling	2303.1.6, 2304.6.2
 A135.6—98	Hardboard Siding	1404.3.2, 2303.1.6
 A194.1—85	Cellulosic Fiber Board		2303.1.5
 American Institute of Steel Construction
One East Wacker Drive, Suite 3100
Chicago, IL 60601-2001
 AISC
Standard							Referenced
reference						in code
number		Title					section number
 335—89s1	Specification for Structural Steel Buildings—Allowable Stress Design and
Plastic Design, including Supplement No.1, 2001 	1604.3.3, Table 1617.6.2, Table 1704.3, 2203.2, 2205.1
 LRFD (1999)	Load and Resistance Factor Design Specification for Structural
Steel Buildings	1604.3.3, Table 1617.6, Table 1704.3, 2203.2, 2205.1, 2205.3
 HSS (2000)	Load and Resistance Factor Design Specification for Steel Hollow
Structural Sections	1604.3.3, Table 1617.6, 2203.2, 2205.1
 341—02	Seismic Provisions for Structural Steel Buildings 	1602.1, Table 1617.6.2, 1707.2, 1708.4,
 2205.2.1, 2205.2.2, 2205.3, 2205.3.1
 American Iron and Steel Institute
1140 Connecticut Avenue
Suite 705
Washington, DC 20036
 AISI
Standard							Referenced
reference						in code
number		Title					section number
 NASPEC 2001	North American Specification for Design of Cold-Formed Steel Structural Members 	 1604.3.3, 2209.1
 General Standard for Cold-Formed Steel Framing-General Provisions, 2001	2210.1
 Header Standard for Cold-Formed Steel Framing-Header Design, 2001	2210.2
 Truss Standard for Cold-Formed Steel Framing-Truss Design, 2001	2210.3
 American Institute of Timber Construction
Suite 140
7012 S. Revere Parkway
Englewood, CO 80112
 AITC
Standard							Referenced
reference						in code
number		Title					section number
 AITC A 190.1—92	Structural Glued Laminated Timber		2303.1.3, 2306.1
 AITC Technical Note 7—96	Calculation of Fire Resistance of Glued Laminated Timbers	721.6.3.3
 AITC 104—84	Typical Construction Details	2306.1
 AITC 110—01	Standard Appearance Grades for Structural Glued Laminated Timber	2306.1
 AITC 112—93	Standard for Tongue-and-Groove Heavy Timber Roof Decking	2306.1
 AITC 113—01	Standard for Dimensions of Structural Glued Laminated Timber	2306.1
 AITC 117—01	Standard Specifications for Structural Glued Laminated Timber of Softwood Species—
Design Requirements—Standard Specifications for Structural Glued Laminated Timber
of Softwood Species—Manufacturing Requirements	2306.1
 AITC 119—96	Standard Specifications for Structural Glued Laminated Timber of Hardwood Species	2306.1
 AITC 200—92	Inspection Manual	2306.1
 AITC 500—91	Determination of Design Values for Structural Glued Laminated Timber	2306.1
 Automotive Lift Institute
P.O. Box 33116
Indialantic, FL 32903-3116
 ALI
Standard							Referenced
reference						in code
number		Title					section number
 ALI ALCTV—98	Standard for Automotive Lifts—Safety Requirements for Construction, Testing and Validation (ANSI)	3001.2
 American National Standards Institute
25 West 43rd Street, Fourth Floor
New York, NY 10036
 ANSI
Standard							Referenced
reference						in code
number		Title					section number
 A 13.1—96	Scheme for the Identification of Piping Systems	415.9.6.4
 A 42.2—71	Portland Cement and Portland Cement Lime Plastering, Exterior (Stucco) and Interior	2109.8.4.6
 A 42.3—71	Lathing and Furring for Portland Cement and Portland Cement Lime Plastering, Exterior Stucco and Interior	2109.8.4.6
 A108.1A—99	Installation of Ceramic Tile in the Wet-set Method, with Portland Cement Mortar	2103.9
 A108.1B—99	Installation of Ceramic Tile, Quarry Tile on a Cured Portland Cement Mortar Setting Bed
with Dry-set or Latex-Portland Mortar	 2103.9
 A108.4—99	Installation of Ceramic Tile with Organic Adhesives or Water-cleanable Tile-Setting Epoxy Adhesive	2103.9.7
 A108.5—99	Installation of Ceramic Tile with Dry-set Portland Cement Mortar or
Latex Portland Cement Mortar	2103.9.1, 2103.9.2, 2103.9.3
 A108.6—99	Installation of Ceramic Tile with Chemical-resistant, Water Cleanable Tile-setting-and-grouting Epoxy	2103.9.4
 A108.7—92	Specification for Electrically Conductive Ceramic Tile Installed with Conductive Dry-set Portland Cement Mortar	2103.9.2
 A108.8—99	Installation of Ceramic Tile with Chemical-resistant Furan Resin Mortar and Grout	2103.9.5
 A108.9—99 	Installation of Ceramic Tile with Modified Epoxy Emulsion Mortar/Grout	2103.9.6
 A 108.10—99	Installation of Grout in Tilework	2103.9.8
 A 118.1—99	 American National Standard Specifications for Dry-set Portland Cement Mortar.	2103.9.1
 A 118.2—99	American National Standard Specifications for Conductive Dry-set Portland Cement Mortar	2103.9.2
 A 118.3—99	American National Standard Specifications for Chemical-resistant, Water-cleanable
Tile-setting and -Grouting Epoxy and Water Cleanable Tile-setting Epoxy Adhesive	2103.9.4
 A 118.4—99	American National Standard Specifications for Latex-portland Cement Mortar..	2103.9.3
 A 118.5—99	American National Standard Specifications for Chemical Resistant Furan Mortar and Grouts for Tile Installation	 2103.9.5
 A 118.6—99	American National Standard Specifications for Cement Grouts for Tile Installation	2103.9.8
 A 118.8—99	American National Standard Specifications for Modified Epoxy Emulsion Mortar/Grout	2103.9.6
 A 136.1—99	American National Standard Specifications for Organic Adhesives for Installation of Ceramic Tile	2103.9.7
 A 137.1—88	American National Standard Specifications for Ceramic Tile	2103.4
 A 208.1—99	Particleboard	2303.1.7, 2303.1.7.1
 ANSI—continued
 B 31.3—01 99	Process Piping—Including Addendum	415.9.6.1
 Z 97.1—84 (R1994)	 Safety Glazing Materials Used in Buildings-safety Performance
Specifications and Methods of Test (Reaffirmed 1994)	2406.1.3, 2406.1.2, 2407.1
 APA - Engineered Wood Association
P.O. Box 11700
Tacoma, WA 98411-0700
 APA
Standard							Referenced
reference						in code
number		Title					section number
 APA PDS—97 	Plywood Design Specification (revised 1998)	2306.1, Table 2306.3.1, 2306.3.2, 2306.4.1
 APA PDS Supplement 1—90	Design and Fabrication of Plywood Curved Panels (revised 1995)	2306.1
 APA PDS Supplement 2—92 	Design and Fabrication of Plywood-lumber beams (revised 1998)	2306.1
 APA PDS Supplement 3—90	Design and Fabrication of Plywood Stressed-skin Panels (revised 1996)	2306.1
 APA PDS Supplement 4—90	Design and Fabrication of Plywood Sandwich Panels (revised 1993)	2306.1
 APA PDS Supplement 5—95	Design and Fabrication of All-plywood Beams (revised 1995)	2306.1
 EWS R540—96	Builders Tips: Proper Storage and Handling of Glulam Beams	2306.1
 EWS S475—99	Glued Laminated Beam Design Tables	2306.1
 EWS S560—99	Field Notching and Drilling of Glued Laminated Timber Beams	2306.1
 EWS T300—99	Glulam Connection Details	2306.1
 EWS X440—00	Product Guide-Glulam..	2306.1
 EWS X445—97	Glulam in Residential Construction —Southern Edition	2306.1
 EWS X450—97	Glulam in Residential Construction —Western Edition	2306.1
 American Society of Agricultural Engineers
2950 Niles Road
St. Joseph, MI 49085-9659
 ASAE
Standard							Referenced
reference						in code
number		Title					section number
EP 484.2 (1998)	Diaphragm Design of Metal-Clad, Post-Frame Rectangular Buildings	2306.1
 EP 486.1 (2000)	Shallow-Post Foundation Design	2306.1
 EP 559 (1997)	Design Requirements and Bending Properties for Mechanically Laminated Columns	2306.1
1933;InLeftRPg=1933;>

American Society of Civil Engineers
Structural Engineering Institute
1801 Alexander Bell Drive
Reston, VA 20191-4400
ASCE/SEI
Standard							Referenced
reference						in code
number		Title					section number
 3—91	Standard Practice for the Construction and Inspection of Composite Slabs	1604.3.3, 2209.2
 5—02	Building Code Requirements for Masonry Structures	1405.5, 1405.5.3, 1405.9, 1604.3.4, 1704.5, 1704.5.1,
 Table 1704.5.1, 1704.5.2, Table 1703.3.1, 1708.1.1, 1708.1.2, 1708.1.3,
1805.5.2, 1812.7, 2101.2.3, 2101.2.4, 2101.2.5, 2103.11.6, 2106.1,
2106.1.1.1, 2106.1.1.2, 2106.1.1.3, 2106.3, 2106.4, 2106.5, 2106.6,
2107.1, 2107.2, 2107.2.1, 2107.2.2, 2107.2.4, 2107.2.5, 2107.2.6, 2108.1,
2108.2, 2108.4, 2109.1, 2109.2.3.1, 2109.2.3.2
 6—02	Specifications for Masonry Structures	1405.5.1, 1405.9.1, Table1704.5.1, Table 1704.5.3, 1805.5.2,
 2103.11.7, 2104.1, 2104.1.1, 2104.3,
 7—9802	Minimum Design Loads for Buildings and Other Structures	1605.1, 1605.2.2, 1605.3.1.2, 1605.3.2, 1608.1, 1608.3,
 1608.3.4, 1608.3.5, 1608.4, 1608.5, 1608.6, 1608.7, 1608.8,
1608.9, 1609.1.1, 1609.1.4.1, 1609.3, Table 1609.3.1, 1609.7.3, 1612.2,
1614.1, 1616.1, 1616.3, 1616.4.5, 1616.5, Table 1616.5.1.1, Table 1616.5.1.2,
1616.6, 1617.1, 1617.2, 1617.2.1, 1617.2.2.2, 1617.3, 1617.4, 1617.6,
1617.6.1, 1617.6.1.1, 1618.1, 1619, 1620.1, 1620.1.1, 1620.1.2, 1620.1.3,
1620.2.1, 1620.2.7, 1620.3.1, 1621.1, 1621.1.1, 1621.1.2, 1621.1.3,
1622.1, 1622.1.1, 1622.1.2, 1622.1.3, 1623.1, 1623.1.1
 ASCE/SEI—continued
 8—90	Standard Specification for the Design of Cold-formed Stainless Steel Structural Members	1604.3.3, 2209.1
 16—95	Standard for Load Resistance Factor Design (LRFD) for Engineered Wood Construction	2307.1
 19—96	Structural Applications of Steel Cables for Buildings	2207.1, 2207.2
 24—98	Flood Resistant Design and Construction	1203.3.2, 1612.4, 1612.5, 3001.2
 29—99	Standard Calculation Methods for Structural Fire Protection	721.1
 32—01	Design and Construction of Frost Protected Shallow Foundations	1805.2.1
333;>
American Society of Mechanical Engineers
Three Park Avenue
New York, NY 10016-5990
 ASME
Standard							Referenced
reference						in code
number		Title					section number
 A17.1—00	Safety Code for Elevators and Escalators	 1007.4, 1607.8.1, 3001.2, 3001.4, 3002.5, 3003.2, 3409.7.2,
 A18.1—99	Safety Standard for Platform Lifts and Stairway Chairlifts—with Addenda A18.1a-2001	1007.5, 1109.1, 3409.7.3
 A90.1—97	Safety Standard for Belt Manlifts—with Addenda A90.1a-99	3001.2
 B16.18—84 (R1994) 	Cast Copper Alloy Solder Joint Pressure Fittings		909.13.1
 B16.22—95	Wrought Copper and Copper Alloy Solder Joint Pressure Fittings—with Addenda B16.22a-98	909.13.1
 B20.1—00	Safety Standard for Conveyors and Related Equipment	3001.2, 3005.3
333;>

ASTM International
100 Barr Harbor Drive
West Conshohocken, PA 19428-2959
 ASTM
Standard							Referenced
reference						in code
number		Title					section number
 A 6/A 6M— 01b		Specification for General Requirements for Rolled Steel, Structural Steel Bars,
Plates, Shapes, and Sheet Piling	Table 1704.3
 A 36/A 36M—00	Specification for Carbon Structural Steel	1809.3.1, 2103.11.5
 A 82—01	Specification for Steel Wire, Plain, for Concrete Reinforcement 	2103.11.5, 2103.11.6
 A 123/A 123M—97e1Specification for Zinc (Hot-Dip Galvanized) Coating on Iron and Steel Products	2103.11.7.1
 A 153—01a	Specification for Zinc Coating (Hot-Dip) on Iron and Steel Hardware	2103.11.7.1
 A 167—99	Specification for Stainless and Heat-Resisting Chromium-Nickel Steel Plate, Sheet and Strip	2103.11.5
 A 185—01	Specification for Steel Welded Wire Reinforcement, Plain for Concrete 	2103.11.4, 2103.11.5
 A 252—E01	Specification for Welded and Seamless Steel Pipe Piles	1809.3.1, 1810.6.1
 A 283/A 283M—00	Specification for Low and Intermediate Tensile Strength Carbon Steel Plates.	.1809.3.1, 1810.6.1
 A 307—00	Specification for Carbon Steel Bolts and Studs, 60,000 psi Tensile Strength	 1912.1
 A 416—99	Specification for Steel Strand, Uncoated Seven-Wire for Prestressed Concrete	1809.2.3.1, 2103.11.6
 A 421/A 421M—98	Specification for Uncoated Stress-Relieved Steel Wire for Prestressed Concrete	2103.11.6
 A 435/A 435M—90 (2001)	Specification for Straight-Beam Ultrasonic Examination of Steel Plates	1708.4
 A 496—01	Specification for Steel Wire, Deformed for Concrete Reinforcement	2103.11.3, 2103.11.4
 A 510—00	Specification for General Requirements for Wire Rods and Coarse Round Wire, Carbon Steel	2103.11.6
 A 568/A 568M—01	Specification for Steel, Sheet, Carbon, and High-Strength, Low-Alloy, Hot-Rolled and
Cold-Rolled, General Requirements for	Table 1704.3
 A 572/A 572M—01	Specification for High-Strength Low-Alloy Columbium-Vanadium Structural Steel	1809.3.1
 A 588/A 588M—01 	Specification for High-Strength Low-Alloy Structural Steel with 50 ksi (345 Mpa)
Minimum Yield Point to 4 inches (100 mm) Thick	1809.3.1
 A 615/A 615M—01b 00	Specification for Deformed and Plain Billet-Steel Bars for Concrete Reinforcement	1708.3, 1908.1.8, 2103.11.1, 2103.11.6
 A 641/A 641M—98	Specification for Zinc-coated (Galvanized) Carbon Steel Wire	2103.11.7.3
 A 653/A 653M—01a	Specification for Steel Sheet, Zinc-coated Galvanized or Zinc-iron Alloy-Coated
Galvannealed by the Hot-dip Process	Table 1507.4.3, 2211.2, 2211.2.2.1
 A 706/A 706M—00	Specification for Low-Alloy Steel Deformed and Plain Bars for Concrete Reinforcement	1704.4.1, 1903.5.2, 1908.1.3
 A 706/A 706M—01	Specification for Low-Alloy Steel Deformed and Plain Bars for Concrete Reinforcement	2103.11.1, 2103.11.6, 2108.3
 A 722/A 722M—98	Specification for Uncoated High-Strength Steel Bar for Prestressing Concrete	2103.11.6, 2106.1.1.3.1
 A 755/A 755M—01	Specification for Steel Sheet, Metallic-Coated by the Hot-Dip Process and Prepainted
by the Coil-Coating Process for Exterior Exposed Building Products	Table 1507.4.3
 A 767/A 767M—00b	Specification for Zinc-coated (Galvanized) Steel Bars for Concrete Reinforcement	2103.11.1
 A 775/A 775M—01	 Specification for Epoxy-Coated Steel Reinforcing Bars	2103.11.1
 ASTM—continued
 A 792/A 792M—01a	Specification for Steel Sheet, 55% Aluminum-Zinc Alloy-Coated by the
Hot-Dip Process	Table 1507.4.3, 2211.2.2, 2211.2.2.1
 A 875M—01a 99a	Specification for Steel Sheet Zinc-54% Aluminum Alloy-Coated by the Hot Dip Process	2211.2.2, 2211.2.2.1
 A 884—99	Specification for Epoxy-Coated Steel Wire and Welded Wire Fabric for Reinforcement	2103.11.7.2
 A 898/A 898M—91 (2001)	Specification for Straight Beam Ultrasonic Examination of Rolled Steel Shapes	1708.4
 A 899—91 (1999)	Specification for Steel Wire Epoxy-Coated	2103.11.7.2
 A 913/A 913M—01	Specification for High-strength Low-Alloy Steel Shapes of Structural Quality,
Produced by Quenching and Self-tempering Process (QST)	1809.3.1
 A 951—00	Specification for Masonry Joint Reinforcement	2103.11.2
 A 996/A 996M—00	Specification for Rail-Steel and Axle-Steel Deformed Bars Reinforcement for Concrete	2103.11.1, 2103.11.6
 A1008—01A	Specification for Steel, Sheet, Cold-Rolled, Carbon, Structural, High-Strength
Low-Alloy and High-Strength Low-Alloy with Improved Formability	2103.11.5
 B 42—98	Specification for Seamless Copper Pipe, Standard Sizes	909.13.1
 B 43—98	Specification for Seamless Red Brass Pipe, Standard Sizes	909.13.1
 B 68M—99	Specification for Seamless Copper Tube, Bright Annealed (Metric)	909.13.1
 B 88—02 99el	Specification for Seamless Copper Water Tube	909.13.1
 B 101—01	Specification for Lead-Coated Copper Sheet and Strip for Building Construction	Table 1507.4.3
 B 209—96	Specification for Aluminum and Aluminum Alloy Steel and Plate	Table 1507.4.3
 B 251—97	Specification for General Requirements for Wrought Seamless Copper and Copper-alloy Tube	909.13.1
 B 280—99el	Specification for Seamless Copper Tube for Air Conditioning and Refrigeration Field Service	909.13.1
 B 633—98	 Specification for Electrodeposited Coatings of Zinc on Iron and Steel	2211.2
 C 5—75(97)	Specification for Quicklime for Structural Purposes	Table 2507.2
 C 22/C 22M—00	Specification for Gypsum	Table 2506.2
 C 27—98	Specification for Standard Classification of Fireclay and High-Alumina Refractory Brick	2111.5, 2111.8
 C 28/C 28M—00	 Specification for Gypsum Plasters	Table 2507.2
 C 31/31M—98	Practice for Making and Curing Concrete Test Specimens in the Field	Table 1704.4, 1905.6.3.2, 1905.6.4.2
 C 33—99ae1	Specification for Concrete Aggregates	Table 1904.2.1
 C 33—01a	Specification for Concrete Aggregates 	721.3.1.4, 721.4.1.1.3
 C 34—96 (2001)	Specification for Structural Clay Load-bearing Wall Tile	2103.2
 C 35—95 (2001)	Specification for Inorganic Aggregates for Use in Gypsum Plaster 	Table 2507.2
 C 36/C 36M-01	Specification for Gypsum Wallboard 	Figure 721.5.1(2), Figure 721.5.1(3), Table 721.5.1(2), Table 2506.2
 C 37/C 37M-01	Specification for Gypsum Lath	Table 2507.2
 C 39—99ae1	Test Method for Compressive Strength of Cylindrical Concrete Specimens 	1905.6.3.2
 C 42/C 42M—99	Test Method for Obtaining and Testing Drilled Cores and Sawed Beams of Concrete	1905.6.5.2
 C 55—01A	Specification for Concrete Brick	Table 721.3.2, 2103.1, 2105.2.2.1.2
 C 56—96 (2001)	Specification for Structural Clay Non-load Bearing Tile	2103.2
 C 59/C 59M—00 	Specification for Gypsum Casting and Molding Plaster	Table 2507.2
 C 61/C 61M—00 	Specification for Gypsum Keene’s Cement	Table 2507.2
 C 62—01	Specification for Building Brick (Solid Masonry Units Made from Clay or Shale)	2103.2, 2105.2.2.1.1
 C 67—02	Test Methods of Sampling and Testing Brick andStructural Clay Tile 	721.4.1.1.1, 1507.3.5, 2104.5, 2105.2.2.1.1, 2109.8.1.1
 C 73—99a	Specification for Calcium Silicate Face Brick (Sand-lime Brick)	Table 721.3.2, 2103.1
 C 79—01 	Specification for Treated Core and Non-treated Core Gypsum Sheathing Board	Table 2506.2
 C 90—01A	Specification for Loadbearing Concrete Masonry Units	Table 721.3.2, 1805.5.2, 2103.1, 2105.2.2.1.2
 C 91—01	Specification for Masonry CementTable	 2103.7(1), Table 2507.2
 C 94/C 94M—00	Specification for Ready-Mixed Concrete	109.3.1, 1905.8.2
 C 126—99	Specification for Ceramic Glazed Structural Clay Facing Tile, Facing Brick, and Solid Masonry Units	2103.2
 C 140—01 ae1	Test Method Sampling and Testing Concrete Masonry Units and Related Units	721.3.1.2, 1507.3.5, 2105.2.2.1.2
 C 150—99aSpecification for Portland Cement1904.1, Table 1904.2.3
 C 150—01	Specification for Portland Cement	 1904.1, Table 1904.2.3, Table 2103.7(1), Table 2507.2
 C 172—99	Practice for Sampling Freshly Mixed Concrete	Table 1704.4, 1905.6.3.1
 C 199—84 (2000)	Test Method for Pier Test for Refractory Mortars	2111.5, 2111.8, 2113.12
 C 206—84 (1997)	Specification for Finishing Hydrated Lime	Table 2507.2
 C 207—97	Specification for Hydrated Lime for Masonry Purposes	Table 2103.7(1)
 C 208—95(2001) 	Specification for Cellulosic Fiber Insulating Board	2303.1.5
 C 212—00	Specification for Structural Clay Facing Tile	2103.2
 C 216—01A	Specification for Facing Brick (Solid Masonry Units Made from Clay or Shale)	2103.2, 2105.2.2.1.1
 C 270—01A	Specification for Mortar for Unit Masonry2103.7, Table 2103.7(2)
 C 315—02 00	Specification for Clay Flue Linings	2113.11.1, Table 2113.16(1), Table 2113.16(2)
 C 317/C 317M—00	Specification for Gypsum Concrete	1915.1
 ASTM—continued
 C 330—99	Specification for Lightweight Aggregates for Structural Concrete	721.1.1, 1905.1.4
 C 331—01Specification for Lightweight Aggregates for Concrete Masonry Units	721.3.1.4, 721.4.1.1.3
 C 406—00	Specification for Roofing Slate	1507.7.4
 C 442/C 442M—01 	Specification for Gypsum Backing Board and Coreboard and Gypsum Shaftliner Board	Table 2506.2
 C 472— 99	Specification for Standard Test Methods for Physical Testing of Gypsum,
Gypsum Plasters and Gypsum Concrete	Table 2506.2
 C 473—00	Test Method for Physical Testing of Gypsum Panel Products	Table 2506.2
 C 474—01	Test Methods for Joint Treatment Materials for Gypsum Board Construction	Table 2506.2
 C 475—01	Specification for Joint Compound and Joint Tape for Finishing Gypsum Wallboard	Table 2506.2
 C 476—01	Specification for Grout for Masonry	2103.10, 2105.2.2.1.1, 2105.2.2.1.2
 C 503—99e01	Specification for Marble Dimension Stone (Exterior)	2103.3
 C 514—01	Specification for Nails for the Application of Gypsum Board	Table 721.1(2), Table 721.1(3), Table 2306.4.5, Table 2506.2
 C 516—02 E01	Specifications for Vermiculite Loose Fill Thermal Insulation	721.3.1.4, 721.4.1.1.3
 C 547—00	Specification for Mineral Fiber Pipe Insulation	Table 721.1(2), Table 721.1(3)
 C 549—02 81 (1995)	Specification for Perlite Loose Fill Insulation	721.3.1.4, 721.4.1.1.3
 C 557—99	Specification for Adhesives for Fastening Gypsum Wallboard to Wood Framing	Table 2506.2
 C 568—99	Specification for Limestone Dimension Stone	2103.3
 C 587—97	Specification for Gypsum Veneer Plaster	Table 2507.2
 C 588/C 588M—01	Specification for Gypsum Base for Veneer Plasters	Table 2507.2
 C 595—00	Specification for Blended Hydraulic Cements	 1904.1, Table 1904.2.3
 C 595—01	Specification for Blended Hydraulic Cements	Table 2103.7(1), Table 2507.2
 C 615—99	Specification for Granite Dimension Stone	2103.3
 C 616—99	Specification for Quartz-based Dimension Stone	2103.3
 C 618—99	Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan for
Use as a Mineral Admixture in Concrete	1904.1, Table 1904.2.3
 C 629—99	Specification for Slate Dimension Stone	2103.3
 C 630/C 630M—01	Specification for Water-resistant Gypsum Backing Board	Table 2506.2
 C 631—00	Specification for Bonding Compounds for Interior Gypsum Plastering	Table 2507.2
 C 635—00	Specification for the Manufacturer, Performance, and Testing of Metal Suspension
Systems for Acoustical Tile and Lay-in Panel Ceilings	803.9.1.1, 2506.2.1
 C 636—96	Practice for Installation of Metal Ceiling Suspension Systems for Acoustical Tile and Lay-in Panels	803.9.1.1
 C 645—00	Specification for Nonstructural Steel Framing Members	Table 2506.2, Table 2507.2
 C 652—01A	Specification for Hollow Brick (Hollow Masonry Units Made from Clay or Shale)	2103.2, 2105.2.2.1.1
 C 685/ C 685M—98a	Specification for Concrete Made by Volumetric Batching and Continuous Mixing	1905.8.2
 C 744—99	Specification for Prefaced Concrete and Calcium Silicate Masonry Units	2103.1
 C 754—00	Specification for Installation of Steel Framing Members to Receive
Screw-attached Gypsum Panel Products	Table 2508.1, Table 2511.1
 C 836—00	Specification for High-solids Content, Cold Liquid-applied Elastomeric
Waterproofing Membrane for Use with Separate Wearing Course	1507.15.2
 C 840—01	Specification for Application and Finishing of Gypsum Board	Table 2508.1, 2509.2
 C 841—99	Specification for Installation of Interior Lathing and Furring	Table 2508.1, Table 2511.1
 C 842—99	Specification for Application of Interior Gypsum Plaster	Table 2511.1, 2511.3, 2511.4
 C 843—99	Specification for Application of Gypsum Veneer Plaster	Table 2511.1
 C 844—99	Specification for Application of Gypsum Base to Receive Gypsum Veneer Plaster	Table 2508.1
 C 845—96	Specification for Expansive Hydraulic Cement	1904.1, Table 1904.2.3
 C 847—00 	Specification for Metal Lath	Table 2507.2
 C 887—(2001)	Specification for Packaged, Dry Combined Materials for Surface Bonding Mortar	1807.2.2, 2103.8
 C 897—00	Specification for Aggregate for Job-Mixed Portland Cement-Based Plasters	Table 2507.2
 C 926—98a	Specification for Application of Portland Cement Based-Plaster	2510.3, Table 2511.1, 2511.3, 2511.4, 2512.1, 2512.1.2
  2512.2, 2512.6, 2512.8.2, 2513.7, 2512.9
 C 931/C 931M—01	Specification for Exterior Gypsum Soffit Board	Table 2506.2
 C 932—98a	Specification for Surface-applied Bonding Agents for Exterior Plastering	Table 2507.2
 C 933—A(2001)	Specification for Welded Wire Lath	Table 2507.2
 C 946—91 (2001)	Specification for Practice for Construction of Dry-stacked, Surface-bonded Walls	2103.8, 2109.2.3.2
 C 954—00	Specification for Steel Drill Screws for the Application of Gypsum Panel Products
or Metal Plaster Bases to Steel Studs from 0.033 inch (0.84 mm) to
0.112 inch (2.84 mm) in Thickness	2211.2.2.2, Table 2506.2, Table 2507.2
 C 955—01	Specification for Load Bearing Transverse and Axial Steel Studs, Runners Tracks,
and Bracing or Bridging, for Screw Application of Gypsum Panel Products
and Metal Plaster Bases	Table 2506.2, Table 2507.2
 C 956—97	Specification for Installation of Cast-in-place Reinforced Gypsum Concrete	1915.1
 ASTM—continued
 C 957—98	Specification for High-solids Content, Cold Liquid-applied Elastomeric
Waterproofing Membrane with Integral Wearing Surface	1507.15.2
 C 960—97	Specification for Predecorated Gypsum Board	Table 2506.2
 C 989—99	Specification for Ground Granulated Blast-furnace Slag for Use in Concrete and Mortars	1904.1, Table 1904.2.3
 C1002—01	Specification for Steel Self-Piercing Tapping Screws for the Application
of Gypsum Panel Products or Metal Plaster Bases to Wood Studs or Steel Studs	Table 2506.2, Table 2507.2
 C1007—00	Specification for Installation of Load Bearing (Transverse and Axial)
Steel Studs and Related Accessories	Table 2508.1, Table 2511.1
 C1019—00B	Test Method of Sampling and Testing Grout 	2105.2.2.1.1, 2105.2.2.1.2
 C1029—96	Specification for Spray-applied Rigid Cellular Polyurethane Thermal Insulation	1507.14.2
 C1032—96	Specification for Woven Wire Plaster Base	Table 2507.2
 C1047—99Specification for Accessories for Gypsum Wallboard and Gypsum Veneer Base	Table 2506.2, Table 2507.2
 C1063—99	Specification for Installation of Lathing and Furring to Receive Interior
and Exterior Portland Cement Based Plaster 	2510.3, Table 2511.1, 2512.1.1
 C1088—01A	Specification for Thin Veneer Brick Units Made from Clay or Shale	2103.2
 C1157—00A 	Performance Specification for Hydraulic Cement	1904.1, Table 1904.2.3
 C1167—96	Specification for Clay Roof Tiles	1507.3.4, 1507.3.5
 C1177/C1177M—01	Specification for Glass Mat Gypsum Substrate for Use as Sheathing	Table 2506.2
 C1178/C1178M—01	Specification for Glass Mat Water-resistant Gypsum Backing Panel	Table 2506.2
 C1186—99 	Specification for Flat Nonasbestos Fiber Cement Sheets	 1404.10
 C1218/ C1218M—99	Test Method for Water-soluble Chloride in Mortar and Concrete	1904.4.1
 C1240—00E1	Specification for Silica Fume for Use as a Mineral Admixture in
Hydraulic-Cement Concrete, Mortar and Grout	1904.1, Table 1904.2.3
 C1261—98	Specification for Firebox Brick for Residential Fireplaces	2111.5, 2111.8
 C1278/C 1278M—01	Specification for Fiber-reinforced Gypsum Panels	Table 2506.2
 C1280—99	Specification for Application of Gypsum Sheathing	Table 2508.1, 2508.1,Table 2508.2, 2508.2
 C1283—00	Practice for Installing Clay Flue Liners	2113.12
 C1314—02	Test Method for Compressive Strength of Masonry Prisms	2105.2.2.2.2, 2105.3.1, 2105.3.2
 C1328—00	Specification for Plastic (Stucco Cement)	Table 2507.2
 C1329—00	Specification for Mortar Cement	Table 2103.7(1)
 C1395/1395M—01	Specification for Gypsum Ceiling Board	Table 2506.2
 D 25—99E01	Specification for Round Timber Piles	1809.1.1
 D 41—E01	Specification for Asphalt Primer Used in Roofing, Dampproofing and Waterproofing	Table 1507.10.2
 D 43—00	Coal Tar Primer Used in Roofing, Dampproofing and Waterproofing 	Table 1507.10.2
 D 56—02A 01	Test Method for Flash Point By Tag Closed Tester	307.2
 D 86—01e01	Test Method for Distillation of Petroleum Products	307.2
 D 93—02a 00 	Test Method for Flash Point By Pensky-Martens Closed Cup Tester	307.2
 D 224—89 (1996)	Specification for Smooth-Surfaced Asphalt Roll Roofing (Organic Felt)	1507.2.9.2, 1507.6.4
 D 225—01	Specification for Asphalt Shingles (Organic Felt) Surfaced with Mineral Granules	1507.2.5
 D 226—97a	Specification for Asphalt-Saturated Organic Felt Used in
 Roofing and Waterproofing	1404.2, Table 1507.2, 1507.2.3, 1507.3.3, 1507.5.3, 1507.6.3,
 1507.7.3, Table 1507.8, 1507.8.3, 1507.9.3, 1507.9.4, Table 1507.10.2
 D 227—97a	Specification for Coal-tar-saturated Organic Felt Used in Roofing and Waterproofing	Table 1507.10.2
 D 249—89 (1996)	Specification for Asphalt Roll Roofing (Organic Felt) Surfaced with Mineral Granules	1507.3.3, 1507.6.4
 D 312—00	Specification for Asphalt Used in Roofing	Table 1507.10.2
 D 371—89 (1996)	Specification for Asphalt Roll Roofing (Organic Felt) Surfaced with Mineral Granules: Wide-selvage	1507.6.4
 D 422—63(98) 	Test Method for Particle-size Analysis of Soils	1802.3.2
 D 450—00	Specification for Coal-tar Pitch Used in Roofing, Dampproofing and Waterproofing	Table 1507.10.2
 D 635—98	Test Method for Rate of Burning and/or Extent and Time of Burning of
Self-Supporting Plastics in a Horizontal Position	2606.4
 D1143—81 (1994) E01	Test Method for Piles Under Static Axial Compressive Load	1808.2.8.3
 D1227—00	Specification for Emulsified Asphalt Used as a Protective Coating for Roofing	Table 1507.10.2, 1507.15.2
 D1557—00	Test Method for Laboratory Compaction Characteristics of Soil Using
Modified Effort (56,000 ft-lb/ft3 (2,700 KN m/m3))	1803.5
 D1586—99	Specification for Penetration Test and Split-barrel Sampling of Soils	1615.1.5
 D1761—88(2000)	Test Method for Mechanical Fasteners in Wood	1715.1.1, 1715.1.2, 1715.1.3
 D1863—93 (2000)	Specification for Mineral Aggregate Used on Built-up Roofs	Table 1507.10.2
 D1929—96 (2001)E01	Test Method for Determining Ignition Properties of Plastics	402.14.4, 406.5.2, 1407.11.2.1, 2606.4
 D1970—01	Specification for Self-Adhering Polymer Modified Bituminous Sheet Materials
Used as Steep Roof Underlayment for Ice Dam Protection	1507.2.4, 1507.2.9.2
 D2166—00	Test Method for Unconfined Compressive Strength of Cohesive Soil	1615.1.5
 ASTM—continued
 D2178—97a	Specification for Asphalt Glass Felt Used in Roofing and Waterproofing	Table 1507.10.2
 D2216—98	Test Method for Laboratory Determination of Water(Moisture) Content of Soil and Rock by Mass	1615.1.5
 D2487—00	Practice for Classification of Soils for Engineering Purposes (Unified Soil Classification System)	Table 1610.1, 1802.3.1
 D2626—97b	Specification for Asphalt Saturated and Coated Organic Felt Base Sheet Used in Roofing	1507.3.3, Table 1507.10.2
 D2822—91(97) el	Specification for Asphalt Roof Cement	Table 1507.10.2
 D2823—90(97) el	Specification for Asphalt Roof Coatings	Table 1507.10.2
 D2843—99	Test for Density of Smoke from the Burning or Decomposition of Plastics	2606.4
 D2850—95(1999)	Test Method for Unconsolidated, Undrained Triaxial Compression Test on Cohesive Soils	1615.1.5
 D2898—94 (1999)	Test Methods for Accelerated Weathering of Fire-Retardant-Treated Wood for Fire Testing	1505.1, 2303.2.1, 2303.2.3
 D3019—e01(Supp)	Specification for Lap Cement Used with Asphalt Roll Roofing,
Nonfibered, Asbestos Fibered, and Nonasbestos Fibered	Table 1507.10.2
 D3161—99a	Test Method for a Wind Resistance of Asphalt Shingles (Fan Induced Method)	1507.2.7
 D3201—94 (1998) el	Test Method for Hygroscopic Properties of Fire-Retardant Treated Wood and Wood-base Products	2303.2.4
 D3278—96e01	Test Methods for Flash Point of Liquids by Small Scale Closed-Cup Apparatus	307.2
 D3462—01E01	Specification for Asphalt Shingles Made from Glass Felt and Surfaced with Mineral Granules	1507.2.5
 D3468—99	Specification for Liquid-applied Neoprene and Chlorosulfonated Polyethylene
Used in Roofing and Waterproofing	1507.15.2
 D3679—01c(Supp)	Specification for Rigid Poly [Vinyl Chloride (PVC) Siding]	1404.9, 1405.13
 D3689—90 (1995)	Method for Testing Individual Piles Under Static Axial Tensile Load	1808.2.8.5
 D3737—01B	Practice for Establishing Allowable Properties for Structural Glued Laminated Timber (Glulam)	2303.1.3
 D3746—85 (1996) el	Test Method for Impact Resistance of Bituminous Roofing Systems	1504.7
 D3747—E01	Specification for Emulsified Asphalt Adhesive for Adhering Roof InsulationTable	 1507.10.2
 D3909—97b	Specification for Asphalt Roll Roofing (Glass Felt) Surfaced with Mineral Granules	1507.6.4, Table 1507.10.2
 D4022—94(00)e1	Specification for Coal Tar Roof Cement, Asbestos Containing	Table 1507.10.2
 D4272—99	Test Method for Total Energy Impact of Plastic Films by Dart Drop	1504.7
 D4318—00	Test Methods for Liquid Limit, Plastic Limit, and Plasticity Index of Soils	1615.1.5, 1802.3.2
 D4434—96	Specification for Poly (Vinyl Chloride) Sheet Roofing	1507.13.2
 D4479—00	Specification for Asphalt Roof Coatings - Asbestos-Free	Table 1507.10.2
 D4586—00	Specification for Asphalt Roof Cement, Asbestos-Free	Table 1507.10.2
 D4601—98	Specification for Asphalt-Coated Glass Fiber Base Sheet Used in Roofing	Table 1507.10.2
 D4637—96	Specification for EPDM Sheet Used in Single-ply Roof Membrane	1507.12.2
 D4829—95	Test Method for Expansion Index of Soils	1802.3.2
 D4869—88(93)e1	Specification for Asphalt-Saturated (Organic Felt) Underlayment Used in Steep Slope Roofing	Table1507.2, 1507.2.3
 D4897—01	Specification for Asphalt-Coated Glass Fiber Venting Base Sheet Used in Roofing	Table 1507.10.2
 D4990—97a	Specification for Coal Tar Glass Felt Used in Roofing and Waterproofing	Table 1507.10.2
 D4945—00	Test Method for High-Strain Dynamic Testing of Piles P	1808.2.8.3
 D5019—96 	Specification for Reinforced Nonvulcanized Polymeric Sheet Used in Roofing Membrane	1507.12.2
 D5055—00	Specification for Establishing and Monitoring Structural Capacities of Prefabricated Wood I-joists	2303.1.2
 D5456—01AE01	Specification for Evaluation of Structural Composite Lumber Products	2303.1.9
 D5516—99a	Test Method of Evaluating the Flexural Properties of Fire-Retardant Treated
Softwood Plywood Exposed to the Elevated Temperatures	2303.2.2.1
 D5643—94(00)e1 	Specification for Coal Tar Roof Cement, Asbestos-Free	Table 1507.10.2
 D5664—01	Test Methods for Evaluating the Effects of Fire-Retardant Treatment and
Elevated Temperatures on Strength Properties of Fire-Retardant Treated Lumber	2303.2.2.2
 D5665—99a	Specification for Thermoplastic Fabrics Used in Cold-Applied Roofing and Waterproofing	Table 1507.10.2
 D5726—98	Specification for Thermoplastic Fabrics Used in Hot-Applied Roofing and Waterproofing	Table 1507.10.2
 D6083—97a	Specification for Liquid Applied Acrylic Coating Used in Roofing	Table 1507.10.2, 1507.15.2
 D6162—00A	Specification for Styrene Butadiene Styrene (SBS) Modified Bituminous
Sheet Materials Using a Combination of Polyester and Glass Fiber Reinforcements	1507.11.2
 D6163—00 E01	Specification for Styrene Butadiene Styrene (SBS) Modified Bituminous
Sheet Materials Using Glass Fiber Reinforcements	1507.11.2
 D6164—00	Specification for Styrene Butadiene Styrene (SBS) Modified Bituminous
Sheet Metal Materials Using Polyester Reinforcements	1507.11.2
 D6222—00e0198 	Specification for Atactic Polypropylene (APP) Modified Bituminous
Sheet Materials Using Polyester Reinforcements	1507.11.2
 D6223—00e0198 	Specification for Atactic Polypropylene (APP) Modified Bituminous
Sheet Materials Using a Combination of Polyester and Glass Fiber Reinforcements	1507.11.2
 D6298—98 	Specification for Fiberglass Reinforced Styrene-Butadiene-Styrene (SBS) Modified Bituminous Sheets with a Factory Applied Metal Surface	1507.11.2
 D6305—99e1	Practice for Calculating Bending Strength Design Adjustment Factors for
Fire-Retardant-Treated Plywood Roof Sheathing	2303.2.2.1
 ASTM—continued
 E 84—01	Test Methods for Surface Burning Characteristics of Building Materials	 402.10, 402.14.4, 406.5.2, 410.3.5.3,
  703.4.2, 719.1, 719.4, 802.1, 803.1, 803.5, 803.6.1, 803.6.2,
1407.10, 1407.10.1, 2303.2, 2603.3, 2603.4.1.13, 2603.5.4, 2604.2.4, 2606.4, 3105.3
 E 90—99	Test Method for Laboratory Measurement of Airborne Sound Transmission
Loss of Building Partitions and Elements	1207.2
 E 96—00	Test Method for Water Vapor Transmission of Materials	1203.2
 E 108—00	Test Methods for Fire Tests of Roof Coverings	1505.1, 2603.6, 2610.2, 2610.3
 E 119—00a 	Test Methods for Fire Tests of Building Construction and Materials	 410.3.5.2, 703.2, 703.2.1, 703.2.3,
 703.3, 704.7, 704.9, 706.7, 711.3.2, 712.3.1, 712.4.1, 712.4.6, 713.1, 713.4, 714.7, 715.2,
716.5.2, 715.5.3.1, 715.6.2, 716.5.2, 716.5.3.1, 716.6.2, Table 721.1(1), 1407.10.2,
2103.2, 2603.3, 2603.4, 2603.4.1.13, 2603.5.4, 2604.2.4, 2606.4
 E 136—99e1 	Test Method for Behavior of Materials in a Vertical Tube Furnace at 750°C	703.4.1
 E 328—86	Methods for Stress Relaxation for Materials and Structures 	2103.11.6
 E 330—97e1 	Test Method for Structural Performance of Exterior Windows, Curtain Walls,
and Doors by Uniform Static Air Pressure Difference	1714.5.2
 E 331—00	Test Method for Water Penetration of Exterior Windows, Skylights, Doors,
and Curtain Walls by Uniform Static Air Pressure Difference	1403.2
 E 492—90 (1996)e1	Test Method for Laboratory Measurement of Impact Sound Transmission
Through Floor-ceiling Assemblies Using the Tapping Machine	1207.3
 E 605—00	Test Method for Thickness and Density of Sprayed Fire-resistive Material (SFRM)
Applied to Structural Members	1704.11.3, 1704.11.3.1, 1704.11.3.2, 1704.11.4
 E 681—01	Test Methods for Concentration Limits of Flammability of Chemical Vapors and Gases	307.2
 E 736—00	Test Method for Cohesion/Adhesion of Sprayed Fire-resistive Materials Applied to Structural Members	1704.11.5
 E 814—0200	Test Method of Fire Tests of Through-penetration Firestops	702.1, 712.3.1.2, 712.4.1.2
 E 970—00	Test Method for Critical Radiant Flux of Exposed Attic Floor Insulation Using a Radiant Heat Energy Source	719.3.1
 E1300—00	Practice for Determining Load Resistance of Glass in Buildings	Table 2404.1, Table 2404.2
 E1592—01	Test Method for Structural Performance of Sheet Metal Roof and Siding Systems
by Uniform Static Air Pressure Difference 	1504.3.2
 E1602—01	Guide for Construction of Solid Fuel-Burning Masonry Heaters	2112.2
 E1886—97	Test Method for Performance of Exterior Windows, Curtain Wall, Doors and
Storm Shutters Impacted by Missiles and exposed to Cyclic Pressure Differentials	1609.1.4
 E1966—00	Test Method for Fire-Resistant Joint Systems	702.1, 712.3
 E1996—01	Specification for Performance of Exterior Windows, Glazed Curtain Walls, Doors
and Storm Shutters Impacted by Windborne Debris in Hurricanes	1609.1.4
 F 547—01	Terminology of Nails for Use with Wood and Wood-base Materials	Table 2506.2
 F1346—91 (1996)	Performance Specification for Safety Covers and Labeling Requirements for
All Covers for Swimming Pools, Spas and Hot Tubs	3104.9, 3109.4.1.8
 F1667—01A	Specification for Driven Fasteners: Nails, Spikes, and Staples	Table 721.1(2), Table 721.1(3),
 1507.2.6, 2303.6, Table 2506.2
 G 152—00A	Practice for Operating Open Flame Carbon Arc Light Apparatus for Exposure of Nonmetallic Materials	1504.5
 G 154—00A	Practice for Operating Fluorescent Light Apparatus for UV Exposure of Nonmetallic Materials	1504.5
 G 155—00Ae1 	Practice for Operating Xenon Arc Light Apparatus for Exposure of Non-Metallic Materials	1504.5
 American Wood-Preservers’ Association
P.O. Box 5690
Grandbury, TX 76049
 AWPA
Standard							Referenced
reference						in code
number		Title					section number
 C1—00	All Timber Products—Preservative Treatment by Pressure Processes	1403.6, 1505.6, 2303.1.8
 C2—01	Lumber, Timber, Bridge Ties and Mine Ties—Preservative Treatment by Pressure Processes	1403.6, Table 1507.9.5,
 1805.4.5, 1805.7.1, 2303.1.8, 2304.11.2, 2304.11.4, 2304.11.7
 C3—99	Piles—Preservative Treatment by Pressure Processes	1403.6, 1805.4.5, 1809.1.2, 2303.1.8
 C4—99	Poles—Preservative Treatment by Pressure Processes	1403.6, 1805.7.1, 1808.1.2, 2303.1.8
 C9—00	Plywood—Preservative Treatment by Pressure Processes	1403.6, 2303.1.8, 2304.11.2, 2304.11.4, 2304.11.7
 C14—99	Wood for Highway Construction, Pressure Treatment by Pressure Process	2303.1.8
 C15—00	Wood for Commercial-Residential Construction Preservative Treatment by Pressure Process	1403.6, 2303.1.8
 C16—00	Wood Used on Farms, Pressure Treatment by Pressure Process	 2303.1.8
 C18—99	Standard for Pressure Treated Material in Marine Construction	 1403.6
 C22—96	Lumber and Plywood for Permanent Wood Foundations—Preservative
Treatment by Pressure Processes	1403.6, 1805.4.6, 2303.1.8
 AWPA—continued
C23—00	Round Poles and Posts Used in Building Construction—Preservative Treatment by Pressure Processes	1403.6, 2303.1.8
C24—96	Sawn Timber Piles Used to Support Residential and Commercial Structures	1403.6, 1809.1.2, 2303.1.8
C28—99	Standard for Preservative Treatment by Pressure Process of Structural Glued Laminated
Members and Laminations before Gluing	1403.6, 2303.1.8
C31—0100 	Lumber Used Out of Contact with the Ground and Continuously Protected from LiquidWater—Treatment by Pressure Processes	 2303.1.8
C33—00	Standard for Preservative Treatment of Structural Composite Lumber by Pressure Processes	2303.1.8
M4—01	Standard for the Care of Preservative-Treated Wood Products	1809.1.2, 2303.1.8
P1/13—01	Standard for Creosote Preservative	1403.6, 2303.1.8
P2—01	Standard for Creosote Solutions	1403.6, 2303.1.8
P3—01	Standard for Creosote-Petroleum Solution	1403.6
P5—01	Standard for Waterborne Preservatives	2303.1.8
P8—01	Standard for Oil-borne Preservatives	2303.1.8
P9—01	Standard for Solvents and Formulations for Organic Preservative Systems	2303.1.8
283;>

American Welding Society
550 N.W. LeJeune Road
Miami, FL 33126
 AWS
Standard							Referenced
reference						in code
number		Title					section number
 D1.1—00	Structural Welding Code—Steel	Table 1704.3, 1704.3.1, 1708.4
 D1.3—98	Structural Welding Code—Sheet Steel	Table 1704.3
 D1.4—98	Structural Welding Code—Reinforcing Steel	Table 1704.3, 1903.5.2
Builders Hardware Manufacturers’ Association
355 Lexington Avenue, 17th Floor
New York, NY 10017-6603
 BHMA
Standard							Referenced
reference						in code
number		Title					section number
 A 156.10—99	American National Standard for Power Operated Pedestrian Doors	1008.1.3.2
 A 156.19—97	American National Standard for Power Assist and Low Energy Operated Doors	1008.1.3.2
 Canadian General Standards Board
222 Queens Street
14th Floor, Suite 1402
Ottawa, Ontario, Canada KIA 1G6
 CGSB
Standard							Referenced
reference						in code
number		Title					section number
 37-GP-52M (1984)	Roofing and Waterproofing Membrane, Sheet Applied, Elastomeric	1504.7, 1507.12.2
 CAN/CGSB 37.54—95	Polyvinyl Chloride Roofing and Waterproofing Membrane	1507.13.2
 37-GP-56M (1980)	Membrane, Modified, Bituminous, Prefabricated, and Reinforced for Roofing—
with December 1985 Amendment	1507.11.2
 Consumer Product Safety Commission4330 East West Highway
Bethesada, MD 20814-4408
 CPSC
Standard							Referenced
reference						in code
number		Title					section number
16 CFR Part 1201(1977)	Safety Standard for Architectural Glazing Material	2406.1.1, 2406.2.1, 2407.1, 2408.2.1, 2408.3
16 CFR Part 1209 (1979)	Interim Safety Standard for Cellulose Insulation	719.6
16 CFR Part 1404 (1979)	Cellulose Insulation	719.6
16 CFR Part 1500 (1991)	Hazardous Substances and Articles; Administration and Enforcement Regulations	307.2
16 CFR Part 1500.44 (2001)	Method for Determining Extremely Flammable and Flammable Solids	307.2
16 CFR Part 1507 (2001)	Fireworks Devices	307.2
16 CFR Part 1630 (2000)	Standard for the Surface Flammability of Carpets and Rugs	804.5.1
 Cedar Shake and Shingle Bureau
P.O. Box 1178
Sumas, WA 98295-1178
 CSSB
Standard							Referenced
reference						in code
number		Title					section number
 CSSB—97	Grading and Packing Rules for Western Red Cedar Shakes and Western Red Shingles
of the Cedar Shake and Shingle Bureau	Table 1507.8.4, Table 1507.9.5
 Door and Access Systems Manufacturers
Association International
1300 Summer Avenue 
Cleveland, OH 44115-2851
 DASMA
Standard							Referenced
reference						in code
number		Title					section number
 107—97	Room Fire Test Standard for Garage Doors Using Foam Plastic Insulation	2603.4.1.9
 U.S. Department of Commerce
National Institute of Standards and Technology
100 Bureau Drive Stop 3460
Gaithersburg, MD 20899
 DOC
Standard							Referenced
reference						in code
number		Title					section number
 PS-1—95	Construction and Industrial Plywood	2211.2.2.2, 2303.1.4, 2304.6.2, Table 2304.7(4), 2306.3.2
 PS-2—92	Performance Standard for Wood-based Structural-use Panels	1809.1.1, 2211.3.1, 2303.1.4, 2304.6.2,
 Table 2304.7(4), Table 2304.7(5), Table 2306.3.1, 2306.3.2
 PS 20—99	American Softwood Lumber Standard	1809.1.1, 2302.1, 2303.1.1
 U.S. Department of Labor
c/o Superintendent of Documents
U.S. Government Printing Office
Washington, DC 20402-9325
 DOL
Standard							Referenced
reference						in code
number		Title					section number
 29 CFR Part 1910.1000 (1974)	Air Contaminants		902.1
 U.S. Department of Transportation
c/o Superintendent of Documents
U.S. Government Printing Office
Washington, DC 20402-9325
 DOTn
Standard							Referenced
reference						in code
number		Title					section number
 49 CFR Part 172 (1999) Hazardous Materials Tables, Special Provisions, Hazardous Materials Communications,
Emergency Response Information and Training Requirements	307.2
 49 CFR Parts 173 (1999)	Specification of Transportation of Explosive and Other Dangerous Articles, UN 0335,UN 0336 Shipping Containers 	307.2
 Federal Emergency Management Agency
Federal Center Plaza
500 C Street S.W.
Washington, DC 20472
 FEMA
Standard							Referenced
reference						in code
number		Title					section number
 Pub 302NEHRP	 Recommended Provisions for Seismic Regulations for
New Buildings and Other Structures	Figure 1615(7), Figure 1615(8), Figure 1615(9), Figure 1615(10)
 TB11-01	Crawlspace Construction for Buildings Located in Special Flood Hazard Areas	1807.1.2.1

 Factory Mutual
Standards Laboratories Department
1151 Boston-Providence Turnpike
Norwood, MA 02062
 FM
Standard							Referenced
reference						in code
number		Title					section number
 4450 (1989) 	Approval Standard for Class 1 Insulated Steel Deck Roofs—
with Supplements thru 7/92	1504.3.1, 1508.1, 2603.3, 2603.4.1.5
 4470 (1992) 	Approval Standard for Class 1 Roof Covers	1504.3.1, 1504.7
 4880 (2001)	 American National Standard for Evaluating Insulated Wall or Wall and
Roof/Ceiling Assemblies, Plastic Interior Finish Materials, Plastic Exterior
Building Panels, Wall/Ceiling Coating Systems, Interior and Exterior Finish Systems	2603.4, 2603.8
 Gypsum Association
810 First Street N.E. #510
Washington, DC 20002-4268
 GA
Standard							Referenced
reference						in code
number		Title					section number
 GA 216—00	Application and Finishing of Gypsum Board	Table 2508.1, 2509.2
 GA 600—00	Fire-resistance Design Manual,16th Edition, April, 2000	Table 721.1(1), Table 721.1(2), Table 721.1(3)
 Hardwood Plywood Veneer Association
1825 Michael Faraday Drive
Reston, VA 20190-5350
 HPVA
Standard							Referenced
reference						in code
number		Title					section number
 HP-1—2000 	The American National Standard for Hardwood and Decorative Plywood	2303.3, 2304.6.2

Florida CODES
 International Code Council
5203 Leesburg Pike, Suite 600
Falls Church, VA 22041
 ICC
Standard							Referenced
reference						in code
number		Title					section number
Ch.11 FBC-B 04 ICC/ANSI A117.1—98 	Ch.11, Florida Building Code, Building (Florida Accessibility Code for Building Construction) Accessible and Usable Buildings and Facilities	406.2.2, 907.9.1.3,1007.6.5, 1010.1, 1010.6.5, 1010.9, 1011.3,
 1101.2, 1102.1, 1103.2.13, 1106.6, 1107.2, 1109.2.2, 1109.3,
1109.4, 1109.8, 1109.15, 3001.3, 3409.5, 3409.7.2, 3409.7.3
 ICC 300—02ICC Standard on Bleachers, Folding and Telescopic Seating, and Grandstands1024.1.1
Ch.27 FBC-B 04 ICC EC—03 	Ch. 27 Florida Building Code, Building (Electrical Systems) ICC Electrical Code™	101.4.1, 107.3, 414.5.4, 414.9.2.8.1, 904.3.1, 907.5, 909.11,
 909.12.1, 909.16.3, 1205.4.1, 1405.10.4, 2701.1, 2702.1, 3401.3
FEBC 04 IEBC–—03	Florida International Existing Building Code™101.2
Ch.13 FBC-B 04  IECC—03	Ch. 13 Florida Building Code, Building (Energy Efficiency) International Energy Conservation Code®101.4.7, 1202.3.2, 1301.1.1, 1403.2
 ICC—continued
FFPC 04 IFC—03 	Florida Fire Prevention Code International Fire Code®	101.4.6, 102.6, 201.3, 307.9, Table 307.7(1), Table 307.7(2), 307.9,
 404.2,406.5.1, 406.5.2, 406.6.1, 410.3.6, 411.1, 412.4.1, 413.1, 414.1.1, 414.1.2,
414.1.2.1, 414.2.4, Table 414.2.4, 414.3, 414.5, 414.5.1, Table 414.5.1, 414.5.2,
414.5.4, 414.5.5, 414.6, 415.1, 415.3, 415.3.1, Table 415.3.1, Table 415.3.2, 415.7, 415.7.1,
415.7.1.4, 415.7.2, 415.7.2.3, 415.7.2.5, 415.7.2.7, 415.7.2.8, 415.7.2.9, 415.7.3, 415.7.3.3.3, 415.7.3.5,
415.7.4, 415.8, 415.9.1, 415.9.2.7, 415.9.5.1, 415.9.7.2, 704.8.2, 706.1, 901.2, 901.3, 901.5,
901.6.2, 903.2.6.1, 903.2.11, Table 903.2.13, 903.5, 904.2.1, 905.1, 906.1, 907.2.5, 907.2.12.2, 907.2.14,
907.2.16, 907.19, 909.20, 910.2.3, Table 910.3, 1001.3, 1203.4.2, 1203.5, 2702.2.8, 2702.2.10,
2702.2.11, 2702.2.12, 2702.3, 3102.1, 3103.1, 3309.2, 3401.3, 3410.3.2, 3410.6.8.1, 3410.6.14, 3410.6.14.1
FBC-FG 04  IFGC—03	Florida Building Code, International Fuel Gas Code®101.4.2, 201.3, 415.7.3, 2113.11.1.2, 2113.15, 2801.1, 3401.3
FBC-M 04  IMC—03	Florida Building Code, International Mechanical Code®	101.4.3, 201.3, 307.9, 406.4.2, 406.6.3, 406.6.5, 409.3, 412.4.6, 414.1.2,
 414.1.2.1, 414.1.2.2, 414.3, 415.7.1.4, 415.7.2, 415.7.2.8, 415.7.3, 415.7.4, 415.9.11.1,
416.3, 603.1, 707.2, 716.2.2, 716.5.4, 716.6.1, 716.6.2, 716.6.3, 717.5, 719.1, 903.2.12.1,
904.2.1, 904.11, 908.6, 909.1, 909.10.2, 1014.5, 1016.4.1, 1203.1, 1203.2.1, 1203.4.2,
1203.4.2.1, 1203.5, 1209.3, 2304.5, 3004.3.1, 3410.6.7.1, 3410.6.8
 IPC—03International Plumbing Code®101.4.4, 201.3, 415.7.4, 717.5, 903.3.5, 1206.3.3, 1503.4,
 1807.4.3, 2901.1, 2902.1.1, 3305.1, 3401.3,
 IPMC—03International Property Maintenance Code®101.4.5, 102.6, 103.3, 3401.3, 3410.3.2.
64E 04  IPSDC—03Rule 64E, Florida Administrative Code (sewage disposal) International Private Sewage Disposal Code®	101.4.4, 2901.1, 3401.3
FRC 04 IRC—03	Florida International Residential Code®	101.2, 308.3, 308.5 1706.1.1, 3401.3
 IUWIC—03International Urban—Wildland Interface Code™	Table 1505.1
 SBCCI SSTD 10—99	Standard for Hurricane Resistant Residential Construction	1609.1.1, 2308.2.1
 SBCCI SSTD 11—97	Test Standard for Determining Wind Resistance of Concrete or Clay Roof Tiles	1715.2.1, 1715.2.2
 UBC Standard 18-2	Expansion Index Test	1802.3.2
 National Association of Architectural
Metal Manufacturers
8 South Michigan Ave
Chicago, IL 60603
 NAAMM
Standard							Referenced
reference						in code
number		Title					section number
 FP 1001—90	Guide Specifications for Design of Metal Flag Poles	1609.1.1
 National Concrete Masonry Association
2302 Horse Pen Road
Herndon, VA 22071-3499
 NCMA
Standard							Referenced
reference						in code
number		Title					section number
 TEK 5-8A (1996)	Details for Concrete Masonry Fire Walls	Table 719.1(2)
 National Fire Protection Association
1 Batterymarch Park
Quincy, MA 02269-9101
 NFPA
Standard							Referenced
reference						in code
number		Title					section number
 11—0298	Low-, Medium-, and High- Expansion Foam		904.7
 11A—0299	Medium- and High-Eexpansion Foam Systems	904.7
 12—00	Carbon Dioxide Extinguishing Systems904.8, 904.11
 12A—97	Halon 1301 Fire Extinguishing Systems904.9 
 13—0299	Installation of Sprinkler Systems	704.12, 707.2, 903.3.1.1, 903.3.2, 903.3.5.1.1, 904.11, 907.8,
 1621.3.10.1, 3104.5, 3104.9
 13D—0299	Installation of Sprinkler Systems in One- and Two-family Dwellings and Manufactured Homes	903.1.2, 903.3.1.3, 903.3.5.1.1
 13R—0299	Installation of Sprinkler Systems in Residential Occupancies Up to and
Including Four Stories in Height	 903.1.2, 903.3.1.2, 903.3.5.1.1, 903.3.5.1.2, 903.4
 14—0300	Installation of Standpipe, Private Hydrants and Hose Systems	905.2, 905.3.4, 905.4.2, 905.8
 16—0399	Installation of Foam-Water Sprinkler and Foam-Water Spray Systems	904.7, 904.11
 NFPA—continued
 17—0298	Dry Chemical Extinguishing Systems	904.6, 904.11
 17A—0298	Wet Chemical Extinguishing	 Systems	904.5, 904.11
 30—00 	Flammable and Combustible Liquids Code	415.3
 32—00	 Drycleaning Plants	415.7.4
 40—0197	Storage and Handling of Cellulose Nitrate Motion Picture Film	409.1
 61—0299	Prevention of Fires and Dust Explosions in Agricultural and Food Product Facilities	415.7.1
 72—0299	National Fire Alarm Code	505.4, 901.6, 903.4.1, 904.3.5, 907.2,907.2.1, 907.2.1.1, 907.2.10, 907.2.10.4,
 907.2.11.2, 907.2.11.3, 907.2.12.2.3, 907.2.12.3, 907.4, 907.5, 907.9.2,
907.10, 907.14, 907.16,907.17, 911.1, 3006.5
 80—99	Fire Doors and Fire Windows	302.1.1.1, 715.3, 715.4.6.1, 715.4.4, 715.4.7.2, 715.5, 1008.1.3.3 
 85—01	Boiler and Combustion System Hazards Code	415.7.1
(Note: NFPA 8503 has been incorporated into NFPA 85)
 101—0300	Life Safety Code	1024.6.2
 110—0299	Emergency and Standby Power Systems	2702.1
 111—01	Stored Electrical Energy Emergency and Standby Power Systems	2702.1
 120—99	Coal Preparation Plants	415.7.1
 231C—98	Rack Storage of Materials	507.2
 252—99	Standard Methods of Fire Tests of Door Assemblies	715.3.1, 715.3.2, 715.3.3, 715.3.4.1
 253—00	Test for Critical Radiant Flux of Floor Covering Systems Using a Radiant Heat Energy Source 	406.6.4, 804.2, 804.3
 257—00	Standard for Fire Test for Window and Glass Block Assemblies	715.3.3, 715.4, 715.4.1, 715.4.2
 259—0398	Test Method for Potential Heat of Building Materials	2603.4.1.10, 2603.5.3
 265—0298	Standard Method of Fire Tests for Evaluating Room Fire Growth
Contribution of Textile Wall Coverings on Full Height Panels and Walls	803.6.1, 803.6.1.1, 803.6.1.2
 268—96	Standard Test Method for Determining Ignitibility of Exterior Wall
Assemblies Using a Radiant Heat Energy Source	1406.2.1, 1406.2.1.1, 1406.2.1.2, 2603.5.7
 285—98	Standard Method of Test for the Evaluation of Flammability Characteristics
of Exterior Non-load-bearing Wall Assemblies Containing Combustible Components	1407.10.4, 2603.5.5
 286—00	 Standard Method of Fire Test for Evaluating Contribution of Wall and Ceiling
Interior Finish to Room Fire Growth	402.14.4, 803.2, 803.2.1, 803.5, 2603.4, 2603.8
 409—0195	Standard on Aircraft Hangers	412.2.6, 412.4.5
 418—01	Standard for Heliports	412.5.6
 651—98 	Machining and Finishing of Aluminum and the Production and Handling of Aluminum Powders	415.7.1
 654—00	Prevention of Fire & Dust Explosions from the Manufacturing, Processing, and
Handling of Combustible Particulate Solids	415.7.1
 655—0193	Prevention of Sulfur Fires and Explosions	415.7.1
 664—0298	Prevention of Fires Explosions in Wood Processing and Woodworking Facilities	415.7.1
 701—99	Standard Methods of Fire Tests for Flame-Propagation of Textiles and Films	802.1, 805.1, 805.2, 3102.3.1, 3105.3,
 704—0196	Standard System for the Identification of the Hazards of Materials for Emergency Response	414.7.2, 415.2
 1124—0398	Manufacture, Transportation, and Storage and Retail Sales of Fireworks and Pyrotechnic Articles	415.3.1
 2001—00	Clean Agent Fire Extinguishing Systems	904.10

 National Institute of Standards and Technology
U.S. Department of Commerce
100 Bureau Dr. – Stop 3460
Gaithersburg, MD 20899-3460
 NIST
Standard							Referenced
reference						in code
number		Title					section number
 BMS 71—41	Fire Tests of Wood and Metal-framed Partitions	721.7
 TRBM-44—46	Fire-resistance and Sound-insulation Ratings for Walls, Partitions and Floors	721.7
 Precast Prestressed Concrete Institute
175 W. Jackson Boulevard, Suite 1859Chicago, IL 60604-9773
 PCI
Standard							Referenced
reference						in code
number		Title					section number
 MNL 124—89	Design for Fire Resistance of Precast Prestressed Concrete	721.2.3.1, Table 721.2.3(4)
 MNL 128—01	Recommended Practice for Glass Fiber Reinforced Concrete Panels	1903.8
 Post-Tensioning Institute
1717 W. Northern Avenue, Suite 114
Phoenix, AZ 85021
 PTI
Standard							Referenced
reference						in code
number		Title					section number
 PTI 1996	Design and Construction of Post-tensioned Slabs-on-ground, 2nd Edition	1805.8.2
 Rubber Manufacturers Association
1400 K. Street, N.W. #900
Washington, DC 20005
 RMA
Standard							Referenced
reference						in code
number		Title					section number
 RP-1—90	Minimum Requirements for Non-reinforced Black EPDM Rubber Sheets	1507.12.2
 RP-2—90	Minimum Requirements for Fabric-reinforced Black EPDM Rubber Sheets	1507.12.2
 RP-3—85	Minimum Requirements for Fabric-reinforced Black Polychloroprene Rubber Sheets	1507.12.2
 Rack Manufacturers Institute
8720 Red Oak Boulevard, Suite 201
Charlotte, NC 28217
 RMI
Standard							Referenced
reference						in code
number		Title					section number
 RMI (1997)	Design, Testing and Utilization of Industrial Steel Storage Racks	2208.1
 Steel Joist Institute
3127 10th Avenue, North
Myrtle Beach, SC 29577-6760
 SJI
Standard							Referenced
reference						in code
number		Title					section number
 SJI—1994	Standard Specification for Joist Girders	1604.3.3, 2206
 K-Series Specification—1994	Standard Specification for Open Web Steel Joists, K Series	2206
 SJI—1994	Standard Specification for Longspan Steel Joists, LH Series and Deep Longspan Steel Joists, DLH Series	2206
 Single-Ply Roofing Institute
77 Rumford Ave.
Suite 3-B
Walthem, MA 02453
 SPRI
Standard							Referenced
reference						in code
number		Title					section number
 ES-1—98	Wind Design Standard for Edge Systems Used with Low Slope Roofing Systems	1504.5
 RP-4—88	Wind Design Guide for Ballasted Single-ply Roofing Systems	1504.4
 Telecommunications Industry Association
2500 Wilson Boulevard
Arlington, VA 22201-3834
 TIA
Standard							Referenced
reference						in code
number		Title					section number
 TIA/EIA-222-F—96	Structural Standards for Steel Antenna Towers and Antenna Supporting Structures	1609.1.1, 3108.4
 The Masonry Society
3970 Broadway, Unit 201-D
Boulder, CO 80304-1135
 TMS
Standard							Referenced
reference						in code
number		Title					section number
 0216—97	Standard Method for Determining Fire Resistance of Concrete and Masonry Construction Assemblies	Table 721.1(2), 721.1
 402—02	Building Code Requirements for Masonry Structures	1405.5, 1405.5.3, 1405.9, 1604.3.4, 1704.5, 1704.5.1,
 Table 1704.5.1, 1704.5.2, Table 1703.3.1, 1708.1.1, 1708.1.2, 1708.1.3, 1805.5.2, 1812.7,
2101.2.3, 2101.2.4, 2101.2.5, 2103.11.6, 2106.1, 2106.1.1.1, 2106.1.1.2,
2106.1.1.3, 2106.3, 2106.4, 2106.5, 2106.6, 2107.1, 2107.2, 2107.2.1,
 2107.2.2, 2107.2.4, 2107.2.5, 2107.2.6, 2108.1, 2108.2, 2108.4, 2109.1, 2109.2.3.1, 2109.2.3.2
 602—02	Specification for Masonry Structures	1405.5.1, 1405.9.1, Table1704.5.1, Table 1704.5.3, 1805.5.2, 2103.11.7,
 2104.1, 2104.1.1, 2104.3
 Truss Plate Institute
583 D’Onofrio Drive, Suite 200
Madison, WI 53719
 TPI
Standard							Referenced
reference						in code
number		Title					section number
 TPI 1—2002	National Design Standards for Metal-Plate-Connected Wood Truss Construction	2303.4, 2306.1
 Underwriters Laboratories
333 Pfingsten Road
Northbrook, IL 60062-2096
 UL
Standard							Referenced
reference						in code
number		Title					section number
 10A—98	Tin Clad Fire Doors—with Revisions through July, 1998	715.3
 10B—97	Fire Tests of Door Assemblies	715.3.2
 10C—98	Positive Pressure Fire Tests of Door Assemblies—with Revisions thru November, 2001	715.3.1, 715.3.3
 14B—98	Sliding Hardware for Standard Horizontally Mounted Tin Clad Fire Doors—with Revisions through July, 2000 	715.3
 14C—96	Swinging Hardware for Standard Tin Clad Fire Doors Mounted Singly and in Pairs	715.3
 103—0198	Factory-Built Chimneys, for Residential Type and Building Heating Appliances—
with Revisions through March 1999	717.2.5
 127—9699	Factory-Built Fireplaces—with Revisions through November,1999	717.2.5
 268—96	Smoke Detectors for Fire Protective Signaling Systems—with Revisions through January, 1999	407.6, 907.2.6.1
 300—96	Fire Testing of Fire Extinguishing Systems for Protection of
Restaurant Cooking Areas —with Revisions through December, 1998	904.11
 555—9996	Fire Dampers—with Revisions through January, 2002 October, 2000	716.3
 555C—96	Ceiling Dampers	716.3, 716.6.2
 555S—99	Smoke Dampers—with Revisions through January, 2002 December, 1999	716.3, 716.3.1.1
 580—94	Test for Uplift Resistance of Roof Assemblies—with Revisions through February, 1998	1504.3.1, 1504.3.2
 641—95	Type L Low-Temperature Venting Systems—with Revisions through April, 1999	 2113.11.1.4
 790—97	Tests for Fire Resistance of Roof Covering Materials—with Revisions through July, 1998		1505.1, 2603.6, 2610.2, 2610.3
 864—96	Control Units for Fire Protective Signaling Systems—with Revisions through March, 1999	909.12
 1040—96	Fire Test of Insulated Wall Construction—with Revisions thru April, 2001	1407.10.3, 2603.4, 2603.8
 1256—98	Fire Test of Roof Deck Construction—with Revisions through March, 2000	1508.1, 2603.3, 2603.4.1.5
 1479—9594 	Fire Tests of Through-Penetration Firestops 	712.3.1.2, 712.4.1.2
 1715—97	Fire Test of Interior Finish Material	1407.10.2, 1407.10.3, 2603.4, 2603.8
 1777—98	Chimney Liners—with Revisions through July, 1998	2113.11.1, 2113.19
 1784—0195	Air Leakage Tests of Door Assemblies	707.14.1, 710.5.2, 715.3.3, 715.3.5.1
 1897—98	Uplift Tests for Roof Covering Systems—with Revisions through December, 1999	1504.3.1
 1975—96	Fire Test of Foamed Plastics Used for Decorative Purposes	402.10, 402.14.5
 2079—98	Tests for Fire Resistance of Building Joint Systems	702.1, 712.3
 2200—98	Stationary Engine Generator Assemblies 	2702.1.1
 Underwriters Laboratories of Canada
7 Crouse Road
Scarborough, Ontario, Canada M1R3A9
 ULC
Standard							Referenced
reference						in code
number		Title					section number
 S102.2—M88	Standard Method of Test for Surface Burning Characteristics of Floor Coverings,
and Miscellaneous Materials and Assemblies 	719.4
 United States Code
c/o Superintendent of Documents
U.S. Government Printing Office
Washington, DC 20402-9325
 USC
Standard							Referenced
reference						in code
number		Title					section number
 18 USC Part 1, Ch.40	Importation, Manufacture, Distribution and Storage of Explosive Materials	307.2

 Window and Door Manufacturers Association
1400 East Touhy Avenue #470
Des Plaines, IL 60018
 WDMA
Standard							Referenced
reference						in code
number		Title					section number
 AAMA/NWWDA
101/I.S.2—97	Voluntary Specifications for Aluminum, Vinyl (PVC) and Wood Windows and Glass Doors	1714.5.1
 AAMA/NWWDA
101/I.S.2/NAFS—02	Voluntary Performance Specification for Window, Skylights and Glass Doors	1714.5.1, 2405.5
 Wire Reinforcement Institute, Inc.
203 Loudon Street, S.W.
2nd Floor, Suite 203C
Leesburg, VA 22075
 WRI
Standard							Referenced
reference						in code
number		Title					section number
 WRI/CRSI—96	Design of Slab-on-ground Foundations	1805.8.2