CHAPTER 13
REFERENCED STANDARDS

This chapter lists the standards that are referenced in various sections of this document. The standards are listed herein by the promulgating agency of the standard, the standard identification, the effective date and title, and the section or sections of this document that reference the standard. The application of the referenced standards shall be as specified in Section 102.8.
 American National Standards Institute
25 West 43rd Street, Fourth Floor
New York, NY 10036
 ANSI
 Standard									Referenced
Reference									in code
Number		Title								section number
 Z4.3—95	Minimum Requirements for Nonsewered Waste-Disposal Systems	311.1
 Z21.22—99	Relief Valves for Hot Water Supply Systems				504.2, 504.5
 Z124.1—95	Plastic Bathtub Units						407.1
 Z124.2—95	Plastic Shower Receptors and Shower Stalls				417.1
 Z124.3—95	Plastic Lavatories							416.1, 416.2
 Z124.4—96	Plastic Water Closet Bowls and Tanks				420.1
 Z124.6—97	Plastic Sinks							415.1, 418.1

 Air-Conditioning & Refrigeration Institute
4100 North Fairfax Drive, Suite 200
Arlington, VA 22203
 ARI
 Standard									Referenced
reference									in code
number		Title								section number

 1010—94	Self-Contained, Mechanically-Refrigerated Drinking-Water Coolers	410.1

 American Society of Mechanical Engineers
Three Park Avenue
New York, NY 10016-5990
 ASME
 Standard									Referenced
Reference									in code
Number		Title								section number

 A112.1.2—1991(R1998)	Air Gaps in Plumbing Systems	Table 608.1
 A112.1.3—2000	Air Gap Fittings for Use with Plumbing Fixtures, Appliances and Appurtenances	608.13.1, Table 608.1
 A112.3.1—1993	Performance Standard and Installation Procedures for Stainless Steel Drainage Systems or Sanitary, Storm andChemical Applications, Above and Below Ground	412.1, Table 702.1, Table 702.2, Table 702.3,
 Table 702.4, 708.2, Table 1102.4, Table 1102.5, 1102.6, Table 1102.7
 A112.3.4—2000	Macerating Toilet Systems and Related Components	712.4.1
 A112.4.1—1993(R1998)	Water Heater Relief Valve Drain Tubes	504.6.2
 A112.4.3—1999	Plastic Fittings for Connecting Water Closets to the Sanitary Drainage System	405.4
 A112.6.1M—1997	Floor-Affixed Supports for Off-the-Floor Plumbing Fixtures for Public Use	405.4.3
 A112.6.2—2000	Framing-Affixed Supports for Off-the-Floor Water Closets with Concealed Tanks	405.4.3
 A112.6.3—2001	Floor and Trench Drains	412.1
 A112.6.7—2001	Enameled and Epoxy-coated Cast-iron and PVC plastic Sanitary Floor Sinks	427.1
 A112.14.1—1975(R1998)	Backwater Valves	715.2
 A112.14.3—2000	Grease Interceptors	1003.3.4
 A112.14.4—2001	Grease Removal Devices	1003.3.4
 A112.18.1—2000	Plumbing Fixture Fittings	424.1
 A112.18.3M—1996	Performance Requirements for Backflow Protection Devices and Systems in Plumbing Fixture Fittings	424.5
 A112.18.6—1999	Flexible Water Connectors	605.6
 A112.18.7—1999	Deck mounted Bath/Shower Transfer Valves with Integral Backflow Protection	424.6
 A112.19.1M—1994(R1999)	Enameled Cast Iron Plumbing Fixtures	407.1, 410.1, 415.1, 416.1, 418.1
 A112.19.2M—1998	Vitreous China Plumbing Fixtures	401.2, 405.9, 408.1, 410.1, 416.1, 418.1, 419.1, 420.1
ASME—continued
 
 A112.19.3M—1987(R1996)	Stainless Steel Plumbing Fixtures (Designed for Residential Use)	405.9, 415.1, 416.1, 418.1
 A112.19.4M—1994(R1999)	Porcelain Enameled Formed Steel Plumbing Fixtures	407.1, 416.1, 418.1
 A112.19.5—1999	Trim for Water-Closet Bowls, Tanks, and Urinals	425.4
 A112.19.6—1995	Hydraulic Performance Requirements for Water Closets and Urinals	419.1, 420.1
 A112.19.7M—1995	Whirlpool Bathtub Appliances	421.1
 A112.19.8M—1987(R1996)	Suction Fittings for Use in Swimming Pools, Wading Pools, Spas, Hot Tubs, and Whirlpool Bathtub Appliances	421.4
 A112.19.9M—1998	Non-Vitreous Ceramic Plumbing Fixtures	407.1, 408.1, 410.1, 415.1, 416.1, 417.1, 418.1, 420.1
 A112.19.12—2000	Wall Mounted and Pedestal Mounted, Adjustable and Pivoting Lavatory and Sink Carrier Systems	416.4, 418.3
 A112.19.13—2001	Electrohydraulic Water Closets	420.1
 A112.19.15—2001	Bathtub/Whirlpool Bathtubs with Pressure Sealed Doors	407.4, 421.5
 A112.21.2M—1983	Roof Drains	1102.6
 A112.36.2M—1991(R1998)	Cleanouts	708.2
 B1.20.1—1983(R1999)	Pipe Threads, General Purpose (inch)	605.10.3, 605.12.3, 605.14.4, 605.16.3, 605.18.1,
 705, 705.2.3, 705.4.3
 B16.3—1999	Malleable Iron Threaded Fittings Classes 150 and 300	Table 605.5, Table 702.4, Table 1102.7
 B16.4—1998	Gray Iron Threaded Fittings Classes 125 and 250	Table 605.5, Table 702.4, Table 1102.7
 B16.9—1993	Factory-Made Wrought Steel Buttwelding Fittings	Table 605.5, Table 702.4, Table 1102.7
 B16.11—1996	Forged Fittings, Socket-Welding and Threaded	Table 605.5, Table 702.4, Table 1102.7
 B16.12—1998	Cast-Iron Threaded Drainage Fittings	Table 605.5, Table 702.4, Table 1102.7
 B16.15—1985(R1994)	Cast Bronze Threaded Fittings	Table 605.5, Table 702.4, Table 1102.7
 B16.18—1984(R1994)	Cast Copper Alloy Solder Joint Pressure Fittings	Table 605.5, Table 702.4, Table 1102.7
 B16.22—1995	Wrought Copper and Copper Alloy Solder Joint Pressure Fittings	Table 605.5, Table 702.4, Table 1102.7
 B16.23—1992	Cast Copper Alloy Solder Joint Drainage Fittings DWV	Table 605.5, Table 702.4, Table 1102.7
 B16.26—1988	Cast Copper Alloy Fittings for Flared Copper Tubes	Table 605.5, Table 702.4, Table 1102.7
 B16.28—1994	Wrought Steel Buttwelding Short Radius Elbows and Returns	Table 605.5, Table 702.4, Table 1102.7
 B16.29—1994	Wrought Copper and Wrought Copper Alloy Solder Joint Drainage Fittings—DWV	Table 605.5, Table 702.4, Table 1102.7

 
 American Society of Sanitary Engineering
901 Canterbury Road, Suite A
Westlake, OH 44145
 ASSE
 Standard		Referenced
Reference		in code
Number	Title	section number
 1001—90	Performance Requirements for Pipe Applied Atmospheric Type Vacuum Breakers	425.2, Table 608.1, 608.13.6
 1002—99	Performance Requirements for Water Closet Flush Tank Ball Cocks	425.3.1, Table 608.1
 1003—95	Performance Requirements for Water Pressure Reducing Valves	604.8
 1004—90	Performance Requirements for Commercial Dishwashing Machines	409.1
 1005—99	Performance Requirements for Water Heater Drain Valves	501.3
 1006—89	Performance Requirements for Residential Use (Household) Dishwashers	409.1
 1007—92	Performance Requirements for Home Laundry Equipment	406.1, 406.2
 1008—89	Performance Requirements for Household Food Waste Disposer Units	413.1
 1009—90	Performance Requirements for Commercial Food Waste Grinder Units	413.1
 1010—98	Performance Requirements for Water Hammer Arresters	604.9
 1011—95	Performance Requirements for Hose Connection Vacuum Breakers	Table 608.1, 608.13.6
1012—95	Performance Requirements for Backflow Preventers with
   Intermediate Atmospheric Vent	Table 608.1, 608.13.3, 608.16.2
1013—99	Performance Requirements for Reduced Pressure Principle Backflow Preventers and Reduced Pressure Fire Protection Principle Backflow Preventers Table 608.1, 608.13.2, 608.16.2
1014—90	Performance Requirements for Handheld Showers	424.2
1015—99	Performance Requirements for Double Check Backflow Prevention Assemblies And Double Check Fire Protection Backflow Prevention Assemblies	Table 608.1, 608.13.7
 1016—96	Performance Requirements for Individual Thermostatic, Pressure Balancing and Combination Control Valves for Bathing Facilities	424.3
 
ASSE—continued
 
 1017—99	Performance Requirements for Temperature Actuated Mixing Valves for Hot Water Distribution Systems	424.3, 424.5, 613.1
 1018—86	Performance Requirements for Trap Seal Primer Valves; Water Supply Fed	1002.4
 1019—97	Performance Requirements for Wall Hydrants, Freezeless, Automatic Draining,
	   Anti-Backflow Types	Table 608.1, 608.13.6
 1020—98	Performance Requirements for Pressure Vacuum Breaker Assembly	Table 608.1, 608.13.5
 1022—98	Performance Requirements for Backflow Preventer for Carbonated Beverage Machines	Table 608.1, 608.16.1
 1024—98	Performance Requirements for Dual Check Valve Type Backflow Preventers
	   (for Residential Supply Service or Individual Outlets)	605.3.1, Table 608.1
 1035—95	Performance Requirements for Laboratory Faucet Backflow Preventers	Table 608.1, 608.13.6
 1037—90	Performance Requirements for Pressurized Flushing Devices for Plumbing Fixtures	425.2
 1044—86	Performance Requirements for Trap Seal Primer Valves; Drainage Type	1002.4
 1047—99	Performance Requirements for Reduced Pressure Detector Fire Protection Backflow Prevention Assemblies	Table 608.1, 608.13.2
 1048—99	Performance Requirements for Double Check Detector Fire Protection Backflow   Prevention Assemblies	Table 608.1, 608.13.7
 1051—98	Performance Requirements for Air Admittance Valves for Plumbing Drainage Systems- Fixture and Branch Devices	917.1
 1052—94	Performance Requirements for Hose Connection Backflow Preventers	Table 608.1, 608.13.6
 1055—98	Performance Requirements for Backflow Devices for Chemical Dispensing Systems	608.13.9
 1056—95	Performance Requirements for Back Siphonage Vacuum Breaker	Table 608.1, 608.13.5, 608.13.8
 1060—96	Performance Requirements for Outdoor Enclosures for Backflow Prevention  Assemblies	608.14.1
 1062—97	Performance Requirements for Temperature Actuated, Flow Reduction Valves to Individual Fixture Fittings	424.5
 1066—97	Performance Requirements for Individual Pressure Balancing Valves for Individual Fixture Fittings	604.11
 5013—98	Performance Requirements for Testing Reduced Pressure Principle Backflow Preventers (RP) and Reduced Pressure Fire Protection Principle Backflow Preventers (RFP)	312.9.2
5015—98	Performance Requirements for Testing Double Check Backflow Prevention Assemblies (DC) and
	   Double Check Fire Protection Backflow Prevention Assemblies (DCF)	312.9.2
 5020—98	Performance Requirements for Testing Pressure Vacuum Breaker Assembly (PVBA)	312.9.2
 5047—98	Performance Requirements for Testing Reduced Pressure Detector Fire Protection Backflow Prevention Assemblies (RPDF)	312.9.2
 5048—98	Performance Requirements for Testing Double Check Detector Fire Protection
	   Backflow Prevention Assemblies (DCDF)	312.9.2
 5052—98	Performance Requirements for Testing Hose Connection Backflow Preventers	312.9.2
 5056—98	Performance Requirements for Testing Spill Resistant Vacuum Breaker	312.9.2

 ASTM International
100 Barr Harbor Drive
West Conshohocken, PA 19428-2959
 ASTM
 Standard		Referenced
Reference		in code
Number	Title	section number
 A 53/A 53M—0201	Specification for Pipe, Steel, Black and Hot-Dipped, Zinc-Coated Welded and Seamless	Table 605.3,
 Table 605.4, Table 702.1
 A 74—98	Specification for Cast Iron Soil Pipe and Fittings	Table 702.1, Table 702.2, Table 702.3, Table 702.4, 708.2, Table 1102.4, Table 1102.5, Table 1102.7
 A 312/A 312M—01	Specification for Seamless and Welded Austenitic Stainless Steel Pipes	Table 605.4, Table 605.5, Table 605.6, 605.23.2
 A 733—01	Specification for Welded and Seamless Carbon Steel and Austenitic Stainless Steel Pipe Nipples	Table 605.8
 A 778—01	Specification for Welded Unannealed Austenitic Stainless Steel Tubular Products	Table 605.4, Table 605.5, Table 605.6
 A 888—98e1	Specification for Hubless Cast Iron Soil Pipe and Fittings for Sanitary and Storm Drain, Waste, and Vent Piping Application	Table 702.1, Table 702.2, Table 702.3,  Table 702.4, Table 1102.4, Table 1102.5, Table 1102.7
 B 32—00e1	Specification for Solder Metal	605.14.3, 605.15.4, 705.9.3, 705.10.3
 B 42—98	Specification for Seamless Copper Pipe, Standard Sizes	Table 605.3, Table 605.4, Table 702.1
ASTM—continued
 
 B 43—98	Specification for Seamless Red Brass Pipe, Standard Sizes	Table 605.3, Table 605.4, Table 702.1
 B 75—02 99	Specification for Seamless Copper Tube	Table 605.3, Table 605.4, Table 702.1, Table 702.2, Table 702.3, Table 1102.4
 B 88—02 99el	Specification for Seamless Copper Water Tube	Table 605.3, Table 605.4, Table 702.1, Table 702.2, Table 702.3, Table 1102.4
 B 152/B 152M—00	Specification for Copper Sheet, Strip Plate and Rolled Bar	402.3, 425.3.3, 417.5.2.4, 902.2
 B 251—02 97	Specification for General Requirements for Wrought Seamless Copper and Copper-Alloy Tube	Table 605.3,Table 605.4,
 Table 702.1, Table 702.2, Table 702.3, Table 1102.4
 B 302—02 00	Specification for Threadless Copper Pipe, Standard Sizes	Table 605.3, Table 605.4, Table 702.1
 B 306—99	Specification for Copper Drainage Tube (DWV)	Table 702.1, Table 702.2, Table 1102.4
 B 447—00	Specification for Welded Copper Tube	Table 605.3, Table 605.4
 B 687—99	Specification for Brass, Copper, and Chromium-Plated Pipe Nipples	Table 605.8
 B 813—00e01	Specification for Liquid and Paste Fluxes for Soldering of Copper and
	Copper Alloy Tube	605.14.3, 605.15.4, 705.9.3, 705.10.3
 B 828—00	Practice for Making Capillary Joints by Soldering of Copper and Copper Alloy Tube and Fittings	605.14.3,
 605.15.4, 705.9.3, 705.10.3
 C 4—00	Specification for Clay Drain Tile and Perforated Clay Drain Tile	Table 702.3, Table 1102.4, Table 1102.5
 C 14—99	Specification for Concrete Sewer, Storm Drain, and Culvert Pipe	Table 702.3, Table 1102.4
 C 76—00	Specification for Reinforced Concrete Culvert, Storm Drain, and Sewer Pipe	Table 702.3, Table 1102.4
 C 296—00	Specification for Asbestos-Cement Pressure Pipe	Table 605.4
 C 425—01	Specification for Compression Joints for Vitrified Clay Pipe and Fittings	705.15, 705.16
 C 428—97	Specification for Asbestos-Cement Nonpressure Sewer Pipe	Table 702.2, Table 702.3, Table 1102.4
 C 443—01	Specification for Joints for Concrete Pipe and Manholes, Using Rubber Gaskets	705.6, 705.16
 C 508—00	Specification for Asbestos-Cement Underdrain Pipe	Table 1102.5
 C 564—97	Specification for Rubber Gaskets for Cast Iron Soil Pipe and Fittings	705.5.2, 705.5.3, 705.16
 C 700—00	Specification for Vitrified Clay Pipe, Extra Strength, Standard Strength, and Perforated	Table 702.3, Table 1102.4, Table 1102.5
 C 1053—00	Specification for Borosilicate Glass Pipe and Fittings for Drain, Waste, and
	Vent (DWV) Applications	Table 702.1, Table 702.4
 C 1173—97	Specification for Flexible Transition Couplings for Underground Piping System	705.7.1, 705.14.1, 705.16
 C 1277—97	Specification for Shielded Coupling Joining Hubless Cast Iron Soil Pipe and Fittings	705.5.3
 C 1440—99	Specification for Thermoplastic Elastomeric (TPE) Gasket Materials for Drain, Waste,  and Vent (DWV), Sewer, Sanitary and Storm Plumbing Systems	705.16
 C 1460—00	Specification for Shielded Transition Couplings for Use with Dissimilar DWV Pipe  and Fittings Above Ground	705.16
 C 1461—00	Specification for Mechanical Couplings Using Thermoplastic Elastomeric (TPE) Gaskets for Joining Drain, Waste, and Vent (DWV) Sewer, Sanitary and Storm Plumbing Systems for Above and Below Ground Use	705.16
 D 1527—99	Specification for Acrylonitrile-Butadiene-Styrene (ABS) Plastic Pipe, Schedules 40 and 80	Table 605.3
 D 1785—99	Specification for Poly (Vinyl Chloride) (PVC) Plastic Pipe, Schedules 40, 80 and 120	Table 605.3
 D 1869—95(2000)	Specification for Rubber Rings for Asbestos-Cement Pipe	605.11, 605.22, 705.3, 705.16
 
 D 2235—01	Specification for Solvent Cement for Acrylonitrile-Butadiene-Styrene (ABS) Plastic Pipe and Fittings	605.10.2, 705.2.2, 705.7.2
 D 2239—01	Specification for Polyethylene (PE) Plastic Pipe (SIDR-PR) Based on Controlled Inside Diameter	Table 605.3
 D 2241—00	Specification for Poly (Vinyl Chloride) (PVC) Pressure-Rated Pipe (SDR-Series)	Table 605.3
 D 2282—99	Specification for Acrylonitrile-Butadiene-Styrene (ABS) Plastic Pipe (SDR-PR)	Table 605.3
 D 2464—99	Specification for Threaded Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 80	Table 605.5, Table 1102.7
 D 2466—02 01	Specification for Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 40	Table 605.5, Table 1102.7
 D 2467—01 99	Specification for Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 80	Table 605.5, Table 1102.7
 D 2468—96a	Specification for Acrylonitrile-Butadiene-Styrene (ABS) Plastic Pipe Fittings, Schedule 40	Table 605.5, Table 1102.7
 D 2564—02 96a	Specification for Solvent Cements for Poly (Vinyl Chloride) (PVC) Plastic Piping Systems	605.21.2, 705.8.2, 705.14.2
 D 2609—00	Specification for Plastic Insert Fittings for Polyethylene (PE) Plastic Pipe	Table 605.5, Table 1102.7
 D 2657—97	Standard Practice for Heat Fusion-Joining of Polyolefin Pipe and Fitting	605.19.2, 605.20.2
 D 2661—01	Specification for Acrylonitrile-Butadiene-Styrene (ABS) Schedule
	40 Plastic Drain, Waste, and Vent Pipe and Fittings	Table 702.1, Table 702.2, Table 702.3, Table 702.4, 705.2.2, 705.7.2, Table 1102.4, Table 1102.7

ASTM—continued
 
 D 2662—96a	Specification for Polybutylene (PB) Plastic Pipe (SDR-PR) Based on Controlled Inside Diameter	Table 605.3
 D 2665—01	Specification for Poly (Vinyl Chloride) (PVC) Plastic Drain, Waste, and Vent Pipe and Fittings	Table 702.1,
 Table 702.2, Table 702.3, Table 702.4, Table 1102.4, Table 1102.7
 D 2666—96a	Specification for Polybutylene (PB) Plastic Tubing	Table 605.3
 D 2672—96a	Specification for Joints for IPS PVC Pipe Using Solvent Cement	Table 605.3
 D 2729—96a	Specification for Poly (Vinyl Chloride) (PVC) Sewer Pipe and Fittings	Table 1102.5
 D 2737—01	Specification for Polyethylene (PE) Plastic Tubing	Table 605.3
 D 2751—96a	Specification for Acrylonitrile-Butadiene-Styrene (ABS) Sewer Pipe and Fittings	Table 702.3, Table 1102.4
 D 2846/D 2846M—99	Specification for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Hot and Cold Water  Distribution Systems	Table 605.3, Table 605.4, 605.16.2
 D 2855—96	Standard Practice for Making Solvent-Cemented Joints with Poly (Vinyl Chloride) (PVC) Pipe and  Fittings	605.21.2, 705.8.2, 705.14.2
 D 2949—00a	Specification for 3.25-In Outside Diameter Poly (Vinyl Chloride) (PVC)
	   Plastic Drain, Waste, and Vent Pipe and Fittings	Table 702.1, Table 702.2, Table 702.3
 D 3034—00	Specification for Type PSM Poly (Vinyl Chloride) (PVC) Sewer Pipe and Fittings	Table 702.3,
 Table 702.4, Table 1102.4
 D 3139—98	Specification for Joints for Plastic Pressure Pipes Using Flexible Elastomeric Seals	605.10.1, 605.21.1
 D 3212—96a	Specification for Joints for Drain and Sewer Plastic Pipes Using Flexible Elastomeric Seals	705.2.1,
 705.7.1, 705.8.1, 705.14.1
 D 3309—96a (2002)	Specification for Polybutylene (PB) Plastic Hot and Cold Water Distribution Systems	Table 605.3, Table 605.4,
 605.19.2, 605.19.3
 D 3311—94	Specification for Drain, Waste and Vent (DWV) Plastic Fittings Patterns	Table 702.4
 D 4068—01	Specification for Chlorinated Polyethlene (CPE) Sheeting for Concealed Water-  Containment Membrane	417.5.2.2
 D 4551—96(2001)	Specification for Poly (Vinyl Chloride) (PVC) Plastic Flexible Concealed Water-Containment Membrane	417.5.2.1
 F 405—97	Specification for Corrugated Polyethylene (PE) Tubing and Fittings	Table 1102.5
 F 409—99a	Specification for Thermoplastic Accessible and Replaceable Plastic Tube and
	   Tubular Fittings	424.1.2, Table 1102.7
 F 437—99	Specification for Threaded Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings, Schedule 80	Table 605.5, Table 1102.7
 F 438—02 01	Specification for Socket-Type Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings,  Schedule 40	Table 605.5, Table 1102.7
 F 439—02 01	Specification for Socket-Type Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings,  Schedule 80	Table 605.5, Table 1102.7
 F 441/F 441M—02 99	Specification for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe, Schedules 40 and 80	Table 605.3, Table 605.4, Table 605.5
 F 442/F 442M—99	Specification for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe (SDR-PR)	Table 605.3, Table 605.4, Table 605.5
 F 477—99	Specification for Elastomeric Seals (Gaskets) for Joining Plastic Pipe	605.22, 705.16
 F 493—97	Specification for Solvent Cements for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe and Fittings	605.16.2
 F 628—01	Specification for Acrylonitrile-Butadiene-Styrene (ABS) Schedule 40 Plastic Drain, Waste, and Vent Pipe with a Cellular Core	Table 702.1, Table 702.2, Table 702.3, Table 702.4, 705.2.2, 705.7.2, Table 1102.4
 F 656—96a	Specification for Primers for Use in Solvent Cement Joints of Poly (Vinyl Chloride) (PVC) Plastic Pipe and  Fittings	605.21.2, 705.8.2, 705.14.2
 F 714—00	Specification for Polyethylene (PE) Plastic Pipe (SDR-PR) Based on Outside Diameter	Table 702.3
 F 876—02 00	Specification for Cross-linked Polyethylene (PEX) Tubing	Table 605.3
 F 877—02a 00	Specification for Cross-linked Polyethylene (PEX) Plastic Hot and Cold Water
	   Distribution Systems	Table 605.3, Table 605.4
 F 891—00	Specification for Coextruded Poly (Vinyl Chloride) (PVC) Plastic Pipe with a Cellular Core	Table 702.1, Table 702.2, Table 702.3, Table 702.4, Table 1102.4, Table 1102.5
 F 1281—02e e01	Specification for Cross-Linked Polyethylene/Aluminum/Cross-Linked Polyethylene (PEX-AL-PEX)  Pressure Pipe	Table 605.3, Table 605.4
 F 1282—01a	Specification for Polyethylene/Aluminum/Polyethylene (PE-AL-PE) Composite Pressure Pipe	Table 605.3, Table 605.4
 F 1488—00	Specification for Coextruded Composite Pipe	Table 702.1, Table 702.2, Table 702.3
 F 1807—99	Specification for Metal Insert Fittings Utilizing a Copper Crimp Ring for  SDR9 Cross-linked Polyethylene (PEX) Tubing	Table 605.5, 605.17.2
 F 1866—98	Specification for Poly (Vinyl Chloride) (PVC) Plastic Schedule 40 Drainage and DWV Fabricated Fittings	Table 702.4
ASTM—continued
 
 F 1960—99	Specification for Cold Expansion Fittings with PEX Reinforcing Rings for use with  Cross-linked Polyethylene (PEX) Tubing	Table 605.5
 F 1974—02 00	Specification for Metal Insert Fittings for Polyethylene/Aluminum/ Polyethylene and Cross-linked  Polyethylene/Aluminum/Cross-linked Polyethylene Composite Pressure Pipe	Table 605.5
 F 2080—01	Specifications for Cold-Expansion Fittings with Metal Compression-Sleeves for Cross-linked Polyethylene (PEX) Pipe	Table 605.5
 
 American Welding Society
550 N.W. LeJeune Road
Miami, FL 33126
 AWS
 Standard		Referenced
Reference		in code
Number	Title	section number
 A5.8—92	Specifications for Filler Metals for Brazing and Braze Welding	605.12.1, 605.14.1, 605.15.1, 705.4.1, 705.9.1, 705.10.1

 American Water Works Association
6666 West Quincy Avenue
Denver, CO 80235
 AWWA
 Standard		Referenced
Reference		in code
Number	Title	section number
 C104—95	Standard for Cement-Mortar Lining for Ductile-Iron  Pipe and Fittings for Water	605.3, 605.5
 C110—98	Standard for Ductile-Iron and Gray-Iron Fittings, 3 Inches through 48 Inches,  for Water 	Table 605.5, Table 702.4, Table 1102.7
 C111—00	Standard for Rubber-Gasket Joints for Ductile-Iron
	   Pressure Pipe and Fittings	605.13
 C115—99	Standard for Flanged Ductile-Iron Pipe with Ductile-Iron or Gray-Iron
 	   Threaded Flanges	Table 605.3
 C151—96	Standard for Ductile-Iron Pipe, Centrifugally Cast for Water	Table 605.3
 C153—00	Standard for Ductile-Iron Compact Fittings for Water Service	Table 605.5
 C510—00	Double Check Valve Backflow Prevention Assembly	Table 608.1, 608.13.7
 C511—00	Reduced-Pressure Principle Backflow Prevention Assembly	Table 608.1, 608.13.2, 608.16.2
 C651—99	Disinfecting Water Mains	610.1
 C652—92	Disinfection of Water-Storage Facilities	610.1
 Cast Iron Soil Pipe Institute
5959 Shallowford Road, Suite 419
Chattanooga, TN 37421
 CISPI
 Standard		Referenced
Reference		in code
Number	Title	section number
 301—00	Specification for Hubless Cast Iron Soil Pipe and Fittings for Sanitary and Storm Drain, Waste and Vent Piping Applications	Table 702.1, Table 702.2, Table 702.3, Table 702.4, Table 1102.4, Table 1102.5, Table 1102.7
 310—97	Specification for Coupling for Use in Connection with Hubless Cast Iron Soil Pipe and Fittings   for Sanitary and Storm Drain, Waste and Vent Piping Applications	705.5.3
 Canadian Standards Association
178 Rexdale Blvd.
Rexdale (Toronto), Ontario, Canada M9W 1R3
 CSA
 Standard		Referenced
Reference		in code
Number	Title	section number
 B45.1—99	Ceramic Plumbing Fixtures	408.1, 416.1, 418.1, 419.1, 420.1
 B45.2—99	Enameled Cast-Iron Plumbing Fixtures	407.1, 415.1, 416.1, 418.1
 B45.3—99	Porcelain Enameled Steel Plumbing Fixtures	407.1, 416.1, 418.1
CSA—continued
 
 B45.4—99	Stainless-Steel Plumbing Fixtures	415.1, 416.1, 418.1, 420.1
 B45.5—99	Plastic Plumbing Fixtures	407.1, 416.2, 417.1, 419.1, 420.1, 421.1
 B45.9—99	Macerating Systems and Related Components	712.4.1
 B45.10—01	Hydromassage Bathtubs	421.1
 B64.7—94	Vacuum Breakers, Laboratory Faucet Type (LFVB)	Table 608.1, 608.13.6
 B79—94(2000)	Floor, Area and Shower Drains, and Cleanouts for Residential Construction	412.1
 B125—98	Plumbing Fittings	424.1, 424.3, 424.4, 425.3.1, 425.4, Table 608.1
 B137.1—99	Polyethylene Pipe, Tubing and Fittings for Cold Water Pressure Services	Table 605.3
 B137.2—99	PVC Injection-Moulded Gasketed Fittings for Pressure Applications	Table 605.5, Table 1102.7
 B137.3—99	Rigid Poly (Vinyl Chloride) (PVC) Pipe for Pressure Applications	Table 605.3, 605.21.2, 705.8.2, 705.14.2
 B137.5—99	Cross-Linked Polyethylene (PEX) Tubing Systems for Pressure Applications—with Revisions through September 1992	Table 605.3, Table 605.4
 B137.6—99	CPVC Pipe, Tubing and Fittings for Hot and Cold Water Distribution Systems—with Revisions through May 1986	Table 605.3, Table 605.4
 B181.1—99	ABS Drain, Waste, and Vent Pipe and Pipe Fittings	Table 702.1, Table 702.2, Table 702.4, 705.2.2, 705.7.2, 715.2
 B181.2—99	PVC Drain, Waste, and Vent Pipe and Pipe Fittings—with Revisions through
	December 1993	Table 702.1, Table 702.2, 705.8.2, 705.14.2, 715.2
 B182.1—99	Plastic Drain and Sewer Pipe and Pipe Fittings	705.8.2, 705.14.2
 B182.2—99	PVC Sewer Pipe and Fittings (PSM Type)	Table 702.3, Table 1102.4, Table 1102.5
 CAN3-B137.8M—99	Polybutylene (PB) Piping for Pressure Applications—with Revisions through July 1992	Table 605.3, Table 605.4, 605.19.2, 605.19.3
 CAN/CSA-A257.1M—92	Circular Concrete Culvert, Storm Drain, Sewer Pipe and Fittings	Table 702.3, Table 1102.4
 CAN/CSA-A257.2M—92	Reinforced Circular Concrete Culvert, Storm Drain, Sewer Pipe and Fittings	Table 702.3, Table 1102.4
 CAN/CSA-A257.3M—92	Joints for Circular Concrete Sewer and Culvert Pipe, Manhole Sections, and Fittings Using Rubber Gaskets	705.6, 705.16
 CAN/CSA-B64.1.1—01	Vacuum Breakers, Atmospheric Type (AVB)	425.2, Table 608.1, 608.13.6
 CAN/CSA-B64.2—01	Vacuum Breakers, Hose Connection Type (HCVB)	Table 608.1, 608.13.6
 CAN/CSA-B64.2.2—01	Vacuum Breakers, Hose Connection Type (HCVB) with Automatic Draining Feature	Table 608.1, 608.13.6
 CAN/CSA-B64.3—01	Backflow Preventers, Dual Check Valve Type with Atmospheric Port (DCAP)	Table 608.1, 608.13.3, 608.16.2
 CAN/CSA-B64.4—01	Backflow Preventers, Reduced Pressure Principle Type (RP)	Table 608.1, 608.13.2, 608.16.2
 CAN/CSA-B64.10—01	Manual for the Selection, Installation, Maintenance and Field Testing of Backflow Prevention Devices	312.9.2
 CAN/CSA-B137.9—99	Polyethylene/Aluminum/Polyethylene Composite Pressure Pipe Systems	Table 605.3
 CAN/CSA-B137.10M—99	Cross-linked Polyethylene/Aluminum/Polyethylene Composite Pressure Pipe Systems	Table 605.3, Table 605.4
 CAN/CSA-B181.3—99	Polyolefin Laboratory Drainage Systems	Table 702.1, Table 702.2
 CAN/CSA-B182.4—99	Profile PVC Sewer Pipe and Fittings	Table 702.3, Table 1102.4, Table 1102.5
 CAN/CSA-B602—99	Mechanical Couplings for Drain, Waste, and Vent Pipe and Sewer Pipe	705.2.1, 705.5.3, 705.6, 705.7.1, 705.14.1, 705.15, 705.16

 Federal Specification
1941 Jefferson Davis Highway, Suite 104
Arlington, VA 22202
 FS
 Standard		Referenced
Reference		in code
Number	Title	section number
 TT-P-1536A(1975)	Federal Specification for Plumbing Fixture Setting Compound	405.4
 * Standards are available from the Supt. of Documents, U.S. Government Printing Office, Washington, DC 20402-9325.

 International Code Council
5203 Leesburg Pike, Suite 600Falls Church, VA 22041
 ICC
Florida CODES
 Standard		Referenced
Reference		in code
Number	Title	section number
FBC-B 04 IBC—03	Florida International Building Code, Building®	201.3, 305.4, 307.1, 307.2, 307.3, 308.2, 309.1, 310.1, 310.3, 403.1, Table 403.1, 404.1, 407.3, 417.6, 502.6, 606.5.2, 1106.5
ICC—continued
Ch.27, FBC-B 04 ICC EC—03	Florida Building Code, Building (National Electrical Code) ICC Electrical CodeÔ	201.3, 502.1, 504.3, 1113.1.3
 IEBC—03	International Existing Building CodeÒ	101.2
Ch.13 FBC-B 04 IECC—03	Ch. 13 of the Florida Building Code, Building (Energy Efficiency) International Energy Conservation CodeÒ	313.1, 607.2, 607.2.1
FFPC-04 IFC—03	Florida International Fire Prevention Code®	201.3, 1201.1
FBC-FG 04 IFGC—03	Florida Building Code, International Fuel Gas Code®	101.2, 201.3, 502.1
FBC-M 04 IMC—03	Florida Building Code, International Mechanical Code®	201.3, 307.6, 310.1, 422.9, 502.1, 612.1, 1202.1
64E-6 IPSDC—03	Rule 64E, Florida Administrative Code  International Private Sewage Disposal Code®	701.2
FRC 04 IRC—03 Florida International Residential CodeÒ	101.2

 Industry Safety Equipment Association
1901 N. Moore Street, Suite 808
Arlington, VA 22209
 ISEA
 Standard		Referenced
Reference		in code
Number	Title	section number
 Z358.1—98	Emergency eyewash and shower equipment	411.1
 
 National Fire Protection Association
Batterymarch Park
Quincy, MA 02269
 NFPA
 Standard		Referenced
Reference		in code
Number	Title	section number
 50—01	Bulk Oxygen Systems at Consumer Sites	1203.1
 51—02 97	Design and Installation of Oxygen-Fuel Gas Systems for Welding, Cutting, and Allied Processes	1203.1
 70—02 99	National Electrical Code	502.1, 504.3, 1113.1.3
 99C—99	Gas and Vacuum Systems	1202.1

 National Sanitation Foundation
789 Dixboro Road
Ann Arbor, MI 48105
 NSF
 Standard		ReferencedReference		in code
Number	Title	section number
 3—1996	Commercial Spray-Type Dishwashing and Glasswashing  Machines	409.1
14—1999	Plastic Piping System Components and Related Materials	303.3, 611.3
 18—1996a	Manual Food and Beverage Dispensing Equipment	426.1
42—20010	Drinking Water Treatment Units—Aesthetic Effects	611.1, 611.3
 44—2000	Residential Cation Exchange Water Softeners	611.1, 611.3
 53—2001	Drinking Water Treatment Units—Health Effects	611.1, 611.3
 58—2001	Reverse Osmosis Drinking Water Treatment Systems	611.2
 61—2001	Drinking Water System Components—Health Effects	424.1, 605.3, 605.4, 605.5, 611.3
62—1999	Drinking Water Distillation Systems	611.1
 Plumbing and Drainage Institute
45 Bristol Drive, Suite 101
South Easton, MA 02375
 PDI
 Standard		Referenced
Reference		in code
Number	Title	section number
 G101(1998)	Testing and Rating Procedure for Grease Interceptors with Appendix of Sizing and Installation Data	1003.3.4