|  |
| --- |
| **STRUCTURAL**TAC ACTION VOTES Local Technical Amendments to the2020 7th Edition Florida Building Code |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with****TECHNICAL AMENDMENT** | **SUMMARY OF TECHNICAL AMENDMENT** | **TAC ACTION** |
|  |  |  |  |
| City of Winter Park | FBC – BuildingSec 1609.3 | Section 1609.3 – amendment to give guidance to designers and to provide uniformity with neighboring jurisdictions. This is not a local technical amendment or change in the FBC wind load criteria. | VOTE: |
|  |  |  |  |
| City of Winter Garden | Sec. 18-63 | Local amendment to require that exterior and interior load bearing walls of the first floor (or story) of all structures intended for human habitation or public access must be constructed using masonry block, concrete, or metal, except that this requirement does not apply to single family structures, duplex, triplex, quad-plex, or other residential structures having four (4) or fewer structures. | VOTE: |
|  |  |  |  |
| City of Longwood | FBC – BuildingSec. 1808.4.1 | Sec 1808.4.1 – local amendment to provide for limitation criteria for vibratory compaction.  | VOTE: |
|  |  |  |  |