|  |  |  |  |
| --- | --- | --- | --- |
| **SWIMMING POOL**  TAC ACTION VOTES  Local Technical Amendments to the  2020 7th Edition Florida Building Code | | | |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with**  **TECHNICAL AMENDMENT** | **SUMMARY OF TECHNICAL AMENDMENT** | **TAC ACTION** |
|  |  |  |  |
| County of Broward | FBC – Building  Ch. 4  Sec 454.1.4.1  and  Sec 454.2.16  FBC-Residential  Sec R4501.16 | Section 454.1.4.1 – Local amendment to require all swimming pool lighting fixtures to be low voltage (15 Volts or less) RMS for sinusoidal alternating current.  Section 454.2.16/R4501.16 – Local amendment to require all swimming pool lighting fixtures to be low voltage (15 Volts or less) RMS for sinusoidal alternating current. | VOTE: |
|  |  |  |  |
| County of  Miami-Dade | FBC – Building  Ch. 4  Sec 454.1.4.1  Sec 454.1.10.4.1  and  Sec 454.2.16  FBC – Residential  Sec R4501.16 | Local amendments to require low voltage lighting in newly built private swimming or recreational bathing pools that have underwater lighting installed, and in existing private pools with underwater lighting when permitted construction work is done after the initial construction. | VOTE: |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |