|  |
| --- |
| **SWIMMING POOL**TAC ACTION VOTES Local Technical Amendments to the2020 7th Edition Florida Building Code |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with****TECHNICAL AMENDMENT** | **SUMMARY OF TECHNICAL AMENDMENT** | **TAC ACTION** |
|  |  |  |  |
| County of Broward | FBC – BuildingCh. 4Sec 454.1.4.1andSec 454.2.16FBC-ResidentialSec R4501.16 | Section 454.1.4.1 – Local amendment to require all swimming pool lighting fixtures to be low voltage (15 Volts or less) RMS for sinusoidal alternating current.Section 454.2.16/R4501.16 – Local amendment to require all swimming pool lighting fixtures to be low voltage (15 Volts or less) RMS for sinusoidal alternating current. | **Batts to Deny 2nd Guerasio** **VOTE: 8 yes – 1 No****Passes****Commission Action to Deny Vote: 13-0** |
|  |  |  |  |
| County of Miami-Dade | FBC – BuildingCh. 4Sec 454.1.4.1Sec 454.1.10.4.1andSec 454.2.16FBC – Residential Sec R4501.16 | Local amendments to require low voltage lighting in newly built private swimming or recreational bathing pools that have underwater lighting installed, and in existing private pools with underwater lighting when permitted construction work is done after the initial construction. | **Batts to Deny 2nd Guerasio** **VOTE: 7 Yes – 2 No****Passes****Commission Action to Deny Vote: 13-0** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |