**From:** Jim LePetrie [mailto:jel@wetengineering.net]   
**Sent:** Tuesday, November 22, 2022 10:40 AM  
**To:** Sellers, Chip <Chip.Sellers@myfloridalicense.com>  
**Cc:** Madani, Mo <Mo.Madani@myfloridalicense.com>  
**Subject:** Swimming Pools - Alternate code language

|  |
| --- |
| **[NOTICE] This message comes from a system outside of DBPR. Please exercise caution when clicking on links and/or providing sensitive information. If you have concerns, please contact your Knowledge Champion or the DBPR Helpdesk.** |

Good morning:

I am following up on some alternate code language that I need to submit based on discussions from the TAC meeting held in October.  This adds language per Bob Vincent’s concern regarding depth at a sun shelf that transitions to steps.

We also discussed additional language for SW9942 regarding pool furniture, but I think there was a lot of opposition to this one and I think this one may need to go back to the drawing board.

Please let me know if the attached is acceptable or if I need to submit it in a different manner.  Thanks as always for your help.

Thanks,

Jim LePetrie, Jr., P.E.

SW10190

3.A sun shelf may be installed in pool areas with no more than 4 feet (1219 mm) of water depth, or less, except where the entire sun shelf transitions to steps, where the depth at the bottom of the steps can exceed 4 feet (1219 mm). Where the depth at the bottom of the steps exceeds 5 feet (1524 mm), depth and no dive markers shall be installed along the sun shelf edge in accordance with 454.1.2.8.2.