SUBCHAPTER 13-3
REFERENCED STANDARDS AND ORGANIZATIONS

SECTION 13-301
REFERENCED STANDARDS

[Change Section 13-301.0 as follows:]

13-301.0 General.  The standards (Std), and portions thereof, which are referred to in various parts of this code shall be part of Chapter 13 of the Florida Building Code and are hereby declared to be a part of this code. Section numbers shall read as if prefaced by 13-.

AABC	Associated Air Balance Council, 
1518 K Street, Suite 503, 
Washington, DC 20005		
Standard reference number	Title				Referenced in Code Section Number	
AABC, 1989		Associated Air Balance Council National Standard		410. 1.ABC.4.3	

AAMA	American Architectural Manufacturers Association
1827 Walden Office Square, Suite 104
Schaumburg, IL 60173-4268		
Standard reference number	Title				Referenced in Code Section Number	
AAMA/WDMA/CSANWWDA	Voluntary Specifications for Aluminum, Vinyl (PVC) 
101/I.S. 2-05 97			and Wood Windows and Glass Doors	406. 1.ABC.1.1, 606.ABC.1.1	

ACCA	Air Conditioning Contractors of America
2800 Shirlington Road, Suite 300
Arlington, VA 22206		
Standard reference number	Title				Referenced in Code Section Number	
ACCA Manual D-1995	Residential Duct Systems		410. 1.ABC.2, 610.ABC.1	
ACCA Manual J-2003	Residential Load Calculation, Eighth Edition with posted updates/errata.	 607.ABC.1	
ACCA Manual N-2005 1988	Commercial Load Calculation, Fourth Edition.		607. 1.ABC.1, B-3.1.1	

ADC	Air Diffusion Council
1000 E. Woodfield Rd., Suite 102 11 South LaSalle Street, Suite 1400
Schaumburg, IL 60173-5921Chicago, IL 60603.		
Standard reference number	Title				Referenced in Code Section Number	
ADC 2003 1996	Flexible Duct Performance & Installation 
Standards, Fourth Third Edition.					410. 1.ABC.2.2, 610. 1..ABC.2.2	

AHAM	Association of Home Appliance Manufacturers
20 North Wacker Dr.
Chicago, IL 60606		
Standard reference number	Title				Referenced in Code Section Number	
ANSI/AHAM RAC1-03	Room Air Conditioners.		Table 407. 1.ABC.3.2D, Table 607. 1.ABC.3.2D,	

AMCA	Air Movement and Control Association International
30 West University Drive
Arlington Heights, IL 60004-1806		
Standard reference number	Title	Referenced in Code Section Number	
AMCA 500-1989	Test Methods for Louvers, Dampers, and Shutters		409. 1.ABC.3.4,	

ANSI	American National Standards Institute, Inc.
25 West 43rd Street, Fourth Floor
New York, N.Y.10036.		
Standard reference number	Title				Referenced in Code Section Number	
ANSI A112.18.1M-1999	Finished and Rough Brass Plumbing Fixture Fittings		412. 1.ABC.2.5.1,608.2.A.3.5, 
										612. 1.ABC.2.4	
ANSI Z21.10.3-2004 2001	Gas Water Heater, Volume 3, Storage, with Input Ratings above
 75,000 Btu/h, Circulating and Instantaneous Water Heaters	Table 412. 1.ABC.3, 612. 1.ABC.3.1.2	
ANSI Z21.40.4-96
(with Addenda 1)	American National Standard for Performance Testing and Rating of Gas-Fired, 
Air-Conditioning and Heat Pump Appliances		607.2.A.1, C-5.1.1	
ANSI Z21.47a-04 2001	Gas-Fired Central Furnaces	Table 408. 1.ABC.3.2E, Table 608. 1.ABC.3.2E	
ANSI Z21.56-2006 2001	Gas-Fired Pool Heaters		412. 1.ABC.3.5, 612. 1.ABC.2.3.1	
ANSI Z21.66-1996 (R2001) 1994	Automatic Vent Damper Devices for Use with Gas-Fired Appliances	408. 1.ABC.3.2.1	
ANSI Z83.8/CGA 2.6 -2006 02	Gas Unit Heaters and Gas-Fired Duct Furnaces. CGA 2.6	Table 408. 1.ABC.3.2E, 
											Table 608. 1.ABC.3.2E	

ARDM	Association of Refrigerant Desuperheater Manufacturers, Inc, 
c/o Doucette Industries Trevor-Martin
4151 112 Terrace N
Clearwater, FL 33762		
Standard reference number	Title				Referenced in Code Section Number	
ARDM-88	Residential Heat Recovery Installation Guide, First Edition		600.3.ABC.3.2, 612. 1.B.3.2, 612.2.A.3.1	

ARI	Air-Conditioning and Refrigeration Institute
Suite 200
4100 North Fairfax Drive
Arlington, VA 22203		
Standard reference number	Title				Referenced in Code Section Number	
ARI Std. 210/240-2006 1994	Unitary Air-Conditioning and Air-Source Heat Pump Equipment	
Tables 407. 1.ABC.3.2A,B,
Tables 607. 1.ABC.3.2A,B, 607. 1.ABC.3.1, 608. 1.ABC.3.1	
ARI Std. 310/380-2004 1993	Packaged Terminal Air-Conditioners and Heat Pumps          Tables 407. 1.ABC.3.2D, 
											Tables 607. 1.BC.3.2D
ARI Std. 340/360-2004 2000	Commercial and Industrial Unitary Air-Conditioning and Heat Pump Equipment	
								Tables 407. 1.ABC.3.2A,B, Tables 607. 1.ABC.3.2A,B	
ARI Std. 365-20021994	Commercial and Industrial Unitary Air-Conditioning Condensing Units		
Tables 407. 1.ABC.3.2A, Tables 607.1.ABC.3.2A	
ARI Std. 390-2003 2001	Single Packaged Vertical Air Conditioners and Heat Pumps	Tables 410.ABC.3.2D, 610.ABC.3.2D
ARI Std. 460-2005 2000	Performance Rating of Remote Mechanical Draft Air-Cooled Refrigerant Condensers	
										Tables 407. 1.ABC.3.2G	
ARI Std. 550/590-2003 1998 Water Chilling Packages Using the Vapor Compression Cycle	
(with Addenda)							202, 407. 1.ABC.3.2, Tables 407. 1.ABC.3.2C
ARI Std. 560-2000	Absorption Water Chilling and Water Heating Packages	Tables 407. 1.ABC.3.2
ARI Std. 1160-2004	Performance Rating of Heat Pump Pool Heaters	Table 412.ABC.3, 612. 1.ABC.2.3.4

ASHRAE	American Society of Heating, Refrigerating and Air-Conditioning Engineers, Inc.
1791 Tullie Circle, NE
Atlanta, GA 30329-2305		
Standard reference number	Title				Referenced in Code Section Number	
ANSI/ASHRAE Std. 55-1992 	Thermal Environmental Conditions for Human Occupancy.	412.1.ABC.1, 
412. 1.ABC.1
ANSI/ASHRAE Std. 62.1-2004 01	Ventilation for Acceptable Indoor Air Quality.		407. 1.ABC.2.1.1, 
						407. 1.ABC.2.3, 409. 1.ABC.1.1, 409. 1.ABC.3.5, 609. 1.ABC.1	
ANSI/ASHRAE Std. 90.1-20041	Energy Efficient Design of New Buildings Except Low-Rise 
Residential Buildings.					413.0	
ANSI/ASHRAE Std. 93-1986 (RA91)	Methods of Testing to Determine the Thermal Performance 
of Solar Collectors				612. 1.ABC.3.4	
ANSI/ASHRAE 119-1988		Air Leakage Performance for Detached Single-Family
 (RA 94)				Residential Buildings					Table 13-613A.1-1
ANSI/ASHRAE 124-1991	Methods of Testing for Rating Combination Space-Heating and Water-
Heating Appliances 					608.2.A.3.5, 612.2.A.1	
ANSI/ASHRAE 137-1995 (RA2001)	Methods of Testing for Efficiency of Space-conditioning/Water-Heating 
			Appliances That Include a Desuperheater Water Heater		412. 1.ABC.1, 612.2.A.1
ANSI/ASHRAE 146-1998	Method of Testing for Rating Pool Heaters			Table 412. 1.ABC.3	
ANSI/ASHRAE 152-2004      	Method of Test for Determining the Design and Seasonal 	610.A.2
Efficiencies of Residential Thermal Distribution Systems	Table 13-613A.1-1
ASHRAE Handbook		Fundamentals, 20051					Table 13-613A.1-1
ASHRAE Handbook	HVAC Applications, 20031999				412.1.ABC.1, 412.1.ABC.2.1.1
ASHRAE Handbook	Fundamentals, 20051					202, B-3.1.1, B-3.1.2, B-3.13
ASHRAE Handbook	HVAC Systems & Equipment, 20040			410.1.ABC.3, 610.1.ABC.3
ASHRAE, 1998		Cooling and Heating Load Calculation Principles			607.1.ABC.1	

ASTM	ASTM International
100 Barr Harbor Dr
West Conshohocken, PA 19428-2959		
Standard reference number	Title				Referenced in Code  Section Number	
ASTM C36/C36M-03	Standard Specification for Gypsum Wallboard				202	
ASTM C90-06b 01a	Standard Specification for Loadbearing Concrete Masonry Units	402.1.C.1, B-1.2.3, B-2.2.1.1	
ASTM C 177-04 97	Test Method for Steady-State Heat Flux Measurements and Thermal 
Transmission Properties by Means of the Guarded-Hot-Plate Apparatus		410. 1.ABC.2.3, 
								610. 1.ABC.2.2, B-1.1.1	
ASTM C 236-89 (1993el)	Test Method For Steady-State Thermal Performance of Building Assemblies by 
Means of a Guarded Hot Box			602.1.A.2, B-1.1.1, B-1.1.2, C-2.2.2
ASTM C272-01 91 	Test Method for Water Absorption of Core Materials for Structural Sandwich 
Constructions								B-1.3.4	
ASTM C 335-05ae1 95	Test Method for Steady-State Heat Transfer Properties of Horizontal Pipe Insulations.												Table 411. 1.ABC.2
ASTM C 516-02		Vermiculite Loose Fill Thermal Insulation				Table 6C-2	
ASTM C 518-04 02	Test Method for Steady-State Thermal Transmission Properties by Means 
of the Heat Flow Meter Apparatus.					Table 6C-2
ASTM C 549-06 02	Perlite Loose Fill Insulation			
ASTM C 578-06 01	Rigid, Cellular Polystyrene Thermal Insulation			Table 6C-2	
ASTM C 665-06 01el	Mineral-Fiber Blanket Thermal Insulation for Light Frame Construction 
and Manufactured Housing					Table 6C-2	
ASTM C 727-01		Standard Practice for Installation and Use of Reflective Insulation in 
Building Constructions.						Table 6C-2	
ASTM C 739-05b 2000el	Cellulosic Fiber (Wood-Base) Loose-Fill Thermal Insulation		Table 6C-2	
ASTM C 764-06a 2002	Mineral Fiber Loose-Fill Thermal Insulation		Table 6C-2	
ASTM C835-95 (1999)	Standard Test Method for Total Hemispherical Emittance of Surfaces 
From 20ºC to 1400ºC					Table 6C-2	
ASTM C 976-90 (1996)el	Test Method for Thermal Performance of Building Assemblies by 
Means of a Calibrated Hot Box.					B-1.1.1, B-1.1.2	
ASTM C 1015-06 02	Standard Practice for Installation of Cellulosic and Mineral Fiber Loose-Fill 
Thermal Insulation						Table 13-6C-2
ASTM C 1029-05a	Specification for Spray-Applied Rigid Cellular Polyurethane Thermal Insulation														Appendix 13-C, 
ASTM C 1158-05 01	Standard Practice for Use and Installation of Radiant Barrier Systems (RBS)
 in Building Construction					607. 1.A.4, Table 6C-2	
ASTM C 1224-03 01	Reflective Insulation for Building Applications					607. 1.A.3.2, Table 6C-2	
ASTM C 1289-06 02	Faced Rigid Cellular Polyisocyanurate Thermal Insulation Board		Table 6C-2	
ASTM C 1313-05 00	Sheet Radiant Barriers for Building Construction Applications		607. 1.A.3.2, Table 6C-2	
ASTM C 1320-05 99	Standard Practice for Installation of Mineral Fiber Batt and Blanket Thermal 
			Insulation for Light-Frame Construction					Table 6C-2	
ASTM C 1321-04 96	Standard Practice for Installation and Use of Interior Radiation Control Coating
Systems (IRCC) in Building Construction					607. 1.A.4	
ASTM C1363-05		Standard Test Method for Thermal Performance of Building Materials and 
			Envelope Assemblies by Means of a Hot Box Apparatus	          602. 1.A.2, B-1.1.1, B-1.1.2, C-2.2.2 
ASTM C 1371-04a 98	Test Method for Determination of Emittance of Materials Near Room 
			Temperature Using Portable Emissometers.			404. 1.C.1, 607. 1.A.4	
ASTM C 1549-04 	Standard Test Method for Determination of Solar Reflectance Near Ambient Temperature 
Using a Portable Solar Reflector					404.C.1, 604.A.4
ASTM E 84-06a 01	Test Method for Surface Burning Characteristics of Building Materials												410.1.ABC.3.0.7, 610. 1.ABC.3.0.7	
ASTM E 283-04 91(1999)	Standard Test Method for Determining the Rate of Air Leakage Through Exterior 
Windows, Curtain Walls and Doors Under Specified Pressure Differences Across 
the Specimen.						406. 1.ABC, 406. 1.ABC.1.1, 
						606. 1.ABC.1.1, 606. 1.ABC.1.2.4, C-4.2.3	
ASTM E 408-71 (2002) 	Test Methods for Total Normal Emittance of Surfaces Using 
Inspection-Meter Techniques					404. 1.C.1
ASTM E 903-96 	Test Method for Solar Absorptance, Reflectance, and Transmittance of Materials 
Using Integrating Spheres				 404. 1.C.1, 604.A.4, 13-2C4.2.1.5 	
ASTM E 1175-87 (1996) 	Standard Test Method for Determining Solar or Photopic Reflectance,Transmittance, and Absorptance of Materials Using a Large Diameter Integrating Sphere	     404.1.C.1	
ASTM E 1918-06 97	Standard Test Method for Measuring Solar Reflectance of Horizontal and
 or Low-Sloped Surfaces in the Field				404.1.C.1, 604.A.4	
CRRC	Cool Roof Rating Council
	1738 Excelsior Avenue
	Oakland, CA 94602
Standard reference number	Title			Referenced in Code Section Number	
CRRC-1-2006		CRRC-1 Product Rating Program				404.C.1, 604.A.4

CTI	Cooling Technology Tower Institute
2611 FM 1960 West, Suite H-200
Houston, TX 77068-3730.		
Standard reference number	Title				Referenced in Code Section Number	
CTI ATC-105-2000(97)	Acceptance Test Code for Water Cooling Towers		Table 407. 1.ABC.3.2G	
CTI Std. 201-2002 96	Certification Standard for Water Cooling Tower Thermal Performance		
Table 407. 1.ABC.3.2G	
DASMA	Door and Access Systems Manufacturers Association
1300 Sumner Avenue
Cleveland, OH 44115-2851.		
Standard reference number	Title				Referenced in Code Section Number	
ANSI/DASMA105-1992	Test Method for Thermal Transmittance and Air Infiltration of Garage Doors	
(R1998)										406. 1.ABC.1.1,	

DOE	United States Department of Energy
c/o Superintendent of Documents
U.S. Government Printing Office
Washington, DC 20402-9325			
Standard reference number	Title				Referenced in Code Section Number	
DOE, 10 CFR, Part 430 Subpart B, App. E-1998 	Uniform Test Method for Measuring the Energy Consumption of Water Heaters 		Tables  408. 1.ABC.3.2F, 608. 1.ABC.3.2F, 412. 1.ABC.3,  612. 1.ABC.3.1.1, 612. 1.ABC.3.2Subpart B, App. M	Uniform Test Method for Measuring the Energy Consumption
of Central Air Conditioners						607. 1.ABC.3.1	
10 CFR, Part 430 Subpart B, App N -1998 	Uniform Test Method for Measuring the Energy Consumption
of Furnaces					Tables 408. 1.ABC.3.2E, 608. 1.ABC.3.2E	
DOE, 10 CFR, Part 430 Subpart B, App O-1998	Uniform Test for Measuring the Energy Consumption 
of Vented Home Heating Equipment					202	
EPACT, 92 42 USC 6831, et seq Public Law 102-486	Energy Policy Act of 1992	  407. 1.ABC.3.2, 414. 1.ABC.1, 607. 1.ABC.3.2.1	
NAECA, 1987	National Appliance Energy Conservation Act of 1987		Tables 407. 1.ABC.3.2A, B; 408. 1.ABC.2.2, Table 408. 1.ABC.3.2E, 607. 1.ABC.3.1, Tables 607. 1.ABC.3.2A, B, 608. 1.ABC.3.1 	

Florida Codes	Building Codes and Standards Office
Florida Department of Commuity Affairs
2555 Shumard Oak Blvd.
Tallahassee, FL 32399-2100		
Standard reference number	Title				Referenced in Code Section Number	
FL-1	Florida Standard for Desuperheater/Water Heaters (See Appendix E of this code)											612. 1.B.3.2, 612.2.A.3.1	

FSEC		Florida Solar Energy Center
1679 Clearlake Road
Cocoa, FL 32922-5703		

Standard reference	Title								Referenced in Code number											Section Number
FSEC-RR-54-00		"The HERS Rating Method and the Derivation of the 
Normalized Modified Loads Method", October 11, 2000,		13-613.A.2.1
Fairey, P., J. Tait, D. Goldstein, D. Tracey, M. Holtz, and					R. Judkoff .   Available online at:  
		http://www2.fsec.ucf.edu/en/publications/html/FSEC-RR-54-00/index.htm

2007			EnergyGauge USA Fla/Res			13-600.2, 13-600.A.1, 13-600.A.2, 13-601.A,
13-601.A.3, 13-602.A.1, 13-604.A.1,
13-601.A.4, 13-605.A.1, 13-606.A.1,
13-607.A.1, 13-608.A.1, 13-610.A.1, 
13-610.A.2, 13-612.A.1, 13-613.A.2.1

2007			EnergyGauge Summit Fla/Com			13-400.0.A, 13-400.0.C, 
13-400.0.C.4, 13-400.2, 13-400.3.ABC.1, 
13-400.3.ABC.2, 13-400.3.A, 13-400.3.B, 
Table 13-400.3.ABC.3, 13-401.A, 13-401.B, 
13-402.A, 13-402.B, 13-403.A, 13-403.B, 
13-404.ABC.1, 13-404.A, 13-404.B, 13-405.A, 
13-405.B, 13-407.A, 13-408.A, 13-410.A, 
13-412.A, 13-415.A, 13-415.B, 13-415.B.1

FTC	U.S. Federal Trade Commission
Sixth Street and Pennsylvania Avenue, N.W.
Washington, DC 20580		
Standard reference number	Title				Referenced in Code Section Number	
FTC, 16 CFR, Part 460,
Amended 
Effective 4/29/96	FTC Labeling and Advertising of Home Insulation		202, C-1.2	

GAMA	Gas Appliance Manufacturers Association
PO Box 9245
Arlington, VA 22209		
Standard reference number	Title				Referenced in Code Section Number	
GAMA	Consumers’ Directory of Certified Efficiency Ratings for Water Heating Equipment	Table 408. 1.ABC.3.2F, 
								Table 608. 1.ABC.3.2F, 612. 1.ABC.3.5, 612.2.A.1	

HI	Hydronics  Institute
P.O. Box 218
Berkeley Heights, NH  07922		
Standard reference number	Title				Referenced in Code Section Number	
H.I., HBS 86-1989	Testing and Rating Standard for Heating Boilers	Tables 408. 1.ABC.3.2F, 608. 1.ABC.3.2F	

HUD	U.S. Dept. Housing and Urban Development
451 7th Street S.W.
Washington, DC 20410		
Standard reference number	Title	Referenced in Code Section Number	
HUD, 24 CFR 3282-3283	Manufactured Home Procedural and Enforcement Regulations		202	
HUD, 42 CFR 70, s. 5401
(24 CFR 3280)	Manufactured Home Construction and Safety Standards			202	
HUD, 42 USC 77, s. 6295	 Energy Conservation Standards					202	

ISO	International Standards Organization
1, rue de Varembe, Case postale 56, 
CH-1211 Geneve 20, Switzerland		
Standard reference number	Title				Referenced in Code Section Number	
ISO 9806 (1994, 1995)	Test Methods for Solar Collectors
Part 1: Thermal Performance of glazed liquid heating collectors including pressure drop, December 1, 1994
Part 2: Qualification test procedures", August 15, 1995.
Part 3: Thermal performance of unglazed liquid heating collectors (sensible heat transfer only) including pressure drop", December 15, 1995.		612. 1.ABC.3.4	
ISO 13256-1 (1998)	 Water-Source Heat Pumps—Testing and Rating for Performance—
Part 1 Water-to-Air and Brine-to-Air Heat Pumps		Table 407. 1.ABC.3.2B, Table 607. 1.ABC.3.2B	

NAIMA	North American Insulation Manufacturers Association
44 Canal Center Plaza, Suite 310, 
Alexandria, VA 22314		
Standard reference number	Title				Referenced in Code Section Number	
NAIMA 2002 1993	Fibrous Glass Duct Construction Standards, Fifth Second
Edition					       410. 1.ABC.3.2, 610. 1.ABC.3.2	
NAIMA 2002 1994	Fibrous Glass Duct Liner Standard, Third edition   	  4101.ABC.2.5, 610. 1.ABC.2.4, 
										610. 1.ABC.3

NEBB	National Environmental Balancing Bureau
8575 Grovemont Circle
Gaithersburg, MD 20877-4121		
Standard reference number	Title				Referenced in Code Section Number	
NEBB, 2005 1998	Procedural Standards For Testing Adjusting and Balancing of 
Environmental Systems, Seventh Edition.			410. 1.ABC.4.3,	

NEMA	National Electrical Manufacturers Association
1300 N 17th Street, Suite 1847
Rosslyn, VA 22209		
Standard reference number	Title				Referenced in Code Section Number	
NEMA MG 1-20041998	Motors and Generators		202	

NFPA	National Fire Prevention Assoc.
Batterymarch Park
Quincy, MA 02269		
Standard reference number	Title				Referenced in Code Section Number	
NFPA 96-2004 2001	Ventilation Control and Fire Protection of Commercial Cooking Operations.									407. 1.ABC.3.5, 409. 1.ABC.3.6.1	

NFRC	National Fenestration Rating Council, Inc.
8484 Georgia Avenue, Suite 320
Silver Spring, MD 20910	
Standard reference number	Title				Referenced in Code Section Number	
NFRC 100-2004 01	Procedure for Determining Fenestration Product U-factors	601. 1.ABC.1, B-2.1, B-2.3NFRC 200-2004 01		Procedure for Determining Fenestration Product Solar Heat Gain 	401.2.AB.5,
Coefficients and Visible Transmitttance at Normal Incidence	601. 1.ABC.1, 601.2.A.2	
NFRC 300-2004 01	Standard Test Method for Determining the Solar Optical Properties of
Glazing Materials and Systems						B-2.1	
NFRC 400-2004 01	Procedure for Determining Fenestration Product U-factors Air Leakage		406. 1.ABC.1.1 	

SMACNA	Sheet Metal and Air-Conditioning Contractors’ National Association, Inc.
4201 Lafayette Center Dr.
Chantilly, VA 20151-1209		
Standard reference number	Title				Referenced in Code Section Number	
SMACNA, 1985	HVAC Air Duct Leakage Test Manual		410. 1.ABC.3.1.3, 610. 1.ABC.3, 610. 1.ABC.3.1.3	

SRCC	Solar Rating and Certification Corporation
c/o Florida Solar Energy Center
1679 Clearlake Road
Cocoa, FL 32922-5703		
Standard reference number	Title				Referenced in Code Section Number	
FSEC		Directory of Certified Solar Systems		612. 1.ABC.3.4, 612. 1.B.3.3	
SRCC TM-1	Solar Domestic Hot Water System and Component Test Protocol, December 6, 2002
											612. 1.ABC.3.4,	

UL	Underwriters Laboratory, Inc.
333 Pfingsten Rd.
Northbrook, Il. 60062-2096		
Standard reference number	Title				Referenced in Code Section Number	
UL 181-05 96	Standard for Factory-Made Air Ducts and Air Connectors with revisions
through December 1998.		410. 1.ABC.3.0.7, 410. 1.ABC.3.7.1, 610. 1.ABC.3, 
610.1.ABC.3.0.7, 610. 1.ABC.3.7.1	
UL 181A-0594	Closure Systems for Use With Rigid Air Ducts and Air Connectors, 
with revisions through December 1998.		4101..ABC.3.0.7, 610. 1.ABC.3, 610. 1.ABC.3.0.7
UL 181B-05 95	Closure Systems for Use With Flexible Air Ducts and Air Connectors with 
revisions through May 2000.			410. 1.ABC.3.0.7, 610. 1.ABC.3, 610. 1.ABC.3.0.7
UL 723-03	Standard for Test for Surface Burning Characteristics of Building Materials.	
									410. 1.ABC.3.0.7, 610. 1.ABC.3.0.7
UL 727-06 94	Standard for Oil-Fired Central Furnaces, with revisions through January 1999.		
Table 408. 1.ABC.3.2E, Table 608. 1.ABC.3.2E	
UL 731-95	Standard for Oil-Fired Unit Heaters, with revisions through January 1999.
							Table 408. 1.ABC.3.2E, Table 608. 1.ABC.3.2E	

WDMA	Window & Door Manufacturers Association
	1400 East Touhy Avenue, #470
	Des Plaines, IL 60018
Standard reference number	Title				Referenced in Code Section Number	
101/I.S.2/NAFS-02	Voluntary Performance Specifications for Windows, Skylights and Glass Doors  606.ABC.1.1

[Mod 2324]