REVISE SECTION 3001.1, NOTE2 TO READ AS FOLLOWS:

**SECTION 3001**

**GENERAL**

**3001.1 Scope.** This chapter governs the design, construction, installation, *alteration*, repair and maintenance of elevators and conveying systems and their components.

**Note1:** Other administrative and programmatic provisions may apply. See the Department of Business and Professional Regulation [DBPR] Chapter 399, *Florida Statutes*, and 61C-5, *Florida Administrative Code*. The regulation and enforcement of the following sections of the adopted codes, and their addenda, are preempted to the Bureau of Elevator Safety of the Department of Business and Professional regulation: ASME A17.1, ASME A17.3, and ASME A18.1.

**Note2**: This section does not apply to elevators in a private residence. Exception: elevators in a private residence, are not preempted, see Chapter 1 of this code.

**3001.2 Referenced standards.** Except as otherwise provided for in this code, the design, construction, installation, *alteration*, repair and maintenance of elevators and conveying systems and their components shall conform to ASME A17.1/CSA B44, ASME A17.3 and ASME A18.1, ASME A90.1, ASME B20.1, ALI ALCTV, and ASCE 24 for construction in *flood hazard areas* established in Section 1612.3. The Division of Hotels and Restaurants may grant exceptions, variances and waivers to the *Elevator Safety Code* as authorized by the *Safety Code for Elevators and Escalators* (ASME A17.1, Section 1.2) and *Florida Statutes* (Chapter 120.)

**3001.3 Accessibility.** Passenger elevators are required to be accessible by the *Florida Building Code, Accessibility*.

**3001.4 Change in use.** A change in use of an elevator from freight to passenger, passenger to freight, or from one freight class to another freight class shall comply with Section 8.7 of ASME A17.1/CSA B44.