This document created by the Florida Department of Business and Professional Regulation – Building Codes and Standards Office – 850-487-1824	

I-CODES - ADMINISTRATIVE - STRUCTURAL TAC

W

A

R

N

I

N

G

Copyright Notice: This document has been reproduced solely for considering proposed changes to the Florida Building Code with the permission of the International Code Council, Inc., is the copyrighted property of the International Code Council, Inc., all rights reserved, and may not be further reproduced or distributed.
W	A	R	N	I	N	G

1

BACK

Code Change No: ADM17-16 Part I

Original Proposal

Section: IEBC: 202

Proponent: David Bonowitz, representing Existing Buildings Subcommittee, National Counci of Structural Engineers Associations (dbonowitz@att.net)

THIS IS A 2 PART CODE CHANGE. PART I WILL BE HEARD BY THE IBC-STRUCTURAL CODE COMMITTEE. PART II WILL BE HEARD BY THE IRC-BUILDING CODE COMMITTEE. SEE THE TENTATIVE HEARING ORDERS FOR THESE COMMITTEES.

2015 International Existing Building Code

Delete without substitution:

202 LOAD-BEARING ELEMENT. Any column, girder, beam, joist, truss, rafter, wall, floor or roof sheathing that supports any vertical load in addition to its own weight or any lateral load.

Reason: This proposal deletes a definition that is incomplete and unnecessary.
First consider how the term is used in the codes, then consider the wording of the definition itself.
The term "load-bearing element" is actually never used in the IEBC. In the IRC, this three-word term is defined and used in only one place in Appendix J, to define Renovation to include "the change, strengthening or addition of load-bearing elements ..." However, a number of similar terms are used in a few places in the IEBC and throughout the IRC, but none of those cases relies on the definition (which is given only in the IEBC and in IRC Appendix J). These cases include:

"Load-bearing support": Used in IRC 105.2.2 and IEBC 105.2.2 to describe repairs that do not need permits, as "cutting of any structural beam or load-bearing support." Here the term is self-explanatory, and "structural beam" is redundant.
"Load-bearing member": Used in the IEBC definition of Technically Infeasible, related to accessibility upgrades, as "existing structural conditions require the removal or alteration of a load-bearing member that is an essential part of the structural frame." Here, the essential nature is given by the balance of the definition, so "load-bearing" adds nothing and is redundant. (Note: ICC should propose revisions to this definition from the ADA, but it is outside the scope of Group B.)
"Load bearing 	": Throughout Resource A, with no reliance on the structural meaning given in 202.
"Load-bearing wall": Defined in the IRC (under Walls) as "a wall supporting any vertical load in addition to its own weight." Thus, a wall that carries lateral load IS a "load-bearing element" in the IEBC but is NOT a "load-bearing wall" in the IRC.

Thus, "load-bearing" as actually used in the IEBC is generic and relies on common usage or separate definition, so no definition is needed in Section 202. And in the IRC, the IEBC definition actually creates confusion by overlapping and clashing with a separate IRC term. Since "load-bearing wall" is used much more specifically and frequently throughout the IRC, its definition should remain, and the unnecessary and generic definition from IEBC 202 should be deleted.
Now consider the specific wording of the IEBC definition. Again, the term "load-bearing element" is not used in the IEBC at all, but one might fairly expect the definition to apply where "load-bearing" is used as an adjective for certain structural element types. For example, the following terms are found throughout the IRC, which per R201.3, relies on the IBC and IEBC for definitions of undefined terms:

"Load-bearing values": Used in IRC Chapter 4 for soil properties.
"Load-bearing studs": Used in R505.1.2, R603.1.2, R804.1.2, etc.
"Load-bearing cold-formed steel framing members": Used in R603.2.1 and elsewhere, sometimes to mean wall studs, and sometimes to mean floor framing. As wall studs, these should be subject to the IRC definition of "load-bearing wall," but the definition is not clear.
"Load-bearing units": Used in IEBC A106 and IRC R606.2 to describe certain concrete masonry units, defined by reference to ASTM standards, with no reliance on the definition in 202.
"Load-bearing frames": Used in R606.12.2.2.1.
"Load-bearing piers": Used in AE601, AE602, etc.

Note that the IEBC definition does not mention soil, studs, framing, frames, or piers. Certainly one would expect the definition to apply, but by attempting to be complete, with its long list of structural member types, the definition ends up excluding (confusingly) other terms actually used in the code. And whether or not one would want the IEBC definition -- which considers both gravity and lateral loads -- to apply, confusion remains because the IRC almost routinely uses "load-bearing" to mean "carrying gravity loads other than self-weight."
Thus, the existing definition of Load-Bearing Element adds no value to the IEBC and introduces only confusion to the IRC.

Cost Impact: Will not increase the cost of construction
This is an editorial change, therefore there will be not change to construction requirements.

Report of Committee Action Hearings

Committee Action:	Approved as Submitted

Committee Reason: Deleting the definition for "load bearing element" eliminates a definition of a term that is not used in the IBC.

Assembly Action:	None

Final Action Results

ADM17-16 Part I	AS

BACK

Code Change No: ADM17-16 Part II

Original Proposal

Section: IRC: AJ201.1

Proponent: David Bonowitz, representing Existing Buildings Subcommittee, National Counci of Structural Engineers Associations (dbonowitz@att.net)

THIS IS A 2 PART CODE CHANGE. PART I WILL BE HEARD BY THE IBC-STRUCTURAL CODE COMMITTEE. PART II WILL BE HEARD BY THE IRC-BUILDING CODE COMMITTEE. SEE THE TENTATIVE HEARING ORDERS FOR THESE COMMITTEES.

2015 International Residential Code

AJ201.1 General. For purposes of this appendix, the terms used are defined as follows.

Delete without substitution:

LOAD-BEARING ELEMENT. Any column, girder, beam, joist, truss, rafter, wall, floor or roof sheathing that supports any vertical load in addition to its own weight, or any lateral load.

Reason: This proposal deletes a definition that is incomplete and unnecessary.
First consider how the term is used in the codes, then consider the wording of the definition itself.
The term "load-bearing element" is actually never used in the IEBC. In the IRC, this three-word term is defined and used in only one place in Appendix J, to define Renovation to include "the change, strengthening or addition of load-bearing elements ..." However, a number of similar terms are used in a few places in the IEBC and throughout the IRC, but none of those cases relies on the definition (which is given only in the IEBC and in IRC Appendix J). These cases include:

"Load-bearing support": Used in IRC 105.2.2 and IEBC 105.2.2 to describe repairs that do not need permits, as "cutting of any structural beam or load-bearing support." Here the term is self-explanatory, and "structural beam" is redundant.
"Load-bearing member": Used in the IEBC definition of Technically Infeasible, related to accessibility upgrades, as "existing structural conditions require the removal or alteration of a load-bearing member that is an essential part of the structural frame." Here, the essential nature is given by the balance of the definition, so "load-bearing" adds nothing and is redundant. (Note: ICC should propose revisions to this definition from the ADA, but it is outside the scope of Group B.)
"Load bearing 	": Throughout Resource A, with no reliance on the structural meaning given in 202.
"Load-bearing wall": Defined in the IRC (under Walls) as "a wall supporting any vertical load in addition to its own weight." Thus, a wall that carries lateral load IS a "load-bearing element" in the IEBC but is NOT a "load-bearing wall" in the IRC.

Thus, "load-bearing" as actually used in the IEBC is generic and relies on common usage or separate definition, so no definition is needed in Section 202. And in the IRC, the IEBC definition actually creates confusion by overlapping and clashing with a separate IRC term. Since "load-bearing wall" is used much more specifically and frequently throughout the IRC, its definition should remain, and the unnecessary and generic definition from IEBC 202 should be deleted.
Now consider the specific wording of the IEBC definition. Again, the term "load-bearing element" is not used in the IEBC at all, but one might fairly expect the definition to apply where "load-bearing" is used as an adjective for certain structural element types. For example, the following terms are found throughout the IRC, which per R201.3, relies on the IBC and IEBC for definitions of undefined terms:

"Load-bearing values": Used in IRC Chapter 4 for soil properties.
"Load-bearing studs": Used in R505.1.2, R603.1.2, R804.1.2, etc.
"Load-bearing cold-formed steel framing members": Used in R603.2.1 and elsewhere, sometimes to mean wall studs, and sometimes to mean floor framing. As wall studs, these should be subject to the IRC definition of "load-bearing wall," but the definition is not clear.
"Load-bearing units": Used in IEBC A106 and IRC R606.2 to describe certain concrete masonry units, defined by reference to ASTM standards, with no reliance on the definition in 202.
"Load-bearing frames": Used in R606.12.2.2.1.
"Load-bearing piers": Used in AE601, AE602, etc.

Note that the IEBC definition does not mention soil, studs, framing, frames, or piers. Certainly one would expect the definition to apply, but by attempting to be complete, with its long list of structural member types, the definition ends up excluding (confusingly) other terms actually used in the code. And whether or not one would want the IEBC definition -- which considers both gravity and lateral loads -- to apply, confusion remains because the IRC almost routinely uses "load-bearing" to mean "carrying gravity loads other than self-weight."
Thus, the existing definition of Load-Bearing Element adds no value to the IEBC and introduces only confusion to the IRC.

Cost Impact: Will not increase the cost of construction
This is an editorial change, therefore there will be not change to construction requirements.

Report of Committee Action Hearings

Committee Action:	Approved as Submitted

Committee Reason: The term defined is not used in the IRC.

Assembly Action:	None

Final Action Results

ADM17-16 Part II	AS

BACK

Code Change No: ADM72-16

Original Proposal

Section: IRC: R105.3.1.1, R301.2.4, R322.1

Proponent: Gregory Wilson, representing Federal Emergency Management Agency (gregory.wilson2@fema.dhs.gov); Rebecca Quinn, RCQuinn Consulting, Inc., representing RCQuinn Consulting on behalf of Federal Emergency Management Agency (rcquinn@earthlink.net)

THIS CODE CHANGE WILL BE HEARD BY THE IRC-BUILDING CODE COMMITTEE. SEE THE TENTATIVE HEARING ORDER FOR THIS COMMITTEE.

Revise as follows:

R105.3.1.1 Determination of substantially improved or substantially damaged existing buildings in flood hazard areas. For applications for reconstruction, rehabilitation, addition, alteration, repair or other improvement of existing buildings or structures located in a flood hazard area as established by Table R301.2(1), the building official shall examine or cause to be examined the construction documents and shall make a determination with regard to the value of the proposed work. For buildings that have sustained damage of any origin, the value of the proposed work shall include the cost to repair the building or structure to its predamaged condition. If the building official finds that the value of proposed work equals or exceeds 50 percent of the market value of the building or structure before the damage has occurred or the improvement is started, the proposed work is a substantial improvement
or restoration repair of substantial damage and the building official shall require existing portions of the entire building or structure to meet the requirements of Section R322.
For the purpose of this determination, a substantial improvement shall mean any repair, reconstruction, rehabilitation, addition or improvement of a building or structure, the cost of which equals or exceeds 50 percent of the market value of the building or structure before the improvement or repair is started. Where the building or structure has sustained substantial damage, repairs necessary to restore the building or structure to its predamaged condition shall be considered substantial improvements regardless of the actual repair work performed. The term shall not include either of the following:

Improvements to a building or structure that are required to correct existing health, sanitary or safety code violations identified by the building official and that are the minimum necessary to ensure safe living conditions.
Any alteration of a historic building or structure, provided that the alteration will not preclude the continued designation as a historic building or structure. For the purposes of this exclusion, a historic building shall be any of the following:
Listed or preliminarily determined to be eligible for listing in the National Register of Historic Places.
Determined by the Secretary of the U.S. Department of Interior as contributing to the historical significance of a registered historic district or a district preliminarily determined to qualify as an historic district.
Designated as historic under a state or local historic preservation program that is approved by the Department of Interior.

R301.2.4 Floodplain construction. Buildings and structures constructed in whole or in part in flood hazard areas (including A or V Zones) as established in Table R301.2(1), and substantial improvement and restoration repair of substantial damage of buildings and structures in flood hazard areas, shall be designed and constructed in accordance with Section R322. Buildings and structures that are located in more than one flood hazard area shall comply with the provisions associated with the most restrictive

9

flood hazard area. Buildings and structures located in whole or in part in identified floodways shall be designed and constructed in accordance with ASCE 24.

R322.1 General. Buildings and structures constructed in whole or in part in flood hazard areas, including A or V Zones and Coastal A Zones, as established in Table R301.2(1), and substantial improvement and restoration repair of substantial damage of buildings and structures in flood hazard areas, shall be designed and constructed in accordance with the provisions contained in this section. Buildings and
structures that are located in more than one flood hazard area shall comply with the provisions associated with the most restrictive flood hazard area. Buildings and structures located in whole or in part in identified floodways shall be designed and constructed in accordance with ASCE 24.
Reason: This proposal is editorial for consistency with the definition of "substantial Improvement," which uses the term "repair." It also corrects imprecise usage: damage is not, in fact, restore; damage is repaired.

Cost Impact: Will not increase the cost of construction Clarification of terms does not change the basic requirement.

Report of Committee Action Hearings

Committee Action:	Approved as Submitted

Committee Reason: This proposal clarifies the requirements for repair and restoration.

Assembly Action:	None

Final Action Results

ADM72-16	AS

10

BACK

Code Change No: ADM94-16

Original Proposal

The following table provides a comprehensive list of all standards that the respective standards promulgators have indicated have been, or will be, updated from the listing in the 2015 Editions of the International Codes. According to Section 4.5.1 of ICC Council Policy #CP 28, Code Development Policy, the updating of standards referenced by the Codes shall be accomplished administratively by the Administrative code development committee. Therefore, referenced standards that are to be updated for the 2018 edition of any of the I-Codes are listed in this single code change proposal. Note that the table below indicates the change to the standard, and the code or codes in which each standard appears. The list includes standards that the promulgators have already updated or will have updated by December 1, 2017.

AAMA	American Architectural Manufacturers Association	
Standard Reference Number	Title	Referenced in Code(s):	
AAMA/NSA/NPEA 2100-12	Specifications for Sunrooms	IRC								

AAMA/WDMA/CSA 101/I.S.2/A440-17	North American Fenestration Standard/Specification for Windows, Doors, and Skylights	

IBC	

IRC	

IECC						

AAMA 506-1116	Voluntary Specifications for Impact and Cycle Testing of Fenestrations Products	

IRC								

AAMA 711-1316	Voluntary Specification for Self Adhering Flashing Used for Installation of Exterior Wall Fenestration Products	

IRC								

712-11 14	Voluntary Specification for Mechanically Attached Flexible Flashing	

IRC								

714-12 15	Voluntary Specification for Liquid Applied Flashing Used to Create a Water-Resistive Seal Around Exterior Wall Openings in Buildings	

IRC								
ACCA	Air Conditioning Contractors of America	
Standard Reference Number	Title	Referenced in Code(s):	
Manual D-2011 16	Residential Duct Systems	IMC	IRC							

Manual J-2011 16	Residential Load Calculation - Eighth Edition	IECC-R	
IRC							

Manual S-13 14	
Residential Equipment Selection	IECC-R	
IRC							
ACI	American Concrete Institute	
Standard Reference Number	Title	Referenced in Code(s):	

332-14	Residential Code Requirements
for Structural Concrete Construction	
IRC								
530-13(This is now a TMS only document)	Building Code Requirements for Masonry Structures	
IBC	
IRC							
530.1-13(This is now a TMS only document)	Specifications for Masonry Structures	
IBC	
IRC							
AFSI	Architectural Fabric Structures Institute International	
Standard Reference Number	Title	Referenced in Code(s):	

ASI-77 FSAAS-16	Design and Standard Manual Fabric Structures Association Air Structures 2016	

IFC								
AHAM	Association of Home Appliance Manufacturers	
Standard Reference Number	Title	Referenced in Code(s):				11	

AHAM-HRF-1-20082016	Energy, Performance and Capacity of Household Refrigerators, Refrigerator-Freezers and Freezers	
IECC-C								
AHRI	Air-Conditioning, Heating & Refrigeration Institute	

Standard Reference Number	Title	Referenced in Code(s):	

210/240-08with Addenda 1 and 2 2016	Performance Rating of Unitary Air- Conditioning and Air-Source Heat Pump Equipment	
IECC_C								

310/380-042014 (CSA-C744-04)	Standard for Packaged Terminal Air Conditioners and Heat Pumps	IECC-C								

340/360-2007 with Addendum 2 2015	Performance Rating of Commercial and Industrial Unitary Air- Conditioning and Heat Pump Equipment	

IECC-C								

390-03 (I-P) 2015	Performance Rating of Single Package Vertical Air Conditioners and Heat Pumps	
IECC-C								

400-01 (I-P)-2015	Performance Rating of Liquid to Liquid Heat Exchangers with Addenda 1 and 2	
IECC-C								

440-08 with Addendum 1	
Performance of Room Fan-Coils	IECC-C								

550/590-2011with Addendum 1 (I-P)-2015	Performance Rating of Water- Chilling and Heat Pump Water- Heating Packages Using the Vapor Compression Cycle	

IECC-C								

700-20112015 with Addendum 1	Purity Specifications for Fluorocarbon and Other Refrigerants	

IMC								

1160 (I-P) - 09 2014	Performance Rating of Heat Pump Pool Heaters	IECC-C	ISPSC							

1200-2010 (I-P)-2013	Performance Rating of Commercial Refrigerated Display Merchandisers and Storage Cabinets	
IECC-C								
AISC	American Institute of Steel Construction	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/AISC 341-10 16	Seismic Provisions for Structural Steel Buildings	
IBC								

ANSI/AISC 360-1016	Specification for Structural Steel Buildings	
IBC								
AISI	American Iron and Steel Institute	
Standard Reference Number	Title	Referenced in Code(s):	

AISI S100-1216	North American Specification for the Design of Cold-Formed Steel Structural Members, 2012 2016	

IBC	

IRC							

AISI S220-1115	North American Standard for Cold- Formed Steel Framing-Nonstructural Members, 2011 2015	

IRC	

IBC							

AISI S230-07/S3-12 (2012) 15	Standard for Cold-Formed Steel Framing-Prescriptive Method for One- and Two-Family Dwellings, 2007, with Supplement 3, dated 2012 (Reaffirmed 2012) 2015	

IRC	

IBC							
ALI	Automotive Lift Institute	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/ALI ALCTV-20112016	Standard for Automotive Lifts - Safety Requirements for Construction, Testing, and Validation	

IBC							

12	

AMCA	Air Movement and Control Association International	
Standard Reference Number	Title	Referenced in Code(s):	

540-0813	Test Method for Louvers Impacted by Wind Borne Debris	
IBC								

550-08 09	Test Method for High Velocity Wind Driven Rain Resistant Louvers	
IMC								
ANCE	Association of the Electric Sector	
Standard Reference Number	Title	Referenced in Code(s):	

NMX-J-521/2-40-ANCE-20122014/ CAN/CSA-22.2 No. 60335-2-40-12/ UL/ 60335-2-40	Standard forSafety of Household and Similar Electric Appliances, Part 2- 40: Particular Requirements for Motor-Compressors Heat Pumps, Air Conditioners and Dehumidifiers	

IRC								
ANSI	American National Standards Institute	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI E1.21-20062013	Entertainment Technology- Temporary Structures Used for Technical Production of Outdoor Entertainment Events	

IFC								
APA	APA-The Engineered Wood Association	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/AITC A 190.1-12 2017	Structural Glued Laminated Timber	
IBC	
IRC							
ANSI/APA PRG-320-2011 2017	Standard for Performance-Rated Cross-Laminated Timber	
IBC	
IRC							

ANSI/APA PRP 210-082014	Standard for Performance-Rated Engineered Wood Siding	

IBC	

IRC							

ANSI/APA PRR 410-20112016	Standard for Performance-Rated Engineered Wood Rim Boards	
IRC	
IBC							

ANSI 117-1015	Standard Specification for Structured Glued Laminated Timber of Softwood Species	

IBC								
APA E30-1115	Engineered Wood Construction Guide	
IRC								

APA PDS Supplement 5-12 16	Design and Fabrication of All- plywood Beams (revised 2013)	

IBC								

EWS APA R540-1213	Builders Tips: Proper Storage and Handling of Glulam Beams	
IBC								

EWS APA S475-07 16	Glued Laminated Beam Design Tables	
IBC								

EWS APA S560-1014	Field Notching and Drilling of Glued Laminated Timber Beams	
IBC								

EWS APA T300-07 16	Glulam Connection Details	
IBC								
EWS APA X440-08 17	Product Guide - Glulam	IBC								

EWS APA X450-01	Glulam in Residential Construction - Western Edition	
IBC								
APSP	The Association of Pool & Spa Professionals	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/APSP/ICC-4 2012 Includes Addenda A Approved April 4, 2013	American National Standard for Aboveground/Onground Residential Swimming Pools	

ISPSC								

ANSI/APSP/ICC-14- 112014	American National Standard for Portable Hot Tub Energy Efficiency	
ISPSC	IECC- R							

ANSI/APSP/ICC-15a-20132011 Includes
Addenda A Approved January 9, 2013	American National Standard for Energy Efficiency for Residential Inground Swimming Pools and Spas	

ISPSC	
IECC- R							

ANSI/APSP/ICC 7-2013	American National Standard for Suction Entrapment Avoidance in Swimming Pools, Wading Pools, Spas, Hot Tubs, and Catch Basins	

IBC	

IRC	

ISPSC						
ASABE	American Society of Agricultural & Biological Engineers	
Standard Reference Number	Title	Referenced in Code(s):	

EP 484.2JUNE1998 3 MON2016	Diaphragm Design of Metal-Clad, Wood-Frame Rectangular Buildings	

IBC								

EP 486.2 OCT 2012ED	Shallow Post and Pier Foundation Design	

IBC								

EP 559.1 2 W/Corr. 1 MON2016	Design Requirements and Bending Properties for Mechanically Laminated Wood Assemblies	

IBC								
ASCE	American Society of Civil Engineers	
Standard Reference Number	Title	Referenced in Code(s):	

ASCE 5-13 is now TMS 402	Building Code Requirements for Masonry Structures now a TMS standard	

IBC	

IRC							
ASCE 6-13 is now TMS 602	Specifications for Masonry Structures now a TMS Standard	
IBC	
IRC							

7-10 16	Minimum Design Loads and Associated Criteria for Buildings and Other Structures with Supplement No. 1	

IBC	

IRC	

IEBC						

8—14 17	Standard Specification for the Design of Cold-formed Stainless Steel Structural Members	

IBC								

19-09 16	Structural Applications of Steel Cables for Buildings	
IBC								

29-1417	Standard Calculation Methods for Structural Fire Protection	
IBC								

32-01 17	Design and Construction of Frost Protected Shallow Foundations	
IBC	
IRC							

41-13 17	Seismic Evaluation and Retrofit of Existing Buildings	

IEBC								
55-1016	Tensile Membrane Structures	IBC								
ASHRAE	American Society of Heating, Refrigerating and Air Conditioning Engineers	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/ASHRAE/ACCA 183-(RA20112014)	Peak Cooling and Heating Load Calculations in Buildings, Except Low-rise Residential Buildings	
IECC-C								

ASHRAE-20122016	HVAC Systems and Equipment Handbook	
IMC	IECC- C							

ASHRAE-20132017	ASHRAE Handbook of Fundamentals	
IRC	IECC- R	
IMC						

15-2013 2016	Safety Standard for Refrigeration Systems	
IMC	
IFC							

34-2013 2016	Designation and Safety Classification of Refrigerants	
IRC	
IMC							

62.1-2013 2016	Ventilation for Acceptable Indoor Air Quality	
IMC	
IEBC							

90.1-20132016	Energy Standard for Buildings Except Low-Rise Residential Buildings	
IECC-C								

140-20112017	Standard Method of Test for the Evaluation of Building Energy Analysis Computer Programs	
IECC-C								
170-20082017	Ventilation of Health Care Facilities	IMC								

193-2010 (RA2014)	Method of Test for Determining Air Tightness of HVAC Equipment	
IRC	
IECC							

13256-1(2011) (2017)	Water- to-Air and Brine to Air Heat Pumps - Testing and Rating for Performance	

IECC								

13256-2(2011)(2017)	Water-to-Water and Brine-to-Water Heat Pumps - Testing and Rating for Performance	

IECC								
ASME	The American Society of Mechanical Engineers	
Standard Reference Number	Title	Referenced in Code(s):	

A13.1-2007 2015	Scheme for the Identification of Piping Systems	
IBC	
IFC	
IFGC						

A17.3-2009 2015	Safety Code for Existing Elevators and Escalators	
IFC	
IEBC							

A18.1-2008-2014	Safety Standard for Platform Lifts and Stairway Chairlifts	
IBC	
IFC	
IEBC	
IRC					
A90.1-09 2015	Safety Standards for Belt Manlifts	IBC								

A112.1.2-2004 2012	
Air Gaps in Plumbing Systems	
IPC	
IRC	ISPSC						

A112.1.3-2000(Reaffirmed 2011) (R2015)	Air Gap Fittings for Use with Plumbing Fixtures, Appliances, and Appurtenances	

IPC								

A112.3.1-2007 (R2012)	Stainless Steel Drainage Systems for Sanitary DWV, Storm and Vacuum Applications, Above and Below-Ground	

IPC	

IRC							

A112.4.14-2004(R2010) 2016	Manually Operated, Quarter-Turn Shutoff Valves for Use in Plumbing Systems	

IRC	

IPC							

A112.6.1M-1997(Reaffirmed 2008) (R2012)	Floor-Affixed Supports for Off-the- Floor Plumbing Fixtures for Public Use	

IPC	

IRC							

A112.6.2-2000 (R2010) 2016	Framing-Affixed Supports for Off-the- Floor Water Closets with Concealed Tanks	

IPC	

IRC							
A112.6.3-2001(R2007) 2016	Floor and Trench Drains	IPC	IRC							
A112.6.4-2003 (R2008) (R2012)	Floor and Trench Drains	IPC	IRC							

A112.6.7-2010 (R2015)	Enameled and Epoxy Coated Cast Iron and PVC Plastic Sanitary Floor Sinks	

IPC								
A112.6.9-2005(R2010)2015	Siphonic Roof Drains	IPC								
A112.14.1-2003(R2008)(R2012)	Backwater Valves	IPC								
A112.14.3-2000 (R2004)2016	Grease Interceptors	IPC								

A112.14.4-2001 (R2007)(R2012)	
Grease Removal Devices	
IPC								

A112.14.6-2010 (R2015)	FOG (Fats, Oils, and Greases) Disposal Systems	
IPC								

A112.18.3M-2002 (R2008) (R2012)	Performance Requirements for Backflow Protection Devices and Systems in Plumbing Fixture Fittings	

IPC	

IRC							

A112.19.12-20062014	Wall Mounted and Pedestal Mounted, Adjustable, Elevating,Tilting, and Pivoting Lavatory, and Sink, and Shampoo Bowl Carrier Systems and Drain Waste Systems	

IPC	

IRC							

A112.19.14-2006(R2011)2013	Six-Liter Water Closets Equipped with a Dual Flushing Device	
IPC	
IRC							
A112.19.15-20052012	Vitreous China Non-Water Urinals	IPC								
A112.19.19-2006(R2011)	Vitreous China Non-Water Urinals	IPC								
A112.36.2M-1991(R2008)(R2012)	Cleanouts	IPC	IRC							

ASME A17.1-2013 2016/CSA B44-16	Safety Code for Elevators and Escalators	
IBC	
IFC	
IEBC	
IRC	
IPMC	IECC- C			

ASME A17.7-2007/CSA B44-07 (R2012)	Performance-Based Safety Code for Elevators and Escalators	
IBC								
ASME A112.4.2-2009 2015 /CSA B45.16- 15	Water Closet Personal Hygiene Devices	
IPC	
IRC							
ASME A112.18.2-20112015/CSA B125.1-1115	
Plumbing Waste Fittings	
IPC	
IRC							
ASME A112.18.6-2009/CSA B125.6-09 (R2014)	
Flexible Water Connectors	
IPC	
IRC							
ASME A112.19.5-20112016/CSA B45.15-20112016	Flush Valves and Spuds for Water Closets, Urinals and Tanks	
IPC	
IRC							

B1.20.1-1983(R2006)2013	Pipe Threads, General Purpose (Inch)	
IPC	
IMC	
IRC						

B16.1-20102015	Cast Gray Iron Pipe Flanges and Flanged Fittings, Classes 25, 125
and 250	

IFGC								

B16.3-20112016	Malleable Iron Threaded Fittings Classes 150 and 300	
IPC	
IRC	
IMC						

B16.4—20112016	Gray Iron Threaded Fittings Class 125 and 250	
IPC	
IRC							

B16.5-20092015	Pipe Flanges and Flanged Fittings NPS 1/2 Through NPS 24 Metric/Inch Standard	

IMC	

IFGC							

B16.9-20072012	Factory-Made Wrought Steel Buttwelding Fittings	
IPC	
IRC	
IMC						

B16.11-20112016	Forged Fittings, Socket-Welding and Threaded	
IPC	
IMC	
IRC						

B16.12-2009 (R2014)	Cast Iron Threaded Drainage Fittings	
IRC	
IPC							

B16.15-20112013	Cast BronzeAlloy Threaded Fittings:

 Classes 125 and 250	
IRC	
IMC	
IPC	ISPSC					

B16.22-2001(R2010)2013	Wrought Copper and Copper Alloy Solder Joint Pressure Fittings	
IPC	
IBC	
IRC	
IFC	
IMC				

B16.23-2002(R2011)2016	Cast Copper Alloy Solder Joint Drainage Fittings: DWV	
IPC	
IRC							

B16.24-20112016	Cast Copper Alloy Pipe Flanges and Flanged Fittings: Class 150, 300,
400, 600, 900, 1500 and 2500	

IMC	

IFGC							

B16.26-20112016	Cast Copper Alloy Fittings for Flared Copper Tubes	
IPC	
IMC	
IRC						

B16.34-20092015	Valves Flanged, Threaded and Welding End	
IPC	
IRC							

B16.42-20112016	Ductile Iron Pipe Flanges and Flanged Fittings, Classes 150 and 300	

IFGC								

B16.44-2002(R2007)2012	Manually Operated Metallic Gas Valves For Use in Above Ground Piping Systems up to 5 psi	

IFGC	

IRC							

B16.47-20112016	Large Diameter Steel Flanges: NPS 26 through NPS 60 Metric/Inch Standard	

IFGC								

B16.51-20112013	Copper and Copper Alloy Press- Connect Pressure Fittings	
IRC	
IMC	
IPC						

B20.1-2009 2015	Safety Standard for Conveyors and Related Equipment	
IBC								
B31.1-20122016	Power Piping	IFC								
B31.3-20122016	Process Piping	IBC	IFC	IFGC						

B31.4-20122015	Pipeline Transportation Systems for Liquids and Slurries Hydrocarbons and Other Liquids	

IFC								

B31.5-20102016	Refrigeration Piping and Heat Transfer Components	
IPC	
IMC							
B31.9-20112014	Building Services Piping	IFC	IMC							
B31.12-20082014	Hydrogen Piping and Pipelines	IFGC								

B36.10M-2004 (R2015)	Welded and Seamless Wrought Steel Pipe	
IFGC	
IRC							

BPVC-2010/2011 addenda 2015	ASME Boiler & Pressure Vessel Code (2007 Edition)	
IMC	
IFC	
IFGC	
IRC					

CSD-1-20112016	Controls and Safety Devices for Automatically Fired Boilers	
IRC	
IMC							
PTC 4.1-2008 2013	

Fired Steam Generators	

IECC								
ASSE-Safety	American Society of Safety Engineers	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/ASSE Z359.1-20072016	Safety Requirements for Personal Fall Arrest Systems, Subsystems and Components, Part of
the ANSI/ASSE Z359 Fall Protection Code	

IBC	

IFC	

IMC						
ASSE	ASSE International	
Standard Reference Number	Title	Referenced in Code(s):	

ASSE 1002-2008 2015/ASME A112.1002- 2015/CSA B125.12-15	Performance Requirements for Antisiphon Fill Valves for Water Closet Flush Tanks	

IPC	

IRC							

ASSE 1004-20082016	Performance Requirements for Commercial Dishwashing Machines	
IPC								

ASSE 1037-20102015/ASME A112.1037- 2015/CSA B125.37-15	Performance Requirements for Pressurized Flushing Devices for Plumbing Fixtures	

IPC	

IRC							

ASSE 1070-20042015/ASME A112.1070- 2015/CSA B125.70-15	Performance Requirements for Water Temperature Limiting Devices	

IRC	

IPC							

1001-20082016	Performance Requirements for Atmospheric Type Vacuum Breakers	

IPC	

IRC							

1011-20042016	Performance Requirements for Hose Connection Vacuum Breakers	
IRC	
IPC							

1013-20092017	Performance Requirements for Reduced Pressure Principle Backflow Preventers and Reduced Pressure Principle Fire Protection Backflow Preventers	

IPC	

IRC							

1015-20092017	Performance Requirements for Double Check Backflow Prevention Assemblies and Double Check Fire Protection Backflow Prevention Assemblies	

IPC	

IRC							

1018-20102017	Performance Requirements for Trap Seal Primer Valves - Potable Water Supplied	

IPC	

IRC							

1019-20112016	Performance Requirements for Vacuum Breaker Wall Hydrants, Freeze Resistant, Automatic Draining Type	

IPC	

IRC							

1022-20032016	Performance Requirements for Backflow Preventer for Beverage Dispensing Equipment	

IPC								

1023-19792016	Performance Requirements for Hot Water Dispensers - Household Storage Type - Electrical	

IRC								

1024-20042016	Performance Requirements for Dual Check Valve Backflow Preventers, Anti-Siphon-type, Residential Applications	

IRC	

IPC							

1047-20092017	Performance Requirements for Reduced Pressure Detector Fire Protection Backflow Prevention Assemblies	

IPC	

IRC							

1048-20092017	Performance Requirements for Double Check Detector Fire Protection Backflow Prevention Assemblies	

IRC	

IPC							

1052-20042016	Performance Requirements for Hose Connection Backflow Preventers	
IRC	
IPC							

1055-20092016	Performance Requirements for Backflow Devices for Chemical Dispensing Systems	

IPC								

1056-20102013	Performance Requirements for Spill Resistant Vacuum Breaker	
IPC	
IRC							

1060-20062016	Performance Requirements for Outdoor Enclosures for Fluid Conveying Components	

IPC	

IRC							

1061-20102015	Performance Requirements for Removable and Non-Removable Push Fit Fittings	

IPC	

IRC							

1062-20062016	Performance Requirements for Temperature Actuated, Flow Reduction (TAFR) Valves to Individual Supply Fittings	

IPC	

IRC							

1066-19972016	Performance Requirements for Individual Pressure Balancing In- Line Valves for Individual Fixture Fittings	

IPC	

IRC							

2060-20062016	Performance Requirements for Outdoor Enclosures for Fluid Conveying Components	

IPC	

IRC							

5013-20092015	Performance Requirements for Testing Reduced Pressure Principle Backflow Preventers (RP) and Reduced Pressure Principle Fire Protection Backflow Preventers (RFP)	

IPC								

5015-20092015	Performance Requirements for Testing Double Check Valve Backflow Prevention Assembly (DC) and Double Check Fire Protection Backflow Prevention Assemblies (DCF)	

IPC								

5020-20092015	Performance Requirements for Testing Pressure Vacuum Breaker Assemblies (PVBA)	

IPC								

5047-20092015	Performance Requirements for Testing Reduced Pressure Detector Fire Protection Backflow Prevention Assemblies (RPDA)	

IPC								

5048-20092015	Performance Requirements for Testing Double Check Valve Detector Assembly (DCDA)	

IPC								

5056-20092015	Performance Requirements for Testing Spill Resistant Vacuum Breaker (SRVB)	

IPC								
ASTM	ASTM	
Standard Reference Number	Title	Referenced in Code(s):	

A6/A6M-11 14	Standard Specification for General Requirements for Rolled Structural Steel Bars, Plates, Shapes and Sheet	

IBC								
A36/A 36M-08 14	Specification for Carbon Structural Steel	
IBC	
IRC							

A74-13A15	Specification for Cast Iron Soil Pipe and Fittings	
IPC	
IMC	
IRC	
IFGC					

A106/A 106M-1114	Specification for Seamless Carbon Steel Pipe for High-Temperature Service	

IMC	

IRC	

IFGC						

A123/A123M-0215	Specification of Zinc (Hot-Dip Galvanized) Coating on Iron and Steel Products	

IBC								

A126-0904(2014)	Gray Iron Castings for Valves, Flanges, and Pipe Fittings	
IMC	
IRC							

A182-1315	Standard Specification for Forged and Rolled Alloy and Stainless Steel Pipe Flanges, Forged Fittings and Valves and Parts for High- Temperature Service	

ISPSC								

A234/A234M-11a15	Standard Specification for Piping Fittings of Wrought CarbonSteel and Alloy Steel for Moderate and High Temperature Service	

IMC								

A240/A240M-13A15a	Standard Specification for Chromium and Chromium-Nickel  Stainless Steel Plate, Sheet and Strip for Pressure Vessels and for General Applications	

IBC	

IRC	

ISPSC						

A254-97(2007)12	Specification for Copper Brazed Steel Tubing	
IMC	
IRC	
IFGC						

A283/A283M-12A13	Specification for Low and Intermediate Tensile Strength Carbon Steel Plates	

IBC								

A307-1214	Specification for Carbon Steel Bolts and Studs, 60,000 psi Tensile Strength	

IRC								

A312/A312M-13A15A	Specification for Seamless, and Welded, and Heavily Cold Worked Austenitic Stainless Steel Pipes	

IPC	

IRC	
ISPSC						

A395/A395-99(2009)(2014)	Standard Specification for Ferritic Ductile Iron Pressure-Retaining Casting for Use at Elevated Temperatures	

IMC								

A403-1315	Standard Specification for Wrought Austenitic Stainless Steel Piple Fittings	

ISPSC								

A416/A416M-12A15	Specification for Steel Strand, Uncoated Seven-Wire for Prestressed Concrete	

IBC								

A420A/A 420M-10A14	Specification for Piping Fittings of Wrought Carbon Steel and Alloy Steel for Low-Temperature Service	

IMC								

A463M/A 463M-1015	Specification for Steel Sheet, Aluminum-Coated, by the Hot Dip Process	

IBC	

IRC							

A510/A510M-13	Specification For General Requirements for Wire Rods and Coarse Round Wire, Carbon Steel, Alloy Steel	

IRC								

A536-84(2009)(2014)	Standard Specification for Ductile Iron Castings	
IMC								

A572/A572M-12A15	Specification for High-Strength Low- Alloy Columbium-Vanadium Structural Steel	

IBC								

A588/A588M-1015	Specification for High-Strength Low- Alloy Structural Steel with 50 ksi (345 Mpa) Minimum Yield Point, with Atmospheric Corrosion Resistance	

IBC								

A615/A615M-122015aE1	Specification for Deformed and Plain Billet Carbon-Steel Bars for Concrete Reinforcement	

IBC	

IRC							

A641/A641M-09A(2014)	Specification for Zinc-Coated (Galvanized) Carbon Steel Wire	
IRC								

A653/A653M-1115	Specification for Steel Sheet, Zinc- Coated Galvanized or Zinc-Iron Alloy-Coated Galvannealed by the Hot-Dip Process	

IBC	

IRC							

A690/690M-07(2012)13a	Standard Specification for High- Strength Low-Alloy Nickel, Copper Phosphorus Steel H-Piles and Sheet Piling with Atmospheric Corrosion Resistance for Use in Marine Environments	

IBC								

A706/A706M-09b15	Specification for Low-Alloy Steel Deformed and Plain Bars for Concrete Reinforcement	

IBC	

IRC							

A722/A722M-1215	Specification for Uncoated High- Strength Steel Bar for Prestressing Concrete	

IBC								

A733-2003(2009)e115	Specification for Welded and Seamless Carbon Steel and Austenitic Stainless Steel Pipe Nipples	

IPC								

A755/A755M-201115	Specification for Steel Sheet, Metallic-Coated by the Hot-Dip Process and Prepainted by the Coil- coating Process for Exterior Exposed Building Products	

IBC	

IRC							

A767/A767M-0509	Specification for Zinc-Coated (Galvanized) Steel Bars for Concrete Reinforcement	

IBC								

A775/A775M-07B(2014)	Specification for Epoxy-Coated Steel Reinforcing Bars	
IBC								

A778-01(2009)e1 /A778M-15	Specification for Welded Unannealed Austenitic Stainless Steel Tubular Products	

IPC	

IRC							

A792/A792M-10(2015)	Specification for Steel Sheet, 55% Aluminum-Zinc Alloy-Coated by the Hot-Dip Process	

IBC	

IRC							

A875/A875M-13	Standard Specification for Steel Sheet Zinc-5%, Aluminum Alloy- Coated by the Hot-Dip Process	

IBC	

IRC							

A888-13A15	Specification for Hubless Cast Iron Soil Pipe and Fittings for Sanitary and Storm Drain, Waste, and Vent Piping Application	

IPC	

IPSDC	

IRC						

A924/A924M-1314	Standard Specification for General Requirements for Steel Sheet, Metallic Coated by the Hot Dip Process	

IBC	

IRC							

A951/A951M-1114	Specification for Steel Wire Masonry Joint Reinforcement	
IRC								

A996/A996M-2009b15	Specification for Rail-Steel and Axle- Steel Deformed Bars for Concrete Reinforcement	

IRC								

A1003/A1003M-13A15	Standard Specification for Steel Sheet, Carbon, Metallic- and Nonmetallic-Coated for Cold-Formed Framing Members	

IRC								

B32-08(2014)	
Specification for Solder Metal	
IPC	
IMC	
IRC	IPSDC					

B42-102015A	Specification for Seamless Copper Pipe, Standard Sizes	
IPC	
IBC	
IRC	
IFC					

B43-0915	Specification for Seamless Red Brass Pipe, Standard Sizes	
IPC	
IBC	
IRC	
IFC					

B68/B68M-11	Specification for Seamless Copper Tube, Bright Annealed (Metric)	
IBC	
IFC	
IMC						

B75/B75M-11	Specification for Seamless Copper Tube	
IPC	IPSDC	
IRC	
IMC					

B88-0914	Specification for Seamless Copper Water Tube	
IPC	
IBC	IPSDC	
IRC					

B209-1014	Specification for Aluminum and Aluminum-Alloy Steel and Plate	
IBC	
IRC							

B227-1015	Specification for Hard-Drawn Copper-Clad Steel Wire	
IRC								

B280-0813	Specification for Seamless Copper Tube for Air Conditioning and Refrigeration Field Service	

IMC	

IFC	

IBC	

IFGC					

B306-0913	Specification for Copper Drainage Tube (DWV)	
IPC	
IRC							

B370-12	Specification for Cold Rolled Copper Sheet and Strip for Building Construction	

IBC	

IRC							

B584-1114	Standard Specification for Copper Alloy Sand Castings for General Applications	

IMC								

C4-04(2009)(14)	Specification for Clay Drain Tile and Perforated Clay Drain Tile	
IPC	IPSDC	
IRC						

C14-1115a	Specification for Nonreinforced Concrete Sewer, Storm Drain, And Culvert Pipe	

IPC	
IPSDC	

IRC						
C22/C22M-00(2010) 2015	Specification for Gypsum	IBC	IRC							

C27-98(2008)(13)	Specification for Standard Classification of Fireclay and High- Alumina Refractory Brick	

IBC	

IRC							
C28/C28M-10(2015)	Specification for Gypsum Plasters	IBC	IRC							

C31/C31M-1215	Practice for Making and Curing Concrete Test Specimens in the Field	

IBC								
C34-1213	Clay Load-Bearing Wall Tile	IBC	IRC							

C35/C35M-1995(2009) (2014)	Specification for Inorganic Aggregates for Use in Gypsum Plaster	

IBC	

IRC							

C55-20112014A	Specification for Concrete Building Brick	
IBC	
IRC							

C56-1213	Specification for Structural Clay Non-Lead-Bearing Tile	
IRC								

C59/C59M-00(2011) 2015	Specification for Gypsum Casting Plaster and Molding Plaster	
IBC	
IRC							

C61/C61M-00(2011)2015	Specification for Gypsum Keene's Cement	
IBC	
IRC							

C62-13A	Specification for Building Brick (Solid Masonry Units Made From Clay or Shale)	

IBC	

IRC							

C67-1314	Test Methods of Sampling and Testing Brick and Structural Clay Tile	

IBC								

C73-1014	Specification for Calcium Silicate Face Brick (Sand-Lime Brick)	
IBC	
IRC							

C76-13A15A	Specification for Reinforced Concrete Culvert, Storm Drain, and Sewer Pipe	

IPC	
IPSDC	

IRC						

C90-1314	Specification for Loadbearing Concrete Masonry Units	
IBC	
IRC	IECC- C	
IEBC					
C91/C91M-12	Specification for Masonry Cement	IBC	IRC							

C94/C94M-1315A	Specification for Ready-Mixed Concrete	
IBC	
IRC							

C109/C109M-122015e1	Standard Test Method for Compressive Strength of Hydraulic Cement Mortars (Using 2-in. or [50- MM] Cube Specimens)	

IRC								

C126-1315	Specification for Ceramic Glazed Structural Clay Facing Tile, Facing Brick, and Solid Masonry Units	

IRC								

C129-1114A	Specification for Nonload-bearing Concrete Masonry Units	
IRC								

C140/C140M-1315	Test Method Sampling and Testing Concrete Masonry Units and Related Units	

IBC	

IRC							

C141/C141M-0914	Standard Specification for Hydrated Hydraulic Lime for Structural Purposes	

IRC								

C143/C143M-1215	Test Method for Slump of Hydraulic Cement Concrete	
IRC								
C150/C150M-1215	Specification for Portland Cement	IBC	IRC							

C172/C172M-1014A	Practice for Sampling Freshly Mixed Concrete	
IBC								

C206-1314	Specification for Finished Hydrated Lime	
IBC	
IRC							

C212-1014	Specification for Structural Clay Facing Tile	
IBC	
IRC							

C216-1315	Specification for Facing Brick (Solid Masonry Units Made from Clay or Shale)	

IBC	

IRC							

C270-12a14A	Specification for Mortar for Unit Masonry	
IBC	
IRC							

C296/C296M-00(2009)e12015	Specification for Asbestos-Cement Pressure Pipe	
IPC	
IRC							
C317/C317M-00(2010)(2015)	Specification for Gypsum Concrete	IBC								

C330/C330M-200914	Specification for Lightweight Aggregates for Structural Concrete	
IBC								

C331/C331-20102014	Specification for Lightweight Aggregates for Concrete Masonry Units	

IBC								
C406/C406M-201015	Specification for Roofing Slate	IBC	IRC							

C425-04(2009)(2013)	Specification for Compression Joints for Vitrified Clay Pipe and Fittings	

IPC	
IPSDC	

IRC						

C472-99(2009) (2014)	Specification for Standard Test Methods for Physical Testing of Gypsum, Gypsum Plasters and Gypsum Concrete	

IBC								

C473-1215	Test Methods for Physical Testing of Gypsum Panel Products	

IBC								

C474-1315	Test Methods for Joint Treatment Materials for Gypsum Board Construction	

IBC								

C475/C475M-1215	Specification for Joint Compound and Joint Tape for Finishing Gypsum Wallboard	

IBC	

IRC							

C503/C503M-2010	Specification for Marble Dimension Stone (Exterior)	

IRC								

C508-00/C508M-00(2009)E1(2015)	Specification for Asbestos-Cement Underdrain Pipe	

IPC	

IRC							

C514-04(2009)e1 (2014)	Specification for Nails for the Application of Gypsum Board	

IBC	

IRC							

C516-08(2014)E1	Specification for Vermiculite Loose Fill Thermal Insulation	

IBC								

C518-0415	Test Method for Steady-State Thermal Transmission Properties by Means of the Heat Flow Meter Apparatus	

IECC								

C547-1215	Specification for Mineral Fiber Pipe Insulation	

IBC								

C552-12b15	Standard Specification for Cellular Glass Thermal Insulation	
IBC	
IRC							

C564-1214	Specification for Rubber Gaskets for Cast Iron Soil Pipe and Fittings	

IPC	
IPSDC	

IRC						

C568/C568M-2010	Specification for Limestone Dimension Stone	

IRC								

C578-12B15	Standard Specification for Rigid, Cellular Polystyrene Thermal Insulation	

IBC	

IRC							
C587-04(2009)(2014)	Specification for Gypsum Veneer Plaster	
IBC	
IRC							

C595/C595M-1314E1	Specification for Blended Hydraulic Cements	

IBC	

IRC							

C629-10/C629M-10	Specification for Slate Dimension Stone	

IRC								

C631-09(2014)	Specification for Bonding Compounds for Interior Gypsum Plastering	

IBC	

IRC							

C635/C635M-13A	Specification for the Manufacture, Performance, and Testing of Metal Suspension Systems for Acoustical Tile and Lay-In Panel Ceilings	

IBC								

C636/C636M-0813	Practice for Installation of Metal Ceiling Suspension Systems for Acoustical Tile and Lay-In Panels	

IBC								

C645-1314	Specification for Nonstructural Steel Framing Members	

IBC	

IRC							

C652-1315	Specification for Hollow Brick (Hollow Masonry Units Made from Clay or Shale)	

IBC	

IRC							

C685/C685M-11 14	Specification for Concrete Made by Volumetric Batching and Continuous Mixing	

IRC								

C726-12	Standard Specification for Mineral FiberWool Roof Insulation Board	
IBC								

C726-12	Standard Specification for Mineral Fiber Wool Roof Insulation Board	

IBC								

C728-05(2013) 15	Standard Specification for Perlite Thermal Insulation Board	

IBC	

IRC							
C744-1114	Specification for Prefaced Concrete and Calcium Silicate Masonry Units	
IBC	
IRC							

C754-1115	Specification for Installation of Steel Framing Members to Receive Screw-Attached Gypsum Panel Products	

IBC								

C836/C836M-1215	Specification for High Solids Content, Cold Liquid-Applied Elastomeric Waterproofing Membrane for Use with Separate Wearing Course	

IBC	

IRC							

C840-1113	Specification for Application and Finishing of Gypsum Board	

IBC								
C841-03(2008)e1 (2013)	Specification for Installation of Interior Lathing and Furring	
IBC								
C842-05(2010)e1 (2015)	Specification for Application of Interior Gypsum Plaster	
IBC								

C844-04(2010) 2015	Specification for Application of Gypsum Base to Receive Gypsum Veneer Plaster	

IBC	

IRC							

C847-1214A	Specification for Metal Lath	
IBC	
IRC							

C887-05(2010) 13	Specification for Packaged, Dry, Combined Materials for Surface Bonding Mortar	

IBC	

IRC							

C897-05(2009) 15	Specification for Aggregate for Job- Mixed Portland Cement-Based Plasters	

IBC	

IRC							

C920-1114A	Standard Specification for Elastomeric Joint Sealants	
IBC	
IRC							

C926-13 15B	
Specification for Application of Portland Cement-Based Plaster	

IBC	

IRC							

C933-1314	Specification for Welded Wire Lath	
IBC	
IRC							

C954-1115	Specification for Steel Drill Screws for the Application of Gypsum Panel Products or Metal Plaster Bases to Steel Studs from 0.033 inch (0.84 mm) to 0.112 inch (2.84 mm) in Thickness	

IBC	

IRC							

C955-11C15	Standard Specification for Load- bearing Transverse and Axial Steel Studs, Runners Tracks, and Bracing or Bridging, for Screw Application of Gypsum Panel Products and Metal Plaster Bases	

IBC	

IRC							

C956-04(2010) (2015)	Specification for Installation of Cast- in-Place Reinforced Gypsum Concrete	

IBC								

C957-10/C957M-15	Specification for High-Solids Content, Cold Liquid-Applied Elastomeric Waterproofing Membrane with Integral Wearing Surface	

IBC	

IRC							

C1002-0714	Specification for Steel Self Piercing TappingDrill Screws for the Application of Gypsum Panel Products or Metal Plaster Bases to Wood Studs or Steel Studs	

IBC	

IRC							

C1007-11a(2015)	Specification for Installation of Load Bearing (Transverse and Axial) Steel Studs and Related Accessories	

IBC								

C1029-1315	Specification for Spray-Applied Rigid Cellular Polyurethane Thermal Insulation	

IBC	

IRC							

C1032-06(2011) 14	Specification for Woven Wire Plaster Base	
IBC	
IRC							

C1047-10A2014a	Specification for Accessories for Gypsum Wallboard and Gypsum Veneer Base	

IBC	

IRC							

C1063-12D15a	Specification for Installation of Lathing and Furring to Receive Interior and Exterior Portland Cement-Based Plaster	

IBC	

IRC							

C1088-1314	Specification for Thin Veneer Brick Units Made From Clay or Shale	
IBC	
IRC							

C1107/C1107-1314A	Standard Specification for Packaged Dry, Hydraulic-Cement Grout (Nonshrink)	

IRC								

C1116/C1116M-10A(2015)	Standard Specification for Fiber - Reinforced Concrete and Shotcrete	

IRC								

C1173-10E1 (2014)	Specification for Flexible Transition Couplings for Underground Piping Systems	

IPC	
IPSDC	

IRC						

C1177/C1177M-0813	Specification for Glass Mat Gypsum Substrate for Use as Sheathing	
IBC	
IRC							

C1178/C1178M-1113	Specification for Coated Mat Water- Resistant Gypsum Backing Panel	

IBC	

IRC							
C1186-08(2012)	Specification for Flat Nonasbestos Fiber Cement Sheets	
IBC	
IRC							

C1261-1013	Specification for Firebox Brick for Residential Fireplaces	
IBC	
IRC							

C1277-1215	Specification for Shielded Couplings Joining Hubless Cast Iron Soil Pipe and Fittings	

IPC	

IPSDC	

IRC						

C1280-13A	Specification for Application of Exterior Gypsum Panel Products for Use as Sheathing	

IBC								

C1288-99(2010) 14	Standard Specification for Discrete Non-Asbestos Fiber-Cement Interior Substrate Sheets	

IBC	

IRC							

C1289—13E115	Standard Specification for Faced Rigid Cellular Polyisocyanurate Thermal Insulation Board	

IBC	

IRC							

C1313/C1313M-12 2013	Standard Specification for Sheet Radiant Barriers for Building Construction Applications	

IBC								

C1325-08b14	Standard Specification for Non- Asbestos Fiber-Mat Reinforced Cement Backer Units	

IBC	

IRC							

C1328/C1328M-12	Specification for Plastic (Stucco Cement)	
IBC	
IRC							

C1371-04a(2010)e115	Standard Test Method For Determination of Emittance of Materials Near Room Temperature Using Portable Emissometers	

IECC								

C1396/C1396M-13 2014A	Specification for Gypsum Ceiling Board	
IBC								

C1405-1215	Standard Specification for Glazed Brick (Single Fired, Solid Brick Units)	

IRC								

C1440-08(2013)	Specification for Thermoplastic Elastomeric (TPE) Gasket Materials for Drain, Waste, and Vent (DWV), Sewer, Sanitary and Storm Plumbing Systems	

IPC	

IPSDC	

IRC						

C1460-082012	Specification for Shielded Transition Couplings for Use with Dissimilar DWV Pipe and Fittings Above Ground	

IPC	

IPSDC	

IRC						

C1461-08(2013)	Specification for Mechanical Couplings Using Thermoplastic Elastomeric (TPE) Gaskets for Joining Drain, Waste, and Vent (DWV) Sewer, Sanitary, and Storm Plumbing Systems for Above and Below Ground Use	

IPC	

IPSDC	

IRC						

C1540-1115	Specfiication for Heavy Duty Shielded Couplings Joining Hubless Cast Iron Soil Pipe and Fittings	

IPC	

IRC							

C1549-09(2014)	Standard Test Method for Determination of Solar Reflectance Near Ambient Temperature Using a Portable Solar Reflectometer	

IECC-C								

C1563-2008(2013)	Standard Test Method for Gaskets for Use in Connection with Hub and Spigot Cast Iron Soil Pipe and Fittings for Sanitary Drain, Waste, Vent and Storm Piping	

IPC								

C1629/C1692M—1115	Standard Classification for Abuse- Resistant Nondecorated Interior Gypsum Panel Products and Fiber- Reinforced Cement Panels	

IBC								

C1634-1115	Standard Specification for Concrete Facing Brick	
IRC								

C1658/C1658-1213	Standard Specification for Glass Mat Gypsum Panels	
IBC	
IRC							

C1668-1213a	Standard Specification for Externally Applied Reflective Insulation systems on Rigid Duct in Heating, Ventilation, and Air Conditioning (HVAC) Systems	

IRC								

D41-05/D41M-2011	Specification for Asphalt Primer Used in Roofing, Dampproofing, and Waterproofing	

IBC	

IRC							

D43/D43M-2000(2006 12)E1	Specification for Coal Tar Primer Used in Roofing, Damproofing, and Waterproofing	

IBC	

IRC							

D56-05(2010)	Test Method for Flash Point by Tag Closed Cup Tester	
IBC	
IFC	
IMC						

D86-201215	Test Method for Distillation of Petroleum Products at Atmospheric Pressure	

IBC	

IFC							

D92-2012B	Test Method for Flash and Fire Points by Cleveland Open Cup Tester	

IFC								

D93-1215	Test Method for Flash Point by Pensky-Martens Closed Cup Tester	
IBC	
IFC	
IMC						

D312-00(2006)/D312M-15	Specification for Asphalt Used in Roofing	
IBC	
IRC							

D323-082015A	Test Method for Vapor Pressure of Petroleum Products (Reid Method)	
IFC								

D422-63(2007)E2	Test Method for Particle-Size Analysis of Soils	
IBC	
IRC							

D448-082012	Standard Classification for Sizes of Aggregate for Road and Bridge Construction	

IBC								

D449/D449M-03(200814)E1	Specification for Asphalt Used in Dampproofing and Waterproofing	

IRC								

D450D450M-07(2013)E1	Specification for Coal-Tar Pitch Used in Roofing, Dampproofing, and Waterproofing	

IBC	

IRC							

D635-1014	Test Method for Rate of Burning and/or Extent and Time of Burning of Self-Supporting Plastics in a Horizontal Position	

IBC								

D1003-11e113	Standard Test Method for Haze and Luminous Transmittance of Transparent Plastics	
IECC-C								

D1143/D1143M-07e1 (2013)	Test Methods for Deep Foundations Piles Under Static Axil Compressive Load	

IBC								

D1227-95(2007) 13	Specification for Emulsified Asphalt Used as a Protective Coating for Roofing	

IBC	

IRC							

D1253-0814	Standard Test Method for Residual Chlorine in Water	
IPC								

D1557-2012 E1	
Test Method for Laboratory Compaction Characteristics of Soil Using Modified Effort (56,000 ft- lb/ft3(2,700kN-m/m3))	

IBC								

D1593-0913	Non-rigid Vinyl Chloride Plastic Film and Sheeting	
ISPSC								

D1622/D1622M-08 14	Standard Test Method for Apparent Density of Rigid Cellular Plastics	
IRC								

D1693-201315	Test Method for Environmental Stress-Cracking of Ethylene Plastics	

IRC	

IMC							

D1785-1215	Specification for Poly (Vinyl Chloride) (PVC) Plastic Pipe, Schedules 40, 80 and 120	

IPC	

IMC	

IRC	
ISPSC					

D1869-95 (2010) 15	Specification for Rubber Rings for Asbestos Fiber-Reinforced Cement Pipe	

IPC	
IPSDC	

IRC						

D1929-16	Standard Test Method for Determining Ignition Temperature of Plastics	

IBC								

D1970/D1970M-132015A	Specification for Self-Adhering Polymer Modified Bituminous Sheet Materials Used as Steep Roof Underlayment for Ice Dam Protection	

IBC	

IRC							

D2126-0915	Standard Test Method for Response of Rigid Cellular Plastics to Thermal and Humid Aging	

IRC								

D2178/D2178M-04 15	Specification for Asphalt Glass Felt Used in Roofing and Waterproofing	
IBC	
IRC							

D2241-0915	Specification for Poly (Vinyl Chloride) (PVC) Pressure-Rated Pipe (SDR-Series)	

IPC	

IRC	

IMC	
ISPSC					

D2464-0615	Specification for Threaded Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 80	

IPC	

IRC	
ISPSC	

IMC					

D2466-0615	Specification for Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 40	

IPC	

IRC	

IMC	
ISPSC					

D2467-0615	Specification for Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 80	

IPC	

IRC	

IMC	
ISPSC					

D2513-20134E1	Specification for Polyethylene (PE) Thermoplastic Gas Pressure Pipe, Tubing, and Fittings	

IRC	

IMC	

IFGC						

D2559-12A	Standard Specification for Adhesives for Bonded StructuralLaminated Wood Products for Use under Exterior (West Use) Exposure Conditions	

IRC								

D2609-02(2008)15	Specification for Plastic Insert Fittings for Polyethylene (PE) Plastic Pipe	

IPC	

IRC							

D2626/D2626M-04(2012)E1	Specification for Asphalt-Saturated and Coated Organic Felt Base Sheet Used in Roofing	

IBC	

IRC							

D2661-1114	Specification for Acrylonitrile- Butadiene-Styrene (ABS) Schedule 40 Plastic Drain, Waste, and Vent Pipe and Fittings	

IPC	

IPSDC	

IRC						

D2665-1214	Specification for Poly (Vinyl Chloride) (PVC) Plastic Drain, Waste, and Vent Pipe and Fittings	

IPC	
IPSDC	

IRC						

D2672-96a(2009)14	Specification for Joints for IPS PVC Pipe Using Solvent Cement	
IPC	
IRC	
IMC						

D2683-10E114	Standard Specification for Socket- Type Polyethylene Fittings for Outside Diameter Controlled Polyethylene Pipe and Tubing	

IPC								

D2683-2010E114	Specification for Socket- Type Polyethylene Fittings for Outside Diameter-Controlled
Polyethylene Pipe and Tubing	

IPC	

IRC	

IMC						

D2824/D2824M-06(2012)E1 2013	Specification for Aluminum- Pigmented Asphalt Roof Coatings, Non-fibered, Asbestos Fibered, and Fibered without Asbestos	

IRC	

IBC							

D2837-11 2013E1	Test Method for Obtaining Hydrostatic Design Basis for Thermoplastic Pipe Materials or Pressure Design Basis for Thermoplastic Pipe Products	

IRC	

IMC							

D2843-1016	Standard Test Method for Density of Smoke from the Burning of Decomposition of Plastics	

IBC								

D2846/D2846M-09BE1 14	Specification for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Hot- and Cold-Water Distribution Systems	

IPC	

IRC	

IMC	

ISPSC					

D2859-06(2011)15	Standard Test Method for Ignition Characteristics of Finished Textile Floor Coverings Materials	

IBC	

IFC							

D2996-01(2007)e0115	Specification for Filament-Wound Fiberglass (Glass Fiber Reinforced Thermosetting Resin) Pipe	

IMC								

D3034-0814a	Specification for Type PSM Poly (Vinyl Chloride) (PVC) Sewer Pipe and Fittings	

IPC	

IRC	

IMC						

D3035-2012E115	Specification for Polyethylene (PE) Plastic Pipe (DR-PR) Based on Controlled Outside Diameter	

IPC	

IRC	

IMC						

D3161/D3161M-201315	Test Method for a Wind-Resistance of Asphalt Shingles Steep Slope Roofing Products (Fan Induced Method)	

IBC	

IRC							

D3201/D3201M-2013	Test Method for Hygoscopic Properties of Fire-Retardant Wood and Wood-Based Products	

IBC	

IRC	
IWUIC						

D3212-07(2013)	Specification for Joints for Drain and Sewer Plastic Pipes Using Flexible Elastomeric Seals	

IPC	

IRC	
IUWIC						

D3261-12E1	Specification for Butt Heat Fusion Polyethylene (PE) Plastic Fittings for Polyethylene (PE) Plastic Pipe and Tubings	

IMC	

IPC							

D3350-12E114	Specification for Polyethylene Plastics Pipe and Fittings Materials	
IRC	
IMC							

D3468/D3468-99(2006)e01(2013)E1*	Specification for Liquid-Applied Neoprene and Chlorosulfonated Polyethylene Used in Roofing and Waterproofing	

IBC	

IRC							

D3679-1113	Specification for Rigid Poly (Vinyl Chloride) (PVC) Siding	
IBC	
IRC							

D3689/D3698M-2007 (2013)E1	Test Methods for Deep Foundations Piles Under Static Axial Tensile Load	

IBC								

D3909/D3909M-97b(2012)e114	Specification for Asphalt Roll Roofing (Glass Felt) Surfaced with Mineral Granules	

IBC	

IRC	
IWUIC						

D4068-0915	Specification for Chlorinated Polyethylene (CPE) Sheeting for Concealed Water-Containment Membrane	

IPC	

IRC							

D4272-0915	Test Method for Total Energy Impact of Plastic Films by Dart Drop	
IBC								

D4318-10E1	Test Method for Liquid Limit, Plastic Limit, and Plasticity Index of Soils	
IBC	
IRC							

D4637/D4637M-201314E1	Specification for EPDM Sheet Used in Single-Ply Roof Membrane	
IBC	
IRC							

D4869/D4869M-05(2011)e0115	Specification for Asphalt-Saturated (Organic Felt) Underlayment Used in Steep Slope Roofing	

IBC	

IRC							

D4945-12	Test Method for High-Strain Dynamic Testing of Piles Deep Foundations	

IBC								

D4990-1997a(2005)e01(2013)	Specification for Coal Tar Glass Felt Used in Roofing and Waterproofing	
IBC	
IRC							

D5055-201313E1	Specification for Establishing and Monitoring Structural Capacities of Prefabricated Wood I-Joists	

IBC	

IRC							

D5456-201314B	Standard Specification for Evaluation of Structural Composite Lumber Products	

IBC	

IRC							

D5665/D5665M-99a(2006)2014E1	Specification for Thermoplastic Fabrics Used in Cold-Applied Roofing and Waterproofing	

IBC	

IRC							

D5726-98(2005) (2013)	Specification for Thermoplastic Fabrics Used in Hot-Applied Roofing and Waterproofing	

IBC	

IRC							

D6162/D6162M-2000a(2008) (2015)E1	Specification for Styrene Butadiene Styrene (SBS) Modified Bituminous Sheet Materials Using a Combination of Polyester and Glass Fiber Reinforcements	

IBC	

IRC							

D6162/D6162M-2000a(2008) A(2015)E1	Specification for Styrene Butadiene Styrene (SBS) Modified Bituminous Sheet Materials Using a Combination of Polyester and Glass Fiber Reinforcements	

IBC	

IRC							

D6163/D6163M-2000(2008) (2015)E1	Specification for Styrene Butadiene Styrene (SBS) Modified Bituminous Sheet Materials Using Glass Fiber Reinforcements	

IBC	

IRC							

D6223/D6223M-02(2011)E1 (2009) E1	Specification for Atactic Polypropylene (APP) Modified Bituminous Sheet Materials Using a Combination of Polyester and Glass Fiber Reinforcements	

IBC	

IRC							

D6298-05e113	Specification for Fiberglass Reinforced Styrene-Butadiene- Styrene (SBS) Modified Bituminous Sheets with a Factory Applied Metal Surface	

IBC	

IRC							

D6305-08(2015)E1	Practice for Calculating Bending Strength Design Adjustment Factors for Fire-Retardant-Treated Plywood Roof Sheathing	

IBC	

IRC							

D6380/D6380-03(2009)(2013)E1	Standard Specification for Asphalt Roll Roofing (Organic) Felt	

IBC	

IRC							

D6509/D6509M—09(2015)	Standard Specification for Atactic Polypropylene (APP) Modified Bituminous Base Sheet Materials Using Glass Fiber Reinforcements	

IBC								

D6694/D6694M-08(2013)E1	Standard Specification for Liquid- applied Silicone Coating Used In Spray Polyurethane Foam Roofing Systems	

IBC	

IRC							

D6757-2013	Standard Specification for Inorganic Underlayment Felt Containing Inorganic Fibers used in Steep- Slope Roofing Products	

IBC	

IRC							

D6878/D6878-11A13	Standard Specification for Thermoplastic Polyolefin Based Sheet Roofing	

IBC	

IRC							

D6947/D6947M-07(2013)E1	Standard Specification for Liquid Applied Moisture Cured Polyurethane Coating Used in Spray Polyurethane Foam Roofing System	

IBC	

IRC							

D7032-10A14	Standard Specification for Establishing Performance Ratings for Wood-Plastic Composite Deck Boards and Guardrail Systems (Guards or Handrails)	

IRC	

IWUIC	

IBC						

D7147-0511	Specification for Testing and Establishing Allowable Loads of Joist Hangers	

IBC								

D 7158/D7158M-11	Standard Test Method for Wind Resistance of Sealed Asphalt Shingles (Uplift Force/Uplift Resistance Method)	

IBC	

IRC							

D7254—0715	Standard Specification for Polypropylene (PP) Siding	
IBC	
IRC							

D7425/D7425M-1113	Standard Specification for Spray Polyurethane Foam Used for Roofing Application	

IRC								

D7655/D7655M-12	Standard Classification for Size of Aggregrate Used as Ballast for Roof Membrane Systems	

IBC								

D7672-201214	Standard Specification for Evaluating Structural Capacities of Rim Board Products and Assemblies	

IBC	

IRC							

E84-2013A2015A	Test Method for Surface Burning Characteristics of Building Materials	
IBC	
IRC	
IFC						

E84-2015B	Standard Test Method for Surface Burning Characteristics of Building Materials	

IBC	

IRC	

IFC	

IMC	

IEBC				

E96/E96M-201315	Test Method for Water Vapor Transmission of Materials	
IBC	
IRC							

E119-2016	Standard Test Methods for Fire Tests of Building Construction and Materials	

IBC	

IRC	

IMC	
IWUIC					

E136-1216	Standard Test Method for Behavior of Materials in a Vertical Tube Furnace at 750 degrees C	

IBC	

IRC	

IMC	
IWUIC	

IFGC				

E283-04(2012)	Test Method for Determining the Rate of Air Leakage Through Exterior Windows, Curtain Walls, and Doors under Specified Pressure Differences Across the Specimen	

IRC	

IECC	

IBC						

E330/E330M-0214	Test Method for Structural Performance of Exterior Windows, Doors, Skylights and Curtain Walls by Uniform Static Air Pressure Difference	

IBC	

IRC							

E408-71(2008)13	Test Methods for Total Normal Emittance of Surfaces Using Inspection-Meter Techniques	
IECC-C								

E408-71(2008)13	Test Methods for Total Normal Emittance of Surfaces Using Inspection-Meter Techniques	
IECC-C								

E488/E488M-1015	Test Method for Strength of Anchors in Concrete and Masonry Elements	
IEBC								

E605/E605M-1993(2011) (2015)E1	Test Method for Thickness and Density of Sprayed Fire-Resistive Material (SFRM) Applied to Structural Members	

IBC								

E681-09(2015)	Test Method for Concentration Limits of Flammability of Chemicals (Vapors and Gases)	

IBC	

IFC							

E736/E736M-00(2011) (2015)E1	Test Method for Cohesion/Adhesion of Sprayed Fire-Resistive Materials Applied to Structural Members	

IBC								

E814-2013A	Standard Test Method of Fire Tests of Penetration Firestop Systems	
IBC	
IRC	
IMC						

E903-9612	Standard Test Method Solar Absorptance, Reflectance and transmittance of Materials Using Integrating Spheres (Withdrawn 2005)	

IECC-C								

E970-201014	Test Method for Critical Radiant Flux of Exposed Attic Floor Insulation Using a Radiant Heat Energy Source	

IBC	

IRC							

E1354-20132016	Standard Test Method for Heat and Visible Smoke Release Rates for Materials and Products Using an Oxygen Consumption Colorimeter	

IBC	

IFC							

E1529-14a	Standard Test Method for Determining Effects of Large Hydrocarbon Pool Fires on Structural Members and Assemblies	

IFC								

E1537-20132015	Standard Test Method for Fire Testing of Upholstered Furniture	
IFC								

E1602-0203(2010)E1	Guide for Construction of Solid Fuel- Burning Masonry Heaters	
IBC	
IRC							

E1677-11	Standard Specification for an Air Retarder (AR) Barrier (AB) Material or Systems for Low-Rise Framed Building Walls	

IECC-C								

E1886-0513A	Test Method for Performance of Exterior Windows, Curtain Walls, Doors and Storm Shutters Impact Protective Systems Impacted by Missiles and Exposed to Cyclic Pressure Differentials	

IBC	

IRC							

E1918-06(2015)	Standard Test Method for Measuring Solar Reflectance of Horizontal and Low-sloped Surfaces in the Field	

IECC-C								

E1966-2015	Standard Test Method for Fire resistant Joint Systems	
IBC	
IFC							

E1996-2012A2014a	Specification for Performance of Exterior Windows, Glazed Curtain Walls, Doors and Impact Protective Systems Impacted by Winborne Debris in Hurricanes	

IBC	

IRC							

E2072-1014	Standard Specification for Photolumiscent (Phosphorescent) Safety Markings	

IBC	

IFC							

E2174-10E1 14B	Standard Practice for On-Site Inspection of Installed Fire Stops	
IBC								

E2231-09 15	Standard Practice for Specimen Preparation and Mounting of Pipe and Duct Insulation Materials to Assess to Surface Burning Characteristics	

IRC	

IMC							

E2307-2010 15B	Standard Test Method for Determining Fire Resistance of Perimeter Joint System Between an Exterior Wall Assembly and Floor AssemblyFire Barriers Using the Intermediate-Scale, Multi-Story Test Apparatus	

IBC								

E2336-2016	Standard Test Methods for Fire Resistive Grease Duct Enclosure Systems	

IMC								

E2357-11	Standard Test Method for Determining Air Leakage Rate of Air Barrier Assemblies	
IECC-C								

E2392/E2392M-10E1	Standard Guide for Design of Earthen Wall Building Systems	
IRC								

E2393-10A a(2015)	Standard Practice for On-Site Inspection of Installed Fire Resistive Joint Systems and Perimeter Fire Barrier	

IBC								

E2397/E2397M-11 2015	Standard Practice for Determination of Dead Loads and Live Loads Associated with Vegatative Green Roof Systems	

IBC								

E2404-15a	Standard Practice for Specimen Preparation and Mounting of Textile, Paper or Polymeric (Including Vinyl) and Wood Wall or Ceiling Coverings, Facing and Veneers to Assess Surface Burning Characteristics	

IBC	

IFC							

E2556/E2556M-10	Standard Specification for Vapor Permeable Flexible Sheet Water- Resistive Barriers Intended for Mechanical Attachment	

IBC								

E2570/E2570—07(2014)E1	Standard Test Method for Evaluating Water-Resistive Barrier (WRB) Coatings Used Under Exterior Insulation and Finish Systems (EIFS) for EIFS with Drainage	

IBC	

IRC							

E2599-15	Standard Practice for Specimen Preparation and Mounting of Reflective Insulation Radiant Barrier and Vinyl Stretch Ceiling Materials for Building Applications to Assess Surface Burning Characteristics	

IBC								

E2634-11(2015)	Standard Specification for Flat Wall Insulating Concrete Form (ICF) Systems	

IBC	

IRC							

E2727-10E1	Standard Practice for Assessment of Rainwater Quality	
IPC								

E2751/E2751M-11 13	Standard Practice for Design and Performance of Supported Laminated Glass Walkways	

IBC								

F437-0915	Specification for Threaded Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings, Schedule 80	

IPC	

IRC	

ISPSC	

IMC					

F438-0915	Specification for Socket-Type Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings, Schedule 40	

IPC	

IRC	

IMC	

ISPSC					

F439-1213	Specification for Socket-Type Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings, Schedule 80	

IPC	

IRC	

IMC	

ISPSC					

F441/F441M-1315	Specification for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe, Schedules 40 and 80	

IPC	

IRC	

IMC						

F442/F442M-13E1	Specification for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe (SDR-PR)	

IPC	

IRC	

IMC						

F447-1014	Specification for Elastomeric Seals (Gaskets) for Joining Plastic Pipe	
IPC	IPSDC	
IRC						

F493-1014	Specification for Solvent Cements for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe and Fittings	

IPC	

IRC	

IMC						

F628-0812E1	Specification for Acrylonitrile- Butadiene-Styrene (ABS) Schedule 40 Plastic Drain, Waste, and Vent Pipe with a Cellular Core	

IPC	

IPSDC	

IRC						

F656-1015	Specification for Primers for Use in Solvent Cement Joints of Poly (Vinyl Chloride) (PVC) Plastic Pipe and Fittings	

IPC	

IPSDC	

IRC						

F876-201315A	Specification for Crosslinked Polyethylene (PEX) Tubing	
IPC	
IRC	
IMC						

F877-2011A	Specification for Crosslinked Polyethylene (PEX) Plastic Hot- and Cold-Water Distribution Systems	

IPC	

IRC	

IMC						

F1085-1014	Standard Specification for Mattress and Box Springs Use in Berths in Marine Vessels	

IFC								

F1085-1014	Standard Specification for Mattress and Box Springs Use in Berths in Marine Vessels	

IFC								

F1476-07(2013)	Standard Specification for Performance of Gasketed Mechanical Couplings for Use in Piping Applications	

IMC	

IPC							

F1488-09E114	Specification for Coextruded Composite Pipe	
IPC	IPSDC	
IRC						

F1548-01(2006)(2012)	Standard Specification for the Performance of Fittings for Use with Gasketed Mechanical Couplings Used In Piping Applications	

IPC								

F1554-07a15	Specification for Anchor Bolts, Steel 36, 55 and 105 ksi Yield Strength	
IRC								

F1667-11E115	Specification for Driven Fasteners: Nails, Spikes, and Staples	
IBc	
IRC							

F1807-201315	Specifications for Metal Insert Fittings Utilizing a Copper Crimp Ring for SDR9 Cross-linked Polyethylene (PEX) Tubing and SDR9 Polyethylene of Raised Temperature (PE-RT) Tubing	

IPC	

IRC	

IMC						

F1866-0713	Specification for Poly (Vinyl Chloride) (PVC) Plastic Schedule 40 Draniage and DWV Fabricated Fittings	

IPC	

IRC							

F1960-1215	Specification for Cold Expansion Fittings with PEX Reinforcing Rings for Use with Cross-linked Polyethylene (PEX) Tubing	

IPC	

IRC							

F1970-12E1	Special Engineered Fittings, Appurtenances or Valves for use in Poly (Vinyl Chloride) (PVC) or Chlorinated Poly (Vinyl Chloride) (CPVC) Systems	

IPC	

IRC							

F1973-0813E1	Standard Specification for Factory Assembled Anodeless Risers and Transition Fittings in Polyethylene (PE) and Polyamide 11 (PA11) and Polyamide 12 (PA12) Fuel Gas Distribution Systems	

IRC	

IFGC							

F1974-09(2015)	Specification for Metal Insert Fittings for Polyethylene/Aluminum/Polyethylene and Crosslinked Polyethylene/Aluminum/Crosslinked Polyethylene Composite Pressure Pipe	

IPC	

IRC	

IMC						

F2080-1215	Specification for Cold-Expansion Fittings with Metal Compression- Sleeves for Cross-linked Polyethylene (PEX) Pipe	

IPC	

IRC							

F2090-1013	Specification for Window Fall Prevention Devices with Emergency Escape (Egress) Release Mechanisms	

IBC	

IRC	

IFC	

IEBC					

F2098-08	Standard Specification for Stainless Steel Clamps for Securing SDR9 Cross-Linked Polyethylene (PEX) Tubing to Metal Insert and Plastic Insert Fittings	

IPC	

IRC							

F2158-08(2013)	Standard Specification for Residential Central-Vacuum Tubes and Fittings	

IRC								

F2159-1114	Specification for Plastic Insert Fittings Utilizing a Copper Crimp Ring for SDR9 Cross-linked Polyethylene (PEX) Tubing and SDR9 Polyethylene of Raised Temperature (PE-RT) Tubing	

IPC	

IRC	

IMC						

F2200-1314	Standard Specification for Automated Vehicular Gate Construction	

IFC								

F2200-13 14	Standard Specification for Automated Vehicular Gate Construction	

IBC								

F2306/F2306M-201314E1	Specification for 12" to 60" 300 to 1500 mm annular Corrugated Profile-Wall Polyethylene (PE) Pipe and Fittings for Gravity-Flow Storm Sewer and Subsurface Drainage Applications	

IPC	

IRC	

IMC						

F2389-1015	Specification for Pressure-Rated Polypropylene (PP) Piping Systems	
IPC	
IRC	
IMC						

F2434-0914	Standard Specification for Metal Insert Fittings Utilizing a Copper Crimp ring for SDR9 Cross-Linked Polyethylene (PEX) Tubing and SDR9 Cross-Linked Polyethylene/Aluminum/Cross- Linked Polyethylene (PEX-AL-PEX) Tubing	

IPC	

IRC	

IMC						

F2623-0814	Standard Specification for Polyethylene of Raised Temperature (PE-RT) SDR 9 Tubing	

IMC	

IRC							

F2735-09	Standard Specification for SDR9 Cross-linked Polyethylene (PEX) and Polyethylene of Raised Temperature (PE-RT) Tubing	

IMC	

IPC	

IRC						

F2769-1014	Polyethylene or Raised Temperature (PE-RT) Plastic Hot and Cold-Water Tubing and Distribution Systems	

IMC	

IPC	

IRC						

F2806-10(2015)	Standard Specification for Acrylonitrile-Butadiene-Styrene (ABS) Plastic Pipe (Metric SDR-PR)	

IMC	

IRC							

F2831-1112	Standard Practice for Internal Non Structural Epoxy Barrier Coating Material Used in Rehabilitation of Metallic Pressurized Piping Systems	

IPC								

F2855-12	Standard Specification for Chlorinated Poly (Vinyl Chloride)/Aluminum/Chlorinated Poly (Vinyl Chloride) (CPVC AL CPVC) Composite PressureTubing	

IRC								

G152-0613	Practice for Operating Open Flame Carbon Arc Light Apparatus for Exposure of Nonmetallic Materials	

IBC								

G154-0612a	Practice for Operating Fluorescent Light Apparatus for UV Exposure of Nonmetallic Materials	

IBC								

G155-05a13	Practice for Operating Xenon Arc Light Apparatus for Exposure of Non-Metallic Materials	

IBC								
AWC	American Wood Council	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/AWC SDPWS-2015	Special Design Provisions for Wind and Seismic	
IBC								

ANSI/AWC WFCM-20152018	Wood Frame Construction Manual for One- and Two-Family Dwellings	
IBC	
IRC							

ANSI/AWSC NDS-20152018	National Design Specification (NDS) for Wood Construction - with 20152018 Supplement	

IBC	

IRC							
AWCI	The Association of the Wall & Ceiling Industries International	
Standard Reference Number	Title	Referenced in Code(s):	

12-B-0414	Technical Manual 12-B Standard Practice for the Testing and Inspection of Field Applied Thin Film Intumescent Fire-Resistive Materials; an Annotated Guide, Second Third Edition	

IBC								
AWPA	American Wood Protection Association	
Standard Reference Number	Title	Referenced in Code(s):	

M4-16	Standard for the Care of Preservative-Treated Wood Products	

IBC	

IRC							

U1-16	USE CATEGORY SYSTEM: User
Specification for Treated Wood except Section 6, Commodity Specification H	

IBC	

IRC							
AWS	American Welding Society	
Standard Reference Number	Title	Referenced in Code(s):	

D1.4/D1.4M-20112017	Structural Welding Code- Reinforcing Steel Including Metal Inserts and Connections in Reinforced Concrete Construction	

IBC								
AWWA	American Water Works Association	
Standard Reference Number	Title	Referenced in Code(s):	

C104/A21.4-0813	Cement-Mortar Lining for Ductile- Iron Pipe and Fittings for Water	
IRC	
IPC							

C507-1115	Standard for Ball Valves, 6 In. Through 60 In. (150mm Through 1,500mm)	

IPC	

IRC							
C651-0514	Disinfecting Water Mains	IPC								

C901-0816	Polyethylene (PE) Pressure Pipe and Tubing, 1/2 3/4 in. (13 19mm) through 3 in. (76mm) for Water Service	

IMC	

IPC	

IRC						

C903-0516	Polyethylene-Aluminum- Polyethylene (PE-AL-PE)& Crosslinked Polyethylene Composite Pressure Pipe (12mm) (1/2)
in through (50 51mm) (2 in) for Water Servi	

IRC								

C904-0816	Cross-Linked Polyethylene (PEX) Pressure Pipe Tubing 1/2 in. (1213mm) Through 3 In. (76mm) for Water Service	

IPC	

IRC							

D100-0511	Standard for Welded Carbon Steel Tanks for Water Storage	
IPC								

D115-0616	Standard for Tendon Prestressed- Concrete Water Tanks	
IPC								
BSI	British Standards Institution	

Standard Reference Number	Title	Referenced in Code(s):	

BS EN 459-2010 2015	Part 1 Building Lime, Definitions and Conformity Criteria, Part 2 Test Methods	

IRC								
CEN	European Committee for Standardization	
Standard Reference Number	Title	Referenced in Code(s):	

EN 1081: 1998	Resilient Floor Coverings - Determination of the Electrical Resistance	

IBC	

IFC							
CGA	Compressed Gas Association	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/G13-0613(2015)	Storage and Handling of Silane and Silane Mixtures (an American National Standard)	

IFC								

ANSI/P-18 (2006) (2013)	Standard for Bulk Inert Gas Systems (an American National Standard)	
IFC								

C-7 (2011)(2014)	Guide to Classification
and Preparation of Precautionary Labeling and Marking of Compressed Gas Containers Gases	

IFC								

P-1 (2000)(2015)	Standard for Safe Handling of Compressed Gases in Containers	
IFC								

S-1.1 (2011)(2017)	Pressure Relief Device Standards - Part 1 Cylinders for Compressed Gases	

IFC	

IFGC							

S-1.2 (2009)	Pressure Relief Device Standards - Part 2 - Cargo and Portable Tanks for Compressed Gases	

IFC	

IFGC							

S-1.3 (2008) (2016)	Pressure Relief Device Standards- Part 3 - Stationary Storage Containers for Compressed Gases	

IFC	

IFGC							

V-1-(2005)(2013)	Standard for Compressed Gas Cylinder Valve Outlet and Inlet Connections	

IFC								
CISPI	Cast Iron Soil Pipe Institute	
Standard Reference Number	Title	Referenced in Code(s):	

301-04a12	Specification for Hubless Cast Iron Soil Pipe and Fittings for Sanitary and Storm Drain, Waste and Vent Pipings Applications	

IRC	

IPC	

IPSDC						

310-0412	Specification for Coupling for Use in Connection with Hubless Cast Iron Soil Pipe and Fittings for Sanitary and Storm Drain, Waste, and Vent Piping Applications	

IRC	

IPC	

IPSDC						
CPA	Composite Panel Association	
Standard Reference Number	Title	Referenced in Code(s):	
A208.1-092016	Particleboard	IBC								
CRRC	Cool Roof Rating Council	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/CRRC-1- S100- 2012 2016	CRRC-1 Standard Test Methods for Determining Radiative Properties of Materials	
IECC-C								

A112.18.1-2012 2017/CSA B125.1-201217	
Plumbing Supply Fittings	
IPC	
IRC							
A112.18.2-20112015/CSA B125.2-20112015	
Plumbing Waste Fittings	
IRC	
IPC							
A112.18.6-2017/CSA B125.6-200917	Flexible Water Connectors	IRC								

A257.3M-200914	Joints for Circular Concrete Sewer and Culvert Pipe, Manhole Sections and Fittings Using Rubber Gaskets	

IRC								

AAMA/WDMA/CSA 101/1.S.2/A440-1116	North American Fenestration Standard/Specifications for Windows, Doors and Unit Skylights	

IBC	

IECC	

IRC						

ASME/A17.1/CSA B44-20132016	Safety Code for Elevators and Escalators	
IRC								
ASME A112.3.4-2013/CSA B 45.9-99 (R2013) 13	
Macerating Systems and Related Components	

IPC	

IRC							
ASME
A112.19.5-20112017/CSA/B45.15-201117	Flush Valves and Spuds Water Closets, Urinals and Tanks	
IRC	
IPC							
ASME A112.19.7-20122017/CSA B45.10-201217	
Hydromassage Bathtubs Systems	
IPC								

ASSE 1016-2017/ASME 112.1016-2017/ CSA B125.16-20112017	Performance Requirements for Automatic Compensating Valves for Individual Showers and Tub/Shower Combinations	

IRC								

B64.1.1-1116	Vacuum Breakers, Atmospheric Type (AVB)	
IRC	
IPC							
B64.1.2-1116	Pressure Vacuum Breakers (PVB)	IRC	IPC							

B64.1.3-11 16	Spill Resistant Pressure Vacuum Breakers (SRPVB)	
IPC	
IRC							

B64.1.3-1116	Spill Resistant Pressure Vacuum Breakers (SRPVB)	
IPC	
IRC							

B64.2-07 16	Hose connection vacuum breakers (HCVB)	
IRC	
IPC							

B64.2-1116	Vacuum Breakers, Hose Connection Type (HCVP)	
IRC	
IPC							

B64.2.1-1116	Vacuum Breakers, Hose Connection (HCVB) with Manual Draining Feature	

IRC	

IPC							

B64.2.2-0716	Hose Connection Vacuum Breakers (HCVB) with Automatic Draining Feature	

IRC	

IPC							

B64.6-1116	Dual Check Valve Backflow Preventers (DuC)	
IPC	
IRC							

B64.10.1-0711	Manual for the Maintenance and Field Testing of Backflow Prevention Devices	

IPC								

B137.1-1316	Polyethylene (PE) Pipe, Tubing and Fittings for Cold Water Pressure Services	

IRC	

IPC	

IMC						

B137.2-1316	Polyvinylchloride PVC Injection- Moulded Gasketed Fittings for Pressure Applications	

IRC	

IPC	
ISPSC	

IMC					

B137.3-1316	Rigid Poly (Vinyl Chloride) (PVC) Pipe for Pressure Applications	
IRC	
IPC	IPSDC	ISPSC	
IMC				

B137.10M-1316	Cross-linked Polyethylene/Aluminum/Cross-linked Polyethylene (PEX-AL-PEX) Composite Pressure-Pipe Systems	

IRC	

IPC	

IMC						

B137.11-1316	Polypropylene (PP-R) Pipe and Fittings for Pressure Applications	
IRC	
IPC							

B181.1-11 15	Acrylonitrile-butadiene-styrene (ABS) Drain, Waste, and Vent Pipe and Pipe Fittings	

IRC	

IPC	
IPSDC						

B181.2-1115	Polyvinylchloride PVC Drain, and chlorinated polyvinylchloride (CPVC) Drain, Waste, and Vent Pipe and Pipe Fittings	

IRC	

IPC	

IPSDC						

B181.3-1115	Polyolefin and polyvinylidene (PVDF) Laboratory Drainage Systems	

IRC	

IPC							

B182.4-1115	
Profile PVC Sewer Pipe and Fittings	
IRC	
IPC	IPSDC						

B182.6-1115	Profile Polyethylene (PE) Sewer Pipe and Fittings for leak proof sewer applications	

IRC	

IPC							

B182.8-1115	Profile Polyethylene (PE) Storm Sewer and Drainage Pipe and Fittings	

IRC	

IPC							
B483.1-07(R2012)	Drinking Water Treatment Systems	IRC								

B602-1015	Mechanical Couplings for Drain, Waste, and Vent Pipe and Sewer Pipe	

IRC	

IPC							

C22.2 No. 108-01 (R2010)14	
Liquid pumps	
ISPSC								

CAN/CSA A257.1M-2009 14	Non-reinforced circular concrete culvert, storm drain, sewer pipe and fittings	

IRC	

IPC	
IPSDC						

CAN/CSA A257.2M-2009 14	Reinforced circular concrete culvert, storm drain, sewer pipe, and fittings	

IRC	

IPC	
IPSDC						

CAN/CSA C448 Series-02-CSA-2002 16	Design and installation of earth energy systems-First Edition; Update 2: October 2009; Consolidated Reprint 10/2009	

IRC	

IMC							
CSA 0O325-07	Construction Sheathing	IRC								

CSA 8-93	Requirements for Gas-Fired Log Lighters for Wood Burning Fireplaces with Revisions through January 1999	

IRC	

IFGC							
CSA B45.5-1117/IAPMO Z124-20112017	Plastic Plumbing Fixtures	IRC	IPC							

CSA B55.1-20122015	Test Method for measuring efficiency and pressure loss of drain water heat recovery units	

IECC								
CSA B55.2-20122015	Drain water heat recovery units	IECC								

CSA B64.2-0716	Hose connection vacuum breakers (HCVB)	
IRC	
IPC							

CSA B64.2.1.1-1116	Hose Connection Dual Check Vacuum Breakers (HCDVB)	
IRC	
IPC							

CSA B64.2.2-0716	Hose Connection Vacuum Breakers (HCVB) with Automatic Draining Feature	

IRC	

IPC							

CSA B64.2.2-11 16	Vacuum Breakers, Hose Connection Type (HCVP) with Automatic Draining Feature	

IRC	

IPC							

CSA B64.3-1116	Dual Check Valve Backflow Preventers Atmospheric Port (DCAP)	

IRC	

IPC							

CSA B64.4-1116	Backflow Preventers, Reduced Pressure Principle (RP)	
IRC	
IPC							

CSA B64.4.1-1116	Reduced Pressure Principle for Fire Sprinklers (RPF)	
IRC	
IPC							

CSA B64.5-1116	Double Check Backflow Preventers (DCVA)	
IRC	
IPC							

CSA B64.5.1-1116	Double Check Valve Backflow Preventers Type for Fire Systems (DCVAF)	

IRC	

IPC							

CSA B64.7-1116	Laboratory Facet Vacuum Breakers (LFVB)	
IRC	
IPC							

CSA B137.5- 1316	Cross-Linked Polyethylene (PEX) Tubing Systems for Pressure Applications	

IRC	

IPC	

IMC						

CSA B137.6- 1316	Chlorinated Polyvinylchloride CPVC Pipe, Tubing and Fittings for Hot and Cold Water Distribution Systems	

IRC	

IPC	

ISPSC	

IMC					

CSA B137.9-1316	Polyethylene/Aluminum/Polyethylene (PE-AL-PE) Composite Pressure- Pipe Systems	

IRC	

IMC							

CSA C22.2 No. 218.1-M89(R2011)13	Spas, hot tubs and associated equipment	
ISPSC	
IMC							
CSA C22.2 No. 236-201115	Heating and cooling equipment	ISPSC	IMC							

UL/CAN/CSA/ANCE C22.2 NO. 60335-2- 40-2012	Standard for Safety of Household and Similar Electrical Appliances, Part 2 -40: Particular Requirements for Motor Compressors electrical heat pumps, air-conditioners and dehumidifiers	

IRC								
Z21.50/CSA 2.22-20122016	Vented Gas Fireplace Heaters	IRC	IFGC							
Z21.56a/CSA 4.7-20132017	Gas-Fired Pool Heaters	ISPSC								
Z21.88/CSA 2.33-152016	Vented Gas Fireplace Heaters	IRC	IFGC							
DASMA	Doors and Access Systems Manufacturers Association International	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/DASMA 105-20122016	Test Method for Thermal Transmittance and Air Infiltration of Garage Doors and Rolling Doors	

IECC								

ANSI/DASMA 107-1997 (R2012)2017	Room Fire Test Standard for Garage Doors Using Foam Plastic Insulation	
IBC								

ANSI/DASMA 108-20122017	Standard Method for Testing Sectional Garage Doors, and Rolling Doors and Flexible Doors: Determination of Structural Performance Under Uniform Static Air Pressure Difference	

IBC	

IRC							

ANSI/DASMA 115-20122016	Standard Method for Testing Sectional Garage Doors,and Rolling Doors and Flexible Doors: Determination of Structural Performance Under Missile Impact and Cyclic Wind Pressure	

IBC	

IRC							
DOC	United States Department of Commerce	
Standard Reference Number	Title	Referenced in Code(s):	

16 CFR Part 1632 (2009)(2015)	Standard for the Flammability of Mattress and Mattress Pads (FF 4- 72, Amended)	

IFC								

DOE	U.S. Department of Energy	
Standard Reference Number	Title	Referenced in Code(s):	

10 CFR, Part 430-19982015	Energy Conservation Program for Consumer Products: Test Procedures and Certification and Enforcement Requirement for Plumbing Products; and Certification and Enforcement Requirements for Residential Appliances; Final Rule	

IECC-C								

10 CFR Part 430, Subpart B, Appendix N (1998)(2015)	Uniform Test Method for Measuring the Energy Consumption of Furnaces and Boilers	
IECC-C								

10 CFR Part 431, 2004 (2015)	Energy Efficiency Program for Certain Commercial and Industrial Equipment: Test Procedures and Efficiency Standards Final Rules	

IECC-C								
DOL	U. S. Department of Labor	
Standard Reference Number	Title	Referenced in Code(s):	
29 CFR Part 1910.1000 (2009)(2015)	Air Contaminants	IBC	IFC	IMC						
29 CFR Part 1910.1025 (2009)(2015)	Toxic and Hazardous Substances	IMC								
29 CFR Part 1910.1200 (2009)(2015)	Hazard Communication	IFC								
DOTn	Department of Transportation	
Standard Reference Number	Title	Referenced in Code(s):	

33 CFR Part 154 (1998)(2015)	Facilities Transferring Oil or Hazardous Material in Bulk	
IFC								

33 CFR Part 155 (1998) (2015)	Oil or Hazardous Material Pollution Prevention Regulations for Vessels	
IFC								

33 CFR Part 156 (1998)(2015)	Oil and Hazardous Material Transfer Operations	
IFC								

49 CFR Part 172-20092015	Hazardous Materials Tables, Special Provisions, Hazardous Materials Communications, Emergency Response Information and Training Requirements	

IBC	

IFC							
49 CFR Parts 100 to 185-2005(2015)	Hazardous Materials Regulations	IBC	IFC							

49 CFR Parts 173-178 (1998)2015	Specification of Transportation of Explosive and Other Dangerous Articles, UN 0335, UN 0336 Shipping Containers	

IBC								
DOTy	U. S. Department of Treasury	
Standard Reference Number	Title	Referenced in Code(s):	
27 CFR Part 55 (1998)(2015)	Commerce in Explosives	IFC								
EPA	Environmental Protection Agency	
Standard Reference Number	Title	Referenced in Code(s):	

40 CFR Part 355-20082015	Emergency Planning and Notification	
IFC								
FCC	Federal Communications Commission	
Standard Reference Number	Title	Referenced in Code(s):	

47 CFR Part 90.219-20072014	Private Land Mobile Radio Services- Use of Signal Boosters	
IFC								
FM	FM Global	
Standard Reference Number	Title	Referenced in Code(s):	

4470-20122016	Approval Standard for Single-Ply Poymer-Modified Bitumen Sheet, Built-Up Roof (BUR) and Liquid Applied Roof Assemblies for Use in Class 1 and Non-combustible Roof Deck Construction	

IBC								

4496-132016	Approval Standard for Classification of Pallets and other Materials Handling Products as Equivalent to Wood Pallet	

IFC								

4880 (2010)2015	Approval Standard for Class 1 Rating of Insulated Wall or Wall and Roof/Ceiling Building Panels, or Interior Finish Materials, or Coatings and Exterior Finish Systems	

IBC	

IRC							
GA	Gypsum Association	
Standard Reference Number	Title	Referenced in Code(s):	

GA-216-20132016	Application and Finishing of Gypsum Panel Products	
IBC								
GA-253-20122017	Application of Gypsum Sheathing	IRC								

GA-600-20122015	Fire Resistance Design Manual, 20th21st Edition	
IBC								
HPVA	Hardwood Plywood and Veneer Association	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/HPVA HP-1-20132016	American National Standard for Hardwood and Decorative Plywood	
IBC								
IAPMO	International Association of Plumbing and Mechanical Officials	
Standard Reference Number	Title	Referenced in Code(s):	
IAPMO Z124.7-20122013	Prefabricated Plastic Spa Shells	ISPSC								

IAPMO Z1001-20072014	Prefabricated Gravity Grease Interceptors	
IPC								
ICC	International Code Council	
Standard Reference Number	Title	Referenced in Code(s):	

IBC-1518	
International Building Code	
IRC	
IFC	
IMC	
IPC	IPSDC	
IFGC	
IECC	IEBC	

ICC 300-1217	ICC Standard on Bleachers, Folding and Telescopic Seating, and Grandstands	

IBC	

IFC	

IEBC						

ICC 400-1217	Standard for The Design and Construction of Log Structures	
IBC	
IRC	IECC- R						

ICC A117.1-09	Accessible and Usable Buildings and Facilities	
IFC	
IZC	
IEBC	
IPC	
IRC	
IBC			

IEBC-1518	
International Existing Building Code	
IBC	
IRC	
IPC	
IMC	
IFGC	
IECC	IPMC	
IPC	

IECC-15 18	International Energy Conservation Code	
IBC	
IRC	
IMC	
IFGC	
IPMC	IPSDC			

IFC-1518	

International Fire Code	

IBC	

IRC	

IMC	

IPC	

IFGC	
IWUIC	

IEBC	

IPM	

IFGC-1518	
International Fuel Gas Code	
IBC	
IRC	
IFC	
IMC	
IPC	
IECC	ISPSC	IEBC	
IMC-1518	International Mechanical Code	IBC	IRC	IFC	IPC	IFGC	IECC			

IPC 1518	
International Plumbing Code	
IBC	
IRC	
IFC	
IMC	IPSDC	
IFGC	
IEBC		

C

IPMC-15 18	International Property Maintenance Code	
IBC	
IRC	
IFC	
IEBC	IWUIC	
IFGC	
IMC	
IPC	

IPSDC-1518	International Private Sewage Disposal Code	
IBC	
IPC	
IRC						

IRC-1518	
International Residential Code	
IBC	
IFC	
IMC	
IFGC	
IEBC	
IPC	IPMC	IPSD	

ISPSC-15 18	International Swimming Pool and Spa Code	
IECC	
IFC	
IFGC	
IMC	
IPC	
IRC			

IWUIC-1518	International Wildland-Urban Interface Code	
IBC	
IFC	
IPMC						
IZC-1518	International Zoning Code	IBC	IMC							
IES	Illuminating Engineering Society	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/ASHRAE/IESNA 90.1-20132016	Energy Standard for Buildings Except Low-Rise Residential Buildings	

IECC								
IIAR	International Institute of Ammonia Refrigeration	
Standard Reference Number	Title	Referenced in Code(s):	

IIAR 02-2014	Addendum A to
Equipment, Safe Design, and Installation of Closed-Circuit Ammonia Mechanical Refrigerating Systems	

IMC	

IFC							
IKECA	International Kitchen Exhaust Cleaning Association	
Standard Reference Number	Title	Referenced in Code(s):	

C10-20112016	IKECA C10, Standard for the Methodology for Cleaning for Commercial Kitchen Exhaust Systems	

IFC								
ISEA	the International Safety Equipment Association	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/ISEA Z358.1-20092014	Emergency Eyewash and Shower Equipment	
IPC								
MSS	Manufacturers Standarization Society of the Valve and Fittings Industry	
Standard Reference Number	Title	Referenced in Code(s):	

SP-42-20092013	Corrosion Resistant Gate, Globe, Angle and Check Valves with Flanged and Butt Weld Ends (Classes 150, 300 & 600)	

IPC	

IRC							

SP-70-20112013	Gray Iron Gate Valves, Flanged and Threaded Ends	
IPC	
IRC							

SP-71-20112013	GreyGray Iron Swing Check Valves, Flanged and Threaded Ends	
IPC	
IRC							

SP-72-2010a	Ball Valves with Flanged or Butt- Welding Ends for General Service	
IPC	
IRC							

SP-78-20112013	Cast Iron Plug Valves, Flanged and Threaded Ends	
IPC	
IRC							

SP-80-20082013	Bronze Gate, Globe, Angle and Check Valves	
IPC	
IRC							

SP-110-2010a	Ball Valves, Threaded, Socket Welded ing, Solder Joint, Grooved and Flared Ends	

IPC	

IRC							
NAAMM	National Association of Architectural Metal Manufacturers	
Standard Reference Number	Title	Referenced in Code(s):	

FP 1001-0717	Guide Specifications for Design of Metal Flag Poles, Fourth Edition	
IBC								
NEMA	National Electrical Manufacturers Association	
Standard Reference Number	Title	Referenced in Code(s):	

MG1-19932014	
Motors and Generators	IECC-C								
Z535-20062017	ANSI/NEMA Color Chart	ISPSC								

250-20032014	Enclosures for Electrical Equipment (1000 Volts Maximum)	
IFC								
NFPA	National Fire Protection Association	
Standard Reference Number	Title	Referenced in Code(s):	
02-1116	Hydrogen Technologies Code	IFC								

10-1317	Standard for Portable Fire Extinguishers	
IFC	
IBC							

11-1015	Standard for Low-, Medium-, and High-Expansion Foam	
IFC	
IBC							

12-1115	Standard on Carbon Dioxide Extinguishing Systems	
IFC	
IBC							

12A-0915	Standard on Halon 1301 Fire Extinguishing Systems	
IFC	
IBC							

13-1316	Standard for the Installation of Sprinkler Systems	
IFC	
IBC	
IRC						

13D-1316	Standard for the Installation of Sprinkler Systems in One- and Two- Family Dwellings and Manufactured Homes	

IFC	

IRC	

IBC						

13R-1316	Standard for the Installation of Sprinkler Systems in Low-Rise Residential Occupancies	

IBC	

IEBC	

IRC						

14-1316	Standard for the Installation of Standpipe, Private Hydrants and Hose Systems	

IFC	

IBC							

15-1217	Standard for Water Spray Fixed Systems for Fire Protection	
IFC								

16-11 15	Standard for the Installation of Foam-Water Sprinkler and Foam- Water Spray Systems	

IFC	

IBC							

17-1317	Standard for Wet Chemical Extinguishing Systems	
IFC	
IBC							

17A-1317	Standard for Wet Chemical Extinguishing Systems	
IFC	
IBC							

20-1316	Standard for the Installation of Stationary Pumps for Fire Protection	

IFC	

IBC							

22-1318	Standard for Water Tanks for Private Fire Protection	
IFC								

24-1316	Standard for the Installation of Private Fire Service Mains and Their Appurtenances	

IFC								

25-1417	Standard for the Inspection, Testing and Maintenance of Water-Based Fire Protection Systems	

IFC	

IPMC							

30-1518	Flammable and Combustible Liquids Code	
IFC	
IBC							

30A-1518	Code for Motor Fuel Dispensing Facilities and Repair Garages	
IFC	
IMC	
IFGC	
IBC					

31-1115	Standard for the Installation of Oil- Burning Equipment	
IFC	
IRC	
IMC	
IBC					
32-1115	Standard for Drycleaning Plants	IFC	IBC							

33-1116	Standard for Spray Application Using Flammable or Combustible Materials	

IFC								

34-1115	Standard for Dipping and Coating Processes Using Flammable or Combustible Liquids	

IFC								

35-1115	Standard for the Manufacture of Organic Coatings	
IFC								

37-1518	Standard for the Installation and Use of Stationary Combustion Engines and Gas Turbines	

IMC	

IFGC							

40-1116	Standard for the Storage and Handling of Cellulose Nitrate Film	
IFC	
IBC							

51-13 18	Standard for the Design and Installation of Oxygen-Fuel Gas Systems for Welding, Cutting, and Allied Processes	

IFC	

IPC	

IFGC						

52-1316	Vehicular Gaseous Fuel Systems Code	
IFC								

55-1316	Compressed Gases and Cryogenic Fluids Code	
IFC								

56-1417	Standard for Fire and Explosion Prevention during Cleaning and Purging of Flammable Gas Piping Systems	

IFC								
58-1417	Liquefied Petroleum Gas Code	IFC								

59A-1316	Standard for the Production, Storage and Handling of Liquefied Natural Gas (LNG)	

IFC								

61-1317	Standard for the Prevention of Fires and Dust Explosions in Agricultural and Food Processing Facilities	

IFC	

IBC							

70-1417	
National Electrical Code	
IRC	
IEBC	
IBC	IWUIC	
IPMC				

72-1316	National Fire Alarm and Signaling Code	
IFC	
IBC	
IRC	
IMC	
IEBC				

80-1316	Standard for Fire Doors and Other Opening Protectives	
IFC	
IBC							

91-1015	Standard for Exhaust Systems for Air Conveying of Vapors, Gases, Mists, and Particulate Solids	

IMC								

91-1015	Standard for Exhaust Systems for Air Conveying of Vapors, Gases, Mists, and Particulate Solids	

IMC								

92-1215	Standard on Smoke Control Systems	
IFC	
IBC	
IMC						

96-1417	Standard for Ventilation Control and Fire Protection Commercial Cooking Operations	

IMC								
99-1518	Health Care Facilities Code	IBC	IFC	IEBC	IPC					
101-1518	Life Safety Code	IBC	IFC	IEBC						

105-1316	Standard for the Installation of Smoke Door Assemblies and Other Opening Protectives	

IBC	

IFC							

110-1316	Standard for Emergency and Standby Power Systems	
IFC	
IBC	
IECC						

120-1015	Standard for Fire Prevention and Control in Coal Mines	
IFC	
IBC							

160-1116	
Standard Use of Flame Effects Before an Audience	

IFC								

170-1518	Standard for Fire Safety and Emergency Symbols	
IFC	
IBC							

204-1215	Standard for Smoke and Heat Venting	
IFC								

211-1316	Standard for Chimneys, Fireplaces, Vents and Solid Fuel-Burning Appliances	

IMC	

IFGC							

221-1518	Standard for High Challenge Fire Walls, Fire Walls and Fire Barrier Walls	

IBC								

241-1318	Standard for Safeguarding Construction, Alteration, and Demolition Operations	

IFC								

252-1217	
Standard Methods of Fire Tests of Door Assemblies	

IBC								

253-11 15	Standard Method of Test for Critical Radiant Flux of Floor Covering Systems Using a Radiant Heat Energy Source	

IBC	

IFC							

257-1217	Standard on Fire Test for Window and Glass Block Assemblies	
IBC								

259-1318	Standard Test Method for Potential Heat of Building Materials	
IBC	
IRC							

260-1318	Standard Methods of Tests and Classification System for Cigarette Ignition Resistance of Components of Upholstered Furniture	

IFC								

261-1318	Standard Method of Test for Determining Resistance of Mock-Up Upholstered Furniture Material Assemblies to Ignition by Smoldering Cigarettes	

IFC								

262-1115	Standard Method of Test for Flame Travel and Smoke of Wires and Cables for Use in Air-Handling Spaces	

IMC	

IBC							

265-1115	Standard Methods of Fire Tests for Evaluating Room Fire Growth Contribution of Textile or Expanded Vinyl Wall overings on Full Height Panels and Walls	

IBC	

IFC							

268-1217	Standard Test Method for Determining Ignitibility of Exterior Wall Assemblies Using a Radiant Heat Energy Source	

IBC								

268-1217	Standard Test Method for Determining Ignitibility of Exterior Wall Assemblies Using a Radiant Heat Energy Source	

IBC								

274-1318	Standard Test Method to Evaluate Fire Performance Characteristics of Pipe Insulation	

IMC								

275-1317	Standard Method of Fire Tests for the Evaluation of Thermal Barriers	
IBC	
IRC							

276-1115	Standard Method of Fire Test For Determining the Heat Release Rate of Roofing Assemblies with Combustible Above-Desk Roofing Components	

IBC								

285-1217	Standard Fire test Method for Evaluation of Fire Propagation Characteristics of Exterior Non- Load-Bearing Wall Assemblies Containing Combustible Components	

IBC								

288-12 17	
Standard Methods of Fire Tests of Horizontal Fire Door Assemblies Installed in Horizontal Fire- Resistance-Rated Assemblies	

IBC								

289-1318	Standard Method of Fire Test for Individual Fuel Packages	
IFC	
IBC							

303-1116	Fire Protection Standard for Marinas and Boatyards	
IFC								

318-1518	Standard for the Protection of Semiconductor Fabrication Facilities	
IFC								

326-1015	Standard for the Safeguarding of Tanks and Containers for Entry, Cleaning or Repair	

IFC								

385-1217	Standard for Tank Vehicles for Flammable and Combustible Liquids	
IFC								
400-1316	Hazardous Materials Code	IFC								
407-1217	Standard for Aircraft Fuel Servicing	IFC								
409-1116	Standard on Aircraft Hangers	IFC	IBC	IFGC						
410-1015	Standard on Aircraft Maintenance	IFC								
418-1116	Standard for Heliports	IBC								
484-1518	Standard for Combustible Metals	IFC								
495-1318	Explosive Materials Code	IFC								

498-1318	Standard for Safe Havens and Interchange Lots for Vehicles Transporting Explosives	

IFC								
501-1317	Standard on Manufactured Housing	IRC								

505-1318	Fire Safety Standard for Powered Industrial Trucks Including Type Designations, Areas of Use, Conversions, Maintenance, and Operations	

IFC								

654-1317	Standard for the Prevention of Fire & Dust Explosions from the Manufacturing, Processing, and Handling of Combustible Particulate Solids	

IBC	

IFC							

655-1217	Standard for the Prevention of Sulfur Fires and Explosions	
IBC	
IFC							

664-1217	Standard for the Prevention of Fires and Explosions in Wood Processing and Woodworking Facilities	

IBC	

IFC							

701-1015	Standard Method of Fire Tests for Flame-Propagation of Textiles and Films	

IFC	

IBC							

703-1518	Standard for Fire Retardant Treated Wood and Fire Retardant Coatings for Building Materials	

IFC								

704-1217	Standard System for the Identification of the Hazards of Materials for Emergency Response	

IFC	

IMC	

IBC						

790-1418	Standard Test for Competency of Third-Party Field Evaluation Bodies	
IFC								

853-1015	Standard for the Installation of Stationary Fuel Cell Power Systems	
IRC	
IMC	
IFGC						

914-1015	Code for Fire Protection of Historic Structures	
IFC								

1122-1318	
Code for Model Rocketry	
IFC								
1123-1418	Code for Fireworks Display	IFC								

1124-1317	Code for the Manufacture, Transportation, Storage and Retail Sales of Fireworks and Pyrotechnic Articles	

IFC	

IBC							

1125-1217	Code for the Manufacture of Model Rocket and High Power Rocket Motors	

IFC								

1126-1116	Standard for the Use of Pyrotechnics Before a Proximate Audience	

IFC								
1127-1318	Code for High Power Rocketry	IFC								

1142-1217	Standard on Water Supplies for Suburban and Rural Fire Fighting	
IFC								

1901-0916	Standard for Automotive Fire Apparatus	
IFC								

2001-1215	Standard on Clean Agent Fire Extinguishing Systems	
IFC	
IBC							
NFRC	National Fenestration Rating Council Inc.	
Standard Reference Number	Title	Referenced in Code(s):	

100-20092017	Procedure for Determining Fenestration Product U-factors- Second Edition	

IECC								

200-20092017	Procedure for Determining Fenestration Product Solar Heat Gain Coefficients and Visible Transmittance at Normal Incidence- Second Edition	

IECC								

400-20092017	Procedure for Determining Fenestration Product Air Leakage- Second Edition	

IECC								
NSF	NSF International	
Standard Reference Number	Title	Referenced in Code(s):	

3-20102012	Commercial Warewashing Equipment	
IPC								

14-20112015	Plastic Piping System Components and Related Materials	
IRC	
IPC	ISPSC	
IMC					

40-20122013	Residential Wastewater Treatment Systems	
IPSDC								

42-20112015	Drinking Water Treatment Units - Aesthetic Effects	
IRC	
IPC							

44-20122015	Residential Cation Exchange Water Softeners	
IRC	
IPC							

50-20122015	Equipment for Swimming Pools, Spas, Hot Tubs, and other Recreational Water Facilities	

ISPSC	

IPC							

53-2011A2015	Drinking Water Treatment Units - Health Effects	
IRC	
IPC							

58-20122015	Reverse Osmosis Drinking Water Treatment Systems	
IRC	
IPC							

61-20122015	Drinking Water System Components
- Health Effects	
IRC	
IPC							
62-20122015	Drinking Water Distillation Systems	IPC								

350-20112014	Onsite Residential and Commercial Water Reuse Treatment Systems	
IPC	
IRC							

358-1-20112014	Polyethylene Pipe and Fittings for Water-Based Ground Source "Geothermal" Heat Pump Systems	

IRC	

IMC							

372-20102011	Drinking Water Systems Components - Lead Content	
IPC								
PSAI	Portable Sanitation Association International	
Standard Reference Number	Title	Referenced in Code(s):	

Z4.3- 9515	Minimum Requirements for Nonsewered Waste-Disposal Systems	

IPC								
SBCA	Structural Building Components Association	
Standard Reference Number	Title	Referenced in Code(s):	

BCSI-2013 (updated March 2015)	Building Component Safety Information Guide to Good Practice for Handling, Installing, Restraining & Bracing of Metal Plate Connected Wood Trusses	

IRC								
SDI	Steel Deck Institute	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/ SDI NC1.0-102017	Standard for Non-Composite Steel Floor Deck	
IBC								
ANSI/ SDI RD1.0-102017	Standard for Steel Roof Deck	IBC								

SDI-C-20112017	Standard for Composite Steel Floor Deck Slabs	
IBC								

SDI QA/QC-20112017	Standard for Quality Control and Quality Assurance for Installation of Steel Deck	

IBC								
SJI	Steel Joist Institute	
Standard Reference Number	Title	Referenced in Code(s):	

CJ-10 SJI-200-16	Standard Specification for Composite Steel Joists, CJ-Series	
IBC								
SMACNA	Sheet Metal & Air Conditioning Contractors	
Standard Reference Number	Title	Referenced in Code(s):	

SMACNA\ANSI (2015) (2016)	HVAC Duct Construction Standards- Metal and Flexible 4th Edition (ANSI) 2016	

IMC	

IRC							
SPRI	Single-Ply Roofing Institute	
Standard Reference Number	Title	Referenced in Code(s):	

ANSI/SPRI/FM4435-ES-1-11	Wind Test Standard for Edge Systems Used with Low Slope Roofing	

IBC								

ANSI/SPRI VF1-10	External Fire Design Standard for Vegetative Roofs	
IBC								
SRCC	Solar Rating Certification Corporation	
Standard Reference Number	Title	Referenced in Code(s):	

ICC 900/SRCC 300-132015	Standard 300 for Solar Water Heating Systems Solar Thermal System Standard	

IRC								

ICC 901/SRCC 100-132015	Standard 100 for Solar
Collectors Solar Thermal Collector Standard	

IRC								
TCNA	Tile Council of North America	
Standard Reference Number	Title	Referenced in Code(s):	

A108.1A-9916	Installation of Ceramic Tile in the Wet-set Method, with Portland Cement Mortar	

IBC	

IRC							

A118.1-9916	American National Standard Specification for Dry-Set Cement Mortar	

IBC	

IRC							

A118.3-99 13	American National Standard Specifications for Chemical Resistant, Water Cleanable Tile- setting and -grouting Epoxy and Water Cleanable Tile-setting Epoxy Adhesive	

IBC	

IRC							

A118.4-9916	American National Standard Specifications for Latex-portland Modified Dry-Set Cement Mortar	

IBC								

A118.6-9910	American National Standard Specifications for Standard Cement Grouts for Tile Installation	

IBC								

A136.1-9908	American National Standard Specifications for Organic Adhesives for Installation of Ceramic Tile	

IBC	

IRC							

A137.1-200817	Standard Specifications for Ceramic Tile	
IBC	
IRC							
TIA	Telecommunications Industry Association	
Standard Reference Number	Title	Referenced in Code(s):	

222-GH-2005 2016	Structural Standards for Antenna Supporting Structures and Antennas, Including-Addendum 1, 222-G-1, Dated 2007, Addendum 2, 222-G-2 dated 2009 Addendum 3, 222-3 dated 2013 and Addendum 4, 222-G-4 dated 2014	

IBC								
TMS	The Masonry Society	
Standard Reference Number	Title	Referenced in Code(s):	

402-20132016	Building Code for Masonry Structures	
IBC	
IRC							

403-20132017	Direct Design Handbook for Masonry Structures	
IBC	
IRC							

602-20132016	Specification for Masonry Structures	
IBC	
IRC							
UL	Underwriter Laboratories	
Standard Reference Number	Title	Referenced in Code(s):	

UL/CSA/ANCE 60335-2-40-2012	Standard for safety of Household and Similar Electrical Appliances, part 2-40: particular requirements for Motor-Compressors
for electrical heat pumps, air- conditioners and dehumidifiers	

IRC								

09-2009	Fire Tests of Window Assemblies with revisions through February 2015.	

IBC								

10A-2009	Tin Clad Fire Doors - with revisions through December 2013.	
IBC								

10B-2008	Fire Tests of Door Assemblies - with revisions through April
2009 February 2015	

IBC								

10C-2009	Positive Pressure Fire Tests of Door Assemblies with revisions through February 2015	

IBC	

IFC							

14B-2008	Sliding Hardware for Standard Horizontally Mounted Tin Clad Fire Doors-with revisions through May 3, 2013	

IBC								

17-2008	Vent or Chimney Connector Dampers for Oil-Fired Appliances - with Revisions through January 2010 September 2013	

IRC	

IMC							

30-95	
Metal Safety Cans - with Revisions through July 2009June 2014	

IFC								

80-2007	Steel Tanks for Oil-Burner Fuels and Other Combustible Liquids - with revisions through August 2009January 2014	

IRC	

IFC							

87A-1215	Outline of Investigation for Power- Operated Dispensing Devices for Gasoline and Gasoline/Ethanol Blends with Nominal Ethanol Concentrations up to 85 percent	

IFC								

127-11	Factory-Built Fireplaces- with revisions through May 2015	
IBC	
IRC	
IMC						

142-06	Steel Aboveground Tanks for Flammable and Combustible Liquids with revisions through February 12, 2010August 2014	

IFC	

IPC							

174-04	Household Electric Storage Tank Water Heaters - with Revisions through September 2012April 2015	

IRC	

IMC							

197-10	
Commercial Electric Cooking Appliances - with revisions through June 2011September 2014	

IMC								

207-2009	Refrigerant-Containing Components and Accessories, Nonelectrical - with revisions through June 2014	

IMC	

IRC							

217-2006	Single and Multiple Stations Smoke Alarms - with revisions through April 2012October 2015	

IBC	

IRC	

IFC						

263-11	Standard for Fire Test of Building Construction and Materials - with revisions through June 2015	

IBC	

IRC	
IWUIC						

268A-2008	
Smoke Detectors for Duct Application - with Revisions through September 2009October 2014	

IMC								

294-1999	Access Control Systems Units with revisions through September
2010 February 2015	

IBC	

IFC							

300-2005(R2010)	Fire Testing of Fire Extinguishing Systems for Protection of Commercial Cooking Equipment with revisions through July 16, 2010December 2014	

IBC	

IFC							

305-2012	Panic Hardware - with revisions through August 2014	
IBC	
IFC							

325-2002	Door, Drapery, Gate, Louver and Window Operations and Systems - with revisions through June 2013May 2015	

IRC	

IFC	

IBC						

372-2007	Automatic Electrical Controls for Household and Simular Use - Part 2: Particular Requirements for Burner Ignition Systems and Components with revisions through July 25, 2012	

ISPSC								

378-06	Draft Equipment - with revisions through January 2010 June 12,2014	

IRC	

IMC							

391-2010	Solid-Fuel and Combination-Fuel Central and Supplementary Furnaces - with revisions through March 2010June 2014	

IMC								

399-2008	Drinking-Water Coolers with revisions through January 14, 2011October 2013	

IPC								

412-2011	Refrigeration Unit Coolers - with Revisions through August 2012September 2013	

IMC								

430-2009	Waste Disposers, with revisions through March 23, 2011September 2015	

IPC								

441-2010	Gas Vents - with revisions through June 12, 2014	
IRC	
IFGC							

499-05	Electric Heating Appliances-with revisions through February 2013November 2014	

IMC	

IFC							

508-99	Industrial Control Equipment - with revisions through March 2013October 2013	

IMC	

IPC	

IRC						

515-2011	Electric Resistance Heat Tracing for Commercial and Industrial Applications including revisions through November 30, 2011July 2015	

IECC-R								

536-1997	Flexible Metallic Hose - with Revisions through June 2003December 2014	

IRC	

IMC							

555-2006	Fire Dampers-with revisions through May 20122014	
IBC	
IRC							

555C-2006	Ceiling Dampers-with revisions through May 2010December 2014	
IBC	
IMC							

555S-1999	Smoke Dampers - with Revisions through May 2012 February 2014									

580-2006	Test for Uplift Resistance of Roof Assemblies with Revisions through July 2009October 2013	

IBC								

586-2009	High-Efficiency, Particulate, Air Filter Units- with revisions through September 2014	

IMC								

641-2010	Type L Low-Temperature Venting Systems - with revisions through May 2013June 2013	

IBC	

IRC	

IMC						

651–2011	Schedule 40 and Schedule 80 Rigid PVC Conduit and Fittings with revisions through March 2012May 2014	

IFGC	

IRC							

705-2004	Standard for Power Ventilators with revisions through March 2012December 2013	

IMC	

IRC							

710-2012	Exhaust Hoods for Commercial Cooking Equipment - with revisions through November 2013	

IMC	
IECC- C							

710B-2011	
Recirculating Systems with revisions through August 2014	

IBC	

IFC	

IMC						

723-08	Standard for Test for Surface Burning Characteristics of Building Materials with revisions through September 2010August 2013	

IBC	

IFC	

IWUIC						

726-1995	Oil-Fired Boiler Assemblies - with Revisions through April 2011October 2013	

IRC	

IMC	

IECC						

727-2006	Oil-Fired Central Furnaces with revisions through April 2010October 2013	

IRC	

IMC	
IECC- C						

729-03	Oil-Fired Floor Furnaces with revisions through August 2012October 2013	

IRC	

IMC							

730-03	Oil-Fired Wall Furnaces with revisions through August 2012October 2013	

IRC	

IMC							

731-1995	Oil-Fired Unit Heaters with Revisions through through August 2012October 2013	

IMC	
IECC- C							

732-1995	Oil-Fired Storage Tank Water Heaters - with revisions through April 2010October 2013	

IRC	

IMC							

737-11	Fireplaces Stoves - with revisions through August 2015	
IRC	
IMC							

762-10	Outline of Investigation for Power Roof Ventilators for Restaurant Exhaust Appliances with revisions through October 2013	

IMC								

790-04	Standard Test Methods for Fire Tests of Roof Coverings with revisions through October 2008July 2014	

IBC	

IRC	

IFC						

791-2006	Residential Incinerators-with revisions through April 2010November 2014	

IMC								

795-2011	Commercial-Industrial Gas Heating Equipment with revisions through September 2012November 2013	

IRC	

IFGC							

834-04	Heating, Water Supply, and Power Boilers - Electric with Revisions through January 2013December 2013	

IRC	

IMC							

842-07	Valves for Flammable Fluids with Revisions through October 2012May 2015	

IRC	

IMC							

858-05	Household Electric Ranges - with Revisions through April 2012June 2015	

IMC	

IRC							

864-03	Control Units and Accessories for Fire Alarm Systems-with Revisions through August 2012December 2014	

IBC	

IFC							

867-2011	Electrostatic Air Cleaners - with Revisions through February 2013 August 2013	

IMC								

873-2007	Temperature-Indicating and - Regulating Equipment, with revisions through July 25, 2012February 2015	

ISPSC								

875-09	Electric Day Bath Heaters with revisions through November 2011December 2013	

IMC	

IRC							

896-1993	Oil-Burning Stoves - with Revisions through August 2012November 2013	

IRC	

IMC							

900-04	Air Filter Units- with revisions through February 2012April 2015									

907-94	Fireplace Accessories - with revisions through April 2010June 2014	

IMC								

923-2013	Microwave Cooking Appliances - with revisions through June 2015	
IRC	
IMC							

924-06	Standard for Safety Emergency Lighting and Power Equipment with revisions through February 2011April 2014	

IBC	

IFC							

959-2010	Medium Heat Appliance Factory- Built Chimneys - with revisions through June 2014	

IRC	

IMC	

IFGC						

1004-1-12	Standard for Rotating Electrical Machines General Requirements with revisions through June 23, 2011	

ISPSC								

1026-2012	Electric Household Cooking and Food Services Appliances - with revisions through August 2015	

IRC								

1042-2009	Electric Baseboard Heating Equipment-with revisions through June 2013September 2014	

IRC								

1081-2008	Standard for Swimming Pool Pumps, Filters and Chlorinators, with revisions through May 2013March 2014	

ISPSC								

1256-2002	Fire Test of Roof Deck Construction with Revisions through January 2007July 2013	

IBC	

IRC							

1275-2005	Flammable Liquid Storage Cabinets with revisions through February 2010November 2014	

IFC								

1363-2007	Relocatable Power Taps - with revisions through September 2012September 2015	

IFC								

1479-03	Standard for Fire Tests of Through- Penetration Firestops with Revisions through October 2012June 2015	

IBC	

IRC	

IMC						

1482-2011	Solid-Fuel Type Room Heaters - with revisions through August 2015	
IBC	
IRC	
IMC						

1563-2009	Standard for Electric Hot Tubs, Spas and Association Equipment with revisions through July 2012March 2015	

ISPSC								

1618-09	Wall Protectors, Floor Protectors, and Hearth Extensions - with revisions through May 2013October 2015	

IRC	

IMC	

IFGC						

1703-02	Flat-plate Photovoltaic Modules and Panels - with revisions through November 2014October 2015	

IRC	

IBC							

1738-2010	Venting Systems for Gas-Burning Appliances, Categories II, III and IV with revisions through May 2011November 2014	

IRC	

IFGC							

1741-2010	Inverters, Converters, Controllers and Interconnection System Equipment with Distributed Energy Resources - with revisions through January 2015	

IRC								

1746-2007	External Corrosion Protection Systems for Steel Underground Storage Tanks - with revisions through December 2014	

IPC								

1777-07	
Chimney Liners with revisions through July 2009October 2015	

IBC	

IRC	

IMC						

1784-2001	
Air Leakage Tests of Door Assemblies - with Revisions through July 2009February 2015	

IBC	

IECC- C							

1795-2009	Hydromassage Bathtubs including revisions through August 23, 2011January 2015	

IPC								

1812-2013	Standard for Ducted Heat Recovery Ventilators - with revisions through April 2014	

IMC								

1815-2012	Standard for Nonducted Heat Recovery Ventilators - with revisions through April 2014	

IMC								

1821-2011	Standard for Thermoplastic Sprinkler Pipe and Fittings for Fire Protection Services - with revisions through August 2015	

IRC								

1897-2012	Uplift Tests for Roof Covering Systems - with revisions through September 2015	

IBC								

1978-2010	Grease Ducts - with revisions through September 2013	
IMC								

1994-04	Luminous Egress Path Marking Systems with Revisions through November 2010May 2015	

IBC								

1995-2011	Heating and Cooling Equipment - with revisions through July 2015	
IRC	
IMC	ISPSC						

1996-2009	Electric Duct Heaters-with revisions through November 2011June 2014	
IRC	
IMC							

2024-2011	Standard for Safety Optical-Fiber and Communications Cable Raceway- with Revisions through April 2011August 2015	

IMC								

2034-2008	Standard for Safety for Single and Multiple Station Carbon Monoxide Alarms with revisions through February 2009March 2015	

IRC	

IFC	

IBC						

2043-2008	Fire Test for Heat and Visible Smoke Release for Discrete Products and their Accessories Installed in Air- Handling Spaces - with revisions through October 2013	

IMC								

2079-2004	Tests for Fire Resistance of Building Joint Systems with Revisions through December 2012August 2015	

IBC	

IFC							

2200-2012	Stationary Engine Generator Assemblies - with revisions through June 2013July 2015	

IBC	

IFC	

IMC						

2208-2010	Solvent Distillation Units - with Revisions through March 2011September 2015	

IFC								
USC	United States Code	
Standard Reference Number	Title	Referenced in Code(s):	
CFR Title 16 (May 31, 2005) (2015)	R-Value Rule	IRC	IECC							
WCLIB	West Coast Lumber Inspection Bureau	
Standard Reference Number	Title	Referenced in Code(s):	
AITC 104-03	Typical Construction Details	IBC								

AITC 110-01	Standards Appearance Grades for Structural Glued Laminated Timber	
IBC								

AITC 113-10	Standard for Dimensions of Structural Glued Laminated Timber	
IBC								

AITC 119-96	Standard Specifications for Structural Glued Laminated Timber of Hardwood Species	

IBC								

AITC 200-09	Manufacturing Quality Control System Manual for Structural Glued Laminated Timber	

IBC								
WDMA	Window and Door Manufacturers Association	
Standard Reference Number	Title	Referenced in Code(s):	

AAMA/WDMA/CSA 101/I.S./A440-1116	North American Fenestration Standard/Specifications for Windows, Doors, and Skylights	

IBC	

IRC	

IECC						
WMA	World Millwork Alliance (formerly the Association of Millwork Distributors Standards)	

Standard Reference Number	Title	Referenced in Code(s):	

ANSI/AMD WMA100-2013 2016	Standard Method of Determining Structural Performance Ratings of Side Hinged Exterior Door Systems
and Procedures for Component Substitution	

IRC								

Reason: THIS IS THE ADMIN STANDARDS UPDATE CODE CHANGE
The CP 28 Code Development Policy, Section 4.6 requires the updating of referenced standards to be accomplished administratively, and be processed as a Code Change Proposal for consideration by the Administrative Code Change Committee. In September 2015, a letter was sent to each developer of standards that is referenced in the International Codes, asking them to provide ICC with a list of their standards in order to update to the current edition. Above is the list of the referenced standards that are to be updated based upon responses from standards developer.

Report of Committee Action Hearings

Committee Action:	Approved as Modified

Modify as follows:

AAMA	American Architectural Manufacturers Association	
Standard Reference Number	Title	Referenced in Code(s):	
AAMA 711-1316	Voluntary Specification for Self Adhering Flashing Used for Installation of Exterior Wall Fenestration Products	IRC							
AAMA 506-1116	Voluntary Specifications for Impact and Cycle Testing of Fenestration Products	IRC							
AAMA/NSA/NPEA 2100- 1112	Specifications for Sunrooms	IRC							
AAMA/WDMA/CSA 101/I.S.2/A440-
1617	North American Fenestration Standard/Specification for Windows, Doors, and Skylights	IBC	IRC	IECC					
									
ASTM	ASTM								
Standard Reference Number	Title	Referenced in Code(s):	
D1929- 1416	Standard Test Method for Determining Ignition Temperature of Plastics	IBC							
D2843-1016	Standard Test Method for Density of Smoke from the Burning of Decomposition of Plastics	IBC							
D2859- 06(2011)15	Standard Test Method for Ignition Characteristics of Finished Textile Floor Covering Materials	IBC	IFC						

E84-2013A 2015B	Standard Test Method for Surface Burning Characteristics of Building Materials	IBC	IRC	IFC	IMC	IEBC			
E119 - 2012a 2016	Standard Test Methods for Fire Tests of Building Construction and Materials	IBC	IRC	IMC	IWUIC				
E136 - 1216	Standard Test Method for Behavior of Materials in a Vertical Tube Furnace at 750 degrees C	IBC	IRC	IMC	IWUIC	IFGC			
E814-20132013A	Standard Test Method of Fire Tests of Penetration Firestop Systems	IBC	IRC	IMC					
E970- 20102014	Standard Test Method for Critical Radiant Flux of Exposed Attic Floor Insulation Using a Radiant Heat Energy Source	IBC	IRC						
E1354 - 20132016	Standard Test Method for Heat and Visible Smoke Release Rates for Materials and Products Using an Oxygen Consumption Colorimeter	IBC	IFC						
E1529-201314a	Standard Test Method for Determining Effects of Large Hydrocarbon Pool Fires on Structural Members and Assemblies	IFC							
E1537 - 20132015	Standard Test Method for Fire Testing of Upholstered Furniture	IFC							
E1966-2012A2015	Standard Test Method for Fire resistant Joint Systems	IBC	IFC						
E2336 - 04(2013)2016	Standard Test Methods for Fire Resistive Grease Duct Enclosure Systems	IMC							
E2404-13E115a	Standard Practice for Specimen Preparation and Mounting of Textile, Paper or
Polymeric (Including Vinyl) and Wood Wall or Ceiling Coverings, Facing and Veneers to Assess Surface Burning Characteristics	IBC	IFC						
E2599 - 1115	Standard Practice for Specimen Preparation and Mounting of Reflective Insulation Radiant Barrier and Vinyl Stretch
Ceiling Materials for Building Applications to Assess Surface Burning Characteristics	IBC							
									
AWPA	American Wood Protection Association		
Standard Reference Number	Title	Referenced in Code(s):		
M4-1116	Standard for the Care of Preservative- Treated Wood Products	IBC	IRC						
U1 - 1416	USE CATEGORY SYSTEM: User
Specification for Treated Wood except ,	IBC	IRC						

	Commodity Specification H								
									
CGA	Compressed Gas Association		
Standard Reference Number	Title	Referenced in Code(s):		
S-1.2 (2005)(2009)	Pressure Relief Device Standards - Part 2 - Cargo and Portable Tanks for Compressed Gases	IFC	IFGC						
									
ICC	International Code Council		
Standard Reference Number	Title	Referenced in Code(s):		
ICC A117.1- 20162009	Accessible and Usable Buildings and Facilities	IBC	IEBC	IFC	IPC	IRC	IZC		
									
SPRI	Single-Ply Roofing Institute		
Standard Reference Number	Title	Referenced in Code(s):		
ANSI/SPRI/FM4435- ES-1-1117	Wind Test Standard for Edge Systems Used with Low Slope Roofing	IBC							
ANSI/SPRI VF1- 1017	External Fire Design Standard for Vegetative Roofs	IBC							

Committee Reason: Hansen19, Hansen 22 and Hansen 24 added updated references for AAMA standards. Hirschler 25 adds updates references for ASTM standards. Hirscher 25 included two standards that are not in the 2015 edition, E648 and E2579, therefore, they are not part of this update. Wangel 14 adds updates for AWPA standards.  These references are updates that  should have been part of the original proposal.
McLaughlin 20 requests not to updated reference for a CGA standard to a 2016 edition. The proponent explained that this is an incorrect reference.
Wilen 10 requests not to update references for two SPRI standards to the 2017 edition. The proponent explained that these standards are not ready for review at this time.
Orlowski 13 requests the ICC A117.1 to not be updated and remain as a reference to the 2009 edition. This standard has significant revisions that are not finalized at the time of this hearing. There should be the opportunity to address scoping and references in the codes and the implications to buildings with these new requirements. There was testimony that the new requirements will no longer be coordinated with the 2010 ADA Standard for Accessible Design. The committee noted that there was no opposition testimony to leaving this standard on the current edition.
The remainder of the standards references are part of the automatic update of currently referenced standards. This is part  of CDP28 allowances for updates and should be approved.

Assembly Action	None

Public Comment(s)

As stated in the posted 2016 Group B Public Comment Hearing Agenda, ADM94-16 was dealt with procedurally by dividing the code change proposal into a multiple part code change proposal; with each referenced standard receiving a public comment being dealt with as a separate part in conjunction with the submitted public comment. In addition, the updates to some of the referenced standards were As Modified by the committee, as shown in the 2016 Report of Committee Action Hearing. The actions taken on proposed updates to the referenced standards listed in ADM94-16 were As Submitted except as noted below:

Standard Ref. No. in 2015 Codes	Final Action	Resulting Version for 2018 Codes	
Updates based on Public Comment Hearing and OGCV	
ASCE 7 - 10	AS	ASCE 7 –16	
ICC A117.1 -09	D	ICC A117.1 -09	
SJI-200-10	AMPC11	SJI-200-15	
ASTM F2006-00 (2005)	AMPC10	ASTM F2006-00 (2017)	
ASTM F2090-10 .	AMPC9	ASTM F2090-17	
ASTM E108 - 2011	AMPC8	ASTM E108 - 2016	
ANSI/SPRI VF1-10	D	ANSI/SPRI VF1-10	
ASTM D7158-11	AMPC3	ASTM D7158-16	
ASHRAE 140- 11	AMPC4	ASHRAE 140- 14	
FM 4996 - 13	AMPC5	FM 4996 – 2015	
ASTM D2859- 06(2011)	AMPC6	ASTM D2859- 2016	
ASTM E84-2013A	AMPC7	ASTM E84-2016	
ANSI/SPRI/FM 4435 – ES – 1-11	D	ANSI/SPRI/FM 4435 – ES – 1-11	
Updates based on the results of the Committee Action Hearing with No Public Comments Received	
AAMA 711-13	AM	AAMA 711-16	
AAMA 506 – 11	AM	AAMA 506-16	
AAMA/WDMA/CSA 101/I.S.2/A440 – 11	AM	AAMA/WDMA/CSA 101/I.S.2/A440 – 17	
ASTM D1929 – 12	AM	ASTM D1929 – 16	
ASTM D2843 – 10	AM	ASTM D2843 – 16	
ASTM E119-2012a	AM	ASTM E119- 2016	
ASTM E136 – 12	AM	ASTM E136 – 16	
ASTM E814-2013	AM	ASTM E814-2013A	
ASTM E970-2010	AM	ASTM E970- 2014	
ASTM E1354 – 2013	AM	ASTM E1354 – 2016	
ASTM E1529-2013	AM	ASTM E1529-2014a	
ASTM E1537 – 2013	AM	ASTM E1537 – 2015	
ASTM E1966-2012A	AM	ASTM E1966-2015	
ASTM E2336 –04(2013)	AM	ASTM E2336 –2016	
ASTM E2404-13E1	AM	ASTM E2404-15a	
ASTM E2599 – 11	AM	ASTM E2599 – 15	
AWPA M4 – 11	AM	AWPA M4 – 16	
AWPA U1-14	AM	AWPA U1-16	
CGA S-1.2 (2005)	AM	CGA S-1.2 (2009)	

Public Comment 3:
Mike Fischer, Kellen, representing Asphalt Roofing Manufacturers Association and the Gypsum Association (mfischer@kellencompany.com) requests Approve as Modified by this Public Comment.

Further modify as follows:

ASTM	ASTM	
Standard Reference Number	
Title	Referenced in Code(s):	
D 7158/D7158M-11 D7158M- 16	Standard Test Method for Wind Resistance of Asphalt Shingles (Uplift Force/Uplift Resistance Method)	
IBC	
IRC	
Commenter's Reason: ASTM D7158 has recently been updated to reflect correlations to ASCE-7-10. This comment updates the edition for the 2018 I-Codes to include the new 2016 edition.

Public Comment 4:
Steven Ferguson, representing American Society of Heating, Refrigerating, and Air-Conditioning Engineers (sferguson@ashrae.org) requests Approve as Modified by this Public Comment.

Modify as follows:

ASHRAE	American Society of Heating, Refrigerating and Air Conditioning Engineers	
Standard Reference Number	
Title	Referenced in Code(s):	
140-2017 140-2014	Standard Method of Test for the Evaluation of Building Energy Analysis	IECC-C	
	Computer Programs		

Commenter's Reason: There is a chance ASHRAE Standard 140-2017 may not be published in time for the administrative reference update. This public comment is being submitted so we refer to the current version of the standard (the 2014 version) rather than the next version of the standard.

Public Comment 5:
Marcelo Hirschler, representing GBH International (gbhint@aol.com) requests Approve as Modified by this Public Comment.

Further modify as follows:

FM	FM Global	
Standard Reference Number	
Title	Referenced in Code(s):	

4496-2016 4996-2015	Approval Standard for Classification of Pallets and other Materials Handling Products as Equivalent to Wood Pallet	
IFC	
			
Commenter's Reason: The actual number of the standard referenced in the IFC is FM 4996 and not FM 4496 and the latest (2015) edition was issued December 2015.

Public Comment 6:
Marcelo Hirschler, representing GBH International (gbhint@aol.com) requests Approve as Modified by this Public Comment.

Further modify as follows:

ASTM	ASTM	
Standard Reference Number	
Title	Referenced in Code(s):	

D2859-2016	Standard Test Method for Ignition Characteristics of Finished Textile Floor Covering Materials		

Commenter's Reason: ASTM D2859 has recently been updated to 2016 editions.

Public Comment 7:
Marcelo Hirschler (gbhint@aol.com) requests Approve as Modified by this Public Comment.

Further modify as follows:

ASTM	ASTM	
Standard Reference Number	
Title	Referenced in Code(s):	

E84-2015B E84-2016	Standard Test Method for Surface Burning Characteristics of Building Materials	IBC	IRC	IFC	IMC	IEBC	

Commenter's Reason: ASTM E84 has recently been updated to 2016 editions.

Public Comment 8:
Marcelo Hirschler (gbhint@aol.com) requests Approve as Modified by this Public Comment.

Further modify as follows:

ASTM	ASTM	
Standard Reference Number	
Title	
Referenced in Code(s):	
E108-16	Standard Test Methods for Fire Tests of Roof Coverings			
					
Commenter's Reason: ASTM E108 has recently been updated to 2016 editions.

Public Comment 9:
Jeff Inks, representing Window & Door Manufacturers Association (jinks@wdma.com) requests Approve as Modified by this Public Comment.
Modify as follows:

ASTM	ASTM	
Standard Reference Number	
Title	Referenced in Code(s):	

F2090-13 F2090-17	Specification for Window Fall Prevention Devices with Emergency Escape (Egress) Release Mechanisms	IBC	IRC	IFC	IEBC	

Commenter's Reason: The correct edition to be referenced in the 2018 codes is the 2017 which is nearing completion.

Public Comment 10:
Jeff Inks, representing Window & Door Manufacturers Association (jinks@wdma.com) requests Approve as Modified by this Public Comment.

Modify as follows:

ASTM	ASTM	
Standard Reference Number	
Title	Referenced in Code(s):	

F2006-00 (2005) 1017	Standard/Safety Specification for Window Fall Prevention Devices for Non- emergency Escape (Egress) and Rescue (Ingress) Windows	
IBC	
IEBC	

Commenter's Reason: This standard is currently referenced in the IBC & IEBC and is currently being revised which will result in the 2017 edition however, the update to the code reference update to the 2017 was inadvertently not included in ADM-94 and is therefore included by this public comment.

Public Comment 11:
Bonnie Manley, AISI, representing SJI (bmanley@steel.org) requests Approve as Modified by this Public Comment.

Modify as follows:

SJI	Steel Joist Institute	
Standard Reference Number	
Title	
Referenced in Code(s):	
SJI-200-16 SJI-200-15	Standard Specification for Composite Steel Joists, CJ-Series	IBC	

Commenter's Reason: This modification simply corrects the publication date of SJI 200. A copy of SJI 200-15 is available at: https://steeljoist.org/ansi/.

Final Action Results

ADM94-16	AMPC3, 4, 5,6, 7, 8,9,10, 11