2018 International Building Code (I-Codes) – Administrative Provisions – Accommodate Florida Specific Need
Structural TAC

IBC/IRC/IEBC Code Change No	IBC/IRC/IEBC
Section	Change Summary b/t 2015 IBC/IRC/IEBC and 2018 IBC/IRC/IEBC	Change Summary b/t 2017 FBC/FRC/FEBC and 2018 IBC/IRC/IEBC	Staff comments	
ADM72-16	IRC: R105.3.1.1, R301.2.4, R322.1	Revises section R105.3.1.1 “Determination of substantially improved or substantially damaged existing buildings in flood hazard areas,” revises section R301.2.4 “Floodplain construction,” and revises section R322.1 “General” to clarify the requirements for repair and restoration.

Cost Impact: Will not increase the cost of construction. Clarification of terms does not change the basic requirement.	Section R105.3.1.1 is reserved under the FRC.  For compliance, the code refers to the FBC, B.
Same as change between 2015 IRC and 2018 IRC with regard to R301.2.4 and R3221.	No action needed with regard to R105.3.1.1.	
     TAC Action

X

     Accommodate Florida Specific Need:
     YES (Select Criteria)                                                     NO: 

 X

X

     a.  b.  c.      d.  e.  f. 

Vote 10 Y – 0 N

     Others (Explain):	Commission Action

Accommodate Florida Specific Need:

YES (Select Criteria)                                                               NO: 

 

a.  b.  c.      d.  e.  f. 
Others (Explain):	
    	
TAC	
Cmsn.	

       No Action Needed 	

	

	

  Overlapping provisions     	

	

	

	

	
ADM94-16	Referenced Standards	Revises Referenced Standard table to update the referenced standard list.
Cost Impact: Will not increase the cost of construction. This is just an update of the referenced standards.	Same as change between 2015 I-Codes and 2018 I-Codes With exception of AAMA A440, AAMA 714 ASTM E 1996, ASTM E 1886 – 2013A and ASTM E330.	Overlapping provision to be considered during step 2 of the code change process  - AAMA A440 - 2017, AAMA 714 - 2014, ASTM E1996  - 2014a , ASTM E1886 – 13a and ASTM E330 - 2014

2017 FBC

AAMA/WDMA/CSA
101/I.S.2/A440—05 or 08 or 11

AAMA 714—12 or 15

ASTM E1886—02 or 05 or 12 or 2013a

ASTM E1996—05, 06, 09,
2012a or 2014a

ASTM E330—02 or 14

     TAC Action

X

     Accommodate Florida Specific Need:
     YES (Select Criteria)                                                     NO: 

X

 

X

     a.  b.  c.      d.  e.  f. 

Vote 10Y – 0 N

     Others (Explain):	Commission Action

Accommodate Florida Specific Need:

YES (Select Criteria)                                                               NO: 

 

a.  b.  c.      d.  e.  f. 
Others (Explain):	
    	
TAC	
Cmsn.	

       No Action Needed 	

	

	

  Overlapping provisions