CHAPTER 35

REFERENCED STANDARDS

This chapter lists the standards that are referenced in various sections of this document. The standards are listed herein by the promulgating agency of the standard, the standard identification, the effective date and title, and the section or sections of this document that reference the standard. The application of the referenced standards shall be as specified in Section 102.4.

AA

Aluminum Association

1525 Wilson Boulevard, Suite 600

Arlington, VA 22209

Standard Referenced
reference in code
number Title section number

ADM1—2015 ADM1—2020 Aluminum Design Manual: Part ~~1—A Specification~~ 1—Specification or Aluminum Structures 1604.3.5, 2002.1

ASM 35—00 Aluminum Sheet Metal Work in Building Construction (Fourth Edition) 2002.1

AAF

Aluminum Association of Florida, Inc.

3203 Lawton Road #110

Orlando, FL 32803

Standard Referenced
reference in code
number Title section number

AAF—20 Guide to Aluminum Construction in High Wind Areas (2020) 2002.4.1, 1622.1.2

AAMA

American Architectural Manufacturers Association

1827 Waldon Office Square, Suite 550

Schaumburg, IL 60173

Standard Referenced
reference in code
number Title section number

1402—09 Standard Specifications for Aluminum Siding, Soffit and Fascia 1404.5.1

AAMA/NSA 2100—19 Voluntary Specifications for Sunrooms 202, 2002.6.1, 2002.6.2

AAMA/WDMA/CSA
101/I.S.2/A440—08, 11 or 17 North American Fenestration Standard/Specifications for
  Windows, Doors and Skylights 1010.1.7, 1709.5.1, 2405.5, 2411.3.2.1

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete 1917.4.4

AAMA 501—15 Methods of Test for Exterior Walls 1709.8.4

AAMA 506—16 Voluntary Specifications for Impact and Cycle Testing of Fenestration Products 1609.1.2

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete ……………..1917.4.4, 1507.1.1.2, 1507.1.1.3

711-20 Voluntary Specification for Liquid Applied Flashing Used to Create a Water-resistive Seal around Exterior Wall Openings in Buildings

~~714—15~~**714—20** Voluntary Specification for Liquid Applied Flashing Used to Create a Water-resistive
  Seal around Exterior Wall Openings in Buildings 1405.4

FMA/AAMA 100—12 Standard Practice for the Installation of Windows with Flanges or Mounting 1405.4.1.4

FMA/AAMA 200—12 Standard Practice for the Installation of Windows with Frontal Flanges 1405.4.1.4

FMA/WDMA 250—10 Standard Practice for the Installation of Non-Frontal Flange Windows with

  Mounting Flanges for Surface Barrier Masonry for Extreme Wind/Water Conditions 1405.4.1.4

FMA/AAMA/WDMA300—12 Standard Practice for the Installation of Exterior Doors in Wood Frame

  Construction for Extreme Wind/Water Exposure 1405.4.1.4

FMA/AAMA/WDMA 400-13 Standard Practice for the Installation of Exterior Doors in Surface Barrier
  Masonry Construction for Extreme Wind/Weather Exposure 1405.4.1.4

**Also – revise as follows:**

**AAMA Standards by FGIA**

~~American Architectural Manufacturers Association~~

Fenestration & Glazing Industry Alliance

~~1827 Walden Office Square, Suite 550~~

1900 E Gold Rd., Suite 1250

Schaumburg, IL 60173

*Update the following, all other existing AAMA Standards remain the same:*

450—10                              Voluntary Performance Rating Method for Mulled Fenestration Assemblies 1709.8

or

450-20                                Performance Rating Method for Mulled Combination Assemblies, Composite Units, and Other Mulled Fenestration Systems         1709.8

711— 13 ~~or 16~~, 20 or 22    Voluntary Specification for Self-A~~a~~dhering Flashing Used for Installation of Exterior Wall Fenestration Products 1405.4, Table 1507.1.1.1, 1507.1.1.2, 1507.1.1.3

714—15 or 19                  Voluntary Specification for Liquid Applied Flashing Used to Create Water-resistive Seal around Exterior Wall      Openings in Buildings                             1405.4

**(S10435 AM A2)**

**Add new standards as follows to Chapter 35 under AAMA and WDMA, respectively:**

AAMA 2502-2019, Comparative Analysis Procedure for Window and Door Protocols............1709.5.1

**(S10417 AS)**

ACI

American Concrete Institute

P.O. Box 9094

Farmington Hills, MI 48333-9094

Standard Referenced
reference in code
number Title section number

216.1—14 Code Requirements for Determining Fire Resistance of Concrete
  and Masonry Construction Assemblies Table 721.1(2), 722.1

318—19 ~~318—14~~ Building Code Requirements for Structural Concrete 1604.3.2, 1615.3.1, 1615.4.1,

1808.8.2, Table 1808.8.2, 1808.8.5, 1808.8.6,
1810.1.3, 1810.2.4.1, 1810.3.2.1.1, 1810.3.2.1.2, 1810.3.8.3.1, 1810.3.8.3.3,
1810.3.9.4.2.1, 1810.3.9.4.2.2, 1810.3.10.1, 1810.3.11.1, 1810.3.12, 1901.2, 1901.3,
1902.1, 1903.1, 1904.1, 1904.2, 1905.1, 1905.1.1, 1905.1.2,
1905.1.3, 1905.1.4, 1905.1.5, 1905.1.6, 1905.1.7, 1905.1.8, 1906.1, 2206.1, E303.2.2

**Add new standard(s) as follows:**

**ACI**

117-10: Specification for Tolerances for Concrete Construction and Materials

ITG-7-09: Specification for Tolerances for Precast Concrete

**(S9596 / S147-19 AS)**

AF & PA

American Forest & Paper Association

1111 19th St, NW Suite 800

Washington, DC 20036

Standard Referenced
reference in code
number Title section number

AF&PA—92 Wood Structural Design Data 2314.4.7

AF&PA—05 Design Values for Joists and Rafters 2314.4.7

PWF—07 Permanent Wood Foundation (PWF) Design Specification 2314.4.7

AF&PA—12 Span Tables for Joists and Rafters 2314.4.7, 2317.1.1

WCD 1—01 Wood Construction Data No. 1, Details for Conventional Wood Frame Construction 2314.4.7

WCD 4—03 Wood Construction Data No. 4, Plank and Beam Framing for Residential Buildings 2314.4.7, 2306.1.2

WCD 5—89 Wood Construction Data No. 5, Heavy Timber
  Construction Details 2314.4.7

, 2203.1, 2203.2, 2205.1, 2205.2.1.1, 2206.1

AHA

American Hardboard Association

1210 West N.W. Highway

Palatine, IL 60067

Standard Referenced
reference in code
number Title section number

A135.4—04 Basic Hardboard 1404.3.1, 2314.4.1

A135.5—04 Prefinished Hardboard Paneling 2314.4.1

A135.6—98 Hardboard Siding 2314.4.1

A194.1—85 Cellulosic Fiber Board 2314.4.1

IB Spec. No. 1 Recommended Product and Application Specification —Structural Insulating

Roof Deck 2314.4.1

IB Spec. No. 2 Recommended Product and Application Specification —1/2 inch Fiberboard
  Nail-Base Sheathing 2314.4.1

IB Spec. No. 3 Recommended Product and Application Specification —1/2 inch Intermediate
   Fiberboard Sheathing 2314.4.1

AISC

American Institute of Steel Construction

One East Wacker Drive, Suite 700

Chicago, IL 60601-18021

Standard Referenced
reference in code
number Title section number

AISC DG09 Torsional Analysis of Structural Steel Members 2003, 2214.3

AISC—09 Detailing for Steel Construction 2214.3

AISC—2017 Steel Construction Manual, 2017 2011, 2214.3

AISC DG15—2018 Rehabilitation and Retrofit Guide A Reference for Historic Shapes and Specifications 2214.3

AISC—continued

AISC DG03 Serviceability Design Considerations for Steel Buildings, 2003 2214.3

ANSI/AISC 341—16 Seismic Provisions for Structural Steel Buildings 1613.4.1, 2205.2.1.1, 2205.2.1.2, 2205.2.2, 2206.2.1

ANSI/AISC 360—16 Specification for Structural Steel Buildings 722.5.2.2.1, 1604.3.3,

2203.1, 2203.2, 2205.1, 2205.2.1.1, 2206.1

**Also – revise as follows:**

AISC

American Institute of Steel Construction

~~One East Wacker Drive, Suite 700~~

130 East Randolph, Suite 2000

Chicago, IL 60601~~-18021~~

AISC DG09-2003, Torsional Analysis of Structural Steel Members, 2003

                        ~~2003,~~2214.3

~~AISC-09, Detailing for Steel Construction~~

~~2214.3~~

AISC-2017, Steel Construction Manual, 2017

                        2214.3

AISC DG15-2018, Rehabilitation and Retrofit~~Guide: A Reference for Historic Shapes and Specifications~~, 2018

                        2214.3

AISC DG03-2003, Serviceability Design Considerations for Steel Buildings, 2003

                        2214.3

**(S10131 AS)**

AISI

American Iron and Steel Institute

25 Massachusetts Avenue, NW Suite 800

Washington, DC 20001

Standard Referenced
reference in code
number Title section number

AISI S100—16/S1-18 North American Specification for the Design of Cold-formed Steel
  Structural Members with supplement 1 dated 2018 1604.3.3, 1905.1.8, 2203.1, 2203.2,

2210.1, 2210.2, 2214.3

AISI S202—~~15~~20 Code of Standard Practice for Cold-formed Steel Framing, 2015 2211.3.1

AISI S220—~~15~~20 North American Standard for Cold-formed Steel Framing-Nonstructural Members, 2015 2203.1, 2203.2,

2211.1, 2211.2, 2214.3, Table 2506.2, Table 2507.2

AISI S230—~~19~~18 Standard for Cold-formed Steel Framing-Prescriptive Method for
  One- and Two-family Dwellings, 2019 1609.1.1,

1609.1.1.1, 2211.1.2, 2214.3

AISI S240—~~15~~20

 AISI S240, North American Standard for Cold-formed Steel Structural Framing, 2015 2203.1, 2203.2,

2211.1, 2214.3, 2211.1.1.1, Table 2306.12.2, Table 2506.2,

Table 2507.2, Table 2603.12.1

(S299—16)

AISI S400—15/S1—~~16~~20 North American Standard for Seismic Design of Cold-formed Steel Structural Systems, 2015, with

  Supplement 1, dated 2016 2210.2, 2211.1.1.1, 2211.1.1.2

AISI S913—17 Test Standard for Hold-Downs Attached to Cold-Formed Steel Structural Framing 2210.3

AISI S914—17 Test Standard for Joist Connectors Attached to Cold-Formed Steel Structural Framing 2210.3

|  |
| --- |
| **Also – revise as follows:** |

|  |
| --- |
| AISIAISI S100—16(2020) w/S2-20     North American Specification for the Design of Cold-formed Steel Structural Members, 2016 Edition (Reaffirmed 2020), with Supplement 2, 2020 Edition1604.3.3, 1905.1.8, 2203.1, 2203.2, 2210.1, 2210.2, 2214.3AISI S202—20~~15~~     Code of Standard Practice for Cold-formed Steel Framing, 2020~~2015~~            2211.1.3.1AISI S220—20~~15~~     North American Standard for Cold-formed Steel Framing-Nonstructural Members, 2020~~2015~~2203.1, 2203.2, 2211.1, 2211.2, 2214.3, Table 2506.2, Table 2507.2AISI S230—19    Standard for Cold-formed Steel Framing-Prescriptive Method for One- and Two-family Dwellings, 20191609.1.1, 1609.1.1.1, 2211.1.2, 2214.3AISI S240—20~~15~~     AISI S240, North American Standard for Cold-formed Steel Structural Framing, 2020~~2015~~2203.1, 2203.2, 2211.1, 2214.3, 2211.1.1.1, Table 2506.2, Table 2507.2, Table 2603.12.1~~(S299—16)~~AISI S400—20~~15/S1—16~~             North American Standard for Seismic Design of Cold-formed Steel Structural Systems, 2020~~2015~~, ~~with Supplement 1, dated 2016~~2210.2, 2211.1.1.1, 2211.1.1.2AISI S913—17     Test Standard for Hold-Downs Attached to Cold-Formed Steel Structural Framing2210.3CAISI S914—17     Test Standard for Joist Connectors Attached to Cold-Formed Steel Structural Framing2210.3 |
|   |
|  |

(S10454 AS)

AITC

American Institute of Timber Construction

333 West Hampden Avenue

Englewood, CO 80110

Standard Referenced
reference in code
number Title section number

A 190.1—07 Structural Glued Laminated Timber 2314.4.2

Technical Note 7—96 Calculation of Fire Resistance of Glued Laminated Timbers 2314.4.2

104—03 Typical Construction Details 2306.1, 2314.4.2

106 Code of Suggested Practices 2314.4.2

108—93 Standard for Heavy Timber Construction 2314.4.2

109—98 Standard for Preservative Treatment for Structural Glued Laminated Timber 2314.4.2

110—01 Standard Appearance Grades for Structural Glued Laminated Timber 2306.1, 2314.4.2

112—93 Tongue-and-Groove Heavy Timber Roof Decking 2314.4.2

113—10 Dimensions of Structural Glued Laminated Timber 2306.1, 2314.4.2

117—10 Standard Specifications for Structural Glued Laminated Timber of Softwood
  Species—Design Requirements—Standard Specifications for Structural Glued
  Laminated Timber of Softwood Species—Manufacturing Requirements 2314.4.2

119—96 Standard Specifications for Structural Glued Laminated Timber of

Hardwood Species 2306.1, 2314.4.2

ALI

Automotive Lift Institute

P.O. Box 85

Courtland, NY 13045

Standard Referenced
reference in code
number Title section number

ALI ALCTV—2017 Standard for Automotive Lifts—Safety Requirements for
  Construction, Testing and Validation (ANSI) 3001.2, Table 3001.2

AMCA

Air Movement and Control Association International

30 West University Drive

Arlington Heights, IL 60004

Standard Referenced
reference in code
number Title section number

540—13 Test Method for Louvers Impacted by Wind Borne Debris 1609.1.2.1, 1626.5.1, 1626.5.2, 1626.5.3

ANSI

American National Standards Institute

25 West 43rd Street, Fourth Floor

New York, NY 10036

Standard Referenced
reference in code
number Title section number

~~A13.1—2015~~ A13.1—2020 Scheme for the Identification of Piping Systems 415.11.6.5

A41.1 Building Code Requirements for Masonry 2121.2.8

A108.1A—~~16~~17 Installation of Ceramic Tile in the Wet-set Method, with Portland Cement Mortar 2103.2.3

A108.1B—~~99~~ 17 Installation of Ceramic Tile, quarry Tile on a Cured Portland
  Cement Mortar Setting Bed with Dry-set or Latex-Portland Mortar 2103.2.3

A108.4—~~99~~09 Installation of Ceramic Tile with Organic Adhesives or
  Water-cleanable Tile-setting Epoxy Adhesive 2103.2.3.6

A108.5—~~99~~19 Installation of Ceramic Tile with Dry-set Portland Cement Mortar
  or Latex-Portland Cement Mortar 2103.2.3.1, 2103.2.3.2

A108.6—~~99~~19 Installation of Ceramic Tile with Chemical-resistant, Water
  Cleanable Tile-setting and -grouting Epoxy 2103.2.3.3

A108.8—~~99~~19 Installation of Ceramic Tile with Chemical-resistant Furan Resin Mortar and Grout 2103.2.3.4

A108.9—~~99~~19 Installation of Ceramic Tile with Modified Epoxy Emulsion Mortar/Grout 2103.2.3.5

A108.10—~~99~~17 Installation of Grout in Tilework 2103.2.3.7

A117—2015 Structural Glued Laminated Timber of Softwood Species 2306.1, 2314.4.3

A118.1—~~16~~18 American National Standard Specifications for Dry-set Portland Cement Mortar 2103.2.3.1

A118.3—~~13~~20 American National Standard Specifications for Chemical-resistant, Water-cleanable
  Tile-setting and -grouting Epoxy and Water Cleanable Tile-setting Epoxy Adhesive 2103.2.3.3

A118.4—~~16~~18 American National Standard Specifications for Latex-Portland Cement Mortar 2103.2.4, 2103.2.3.2

A118.5—99 American National Standard Specifications for
  Chemical Resistant Furan Mortar and Grouts for Tile Installation. 2103.2.3.4

A118.6—~~10~~19 American National Standard Specifications for Cement Grouts for Tile Installation 2103.2.3.7

A118.8—99 American National Standard Specifications for Modified Epoxy Emulsion Mortar/Grout 2103.2.3.5

A136.1—~~08~~19 American National Standard Specifications for
  Organic Adhesives for Installation of Ceramic Tile 2103.2.3.6

A137.1—~~17~~19 American National Standard Specifications for Ceramic Tile 202

ANSI/A190.1—17 Structural Glued Laminated Timber 2303.1.3, 2306.1, 2314.4.3

ANSI B18.6.1-81(2016) Wood Screws (Inch Series) 1506.6

Z535.1 American National Standard Safety Color Code for Making Physical Hazards 453.4.6, 453.14.6

Z358.1 Emergency Eyewash and Shower Equipment 450.3.11.7

Z97.1—14 Safety Glazing Materials Used in Buildings—Safety Performance
  Specifications and Methods of Test 1618.4.6.3, 2406.1.2, 2406.2, Table 2406.2(2), 2406.3.1,

 2407.1, 2407.1.4.1, 2408.2.1, 2408.3, 2409.2, 2409.3, 2409.4.1

**Add new standard(s) as follows:**

**ANSI**

A137.3-17: American National Standard Specifications for Gauged Porcelain Tiles and Gauged Porcelain Tile Panels/Slabs

**(S9328/FS1-19 AS)**

APA

APA - Engineered Wood Association

7011 South 19th

Tacoma, WA 98466

Standard Referenced
reference in code
number Title section number

ANSI 117—~~2015~~20 Structural Glued Laminated Timber of Softwood Species 2306.1, 2314.4.3

ANSI/A 190.1—2017 Structural Glued Laminated Timber 2303.1.3, 2306.1

ANSI/APA PRP 210—~~2014~~ 2019 Standard for Performance-Rated Engineered Wood Siding 2303.1.5, 2304.7, 2306.3, Table 2306.3(1)

ANSI/APA PRG 320—2019 Standard for Performance-rated Cross-laminated Timber

ANSI/APA PRR 410—2016 Standard for Performance-Rated Engineered Wood Rim Boards 2303.1.13

APA PDS—~~12~~PDS-20 Panel Design Specification 2306.1, 2314.4.3

APA PDS
Supplement 1—12 Design and Fabrication of Plywood Curved Panels (revised 2013) 2306.1, 2314.4.3

APA PDS
Supplement 2—12 Design and Fabrication of Plywood-lumber Beams (revised 2013) 2306.1, 2314.4.3

APA PDS
Supplement 3—12 Design and Fabrication of Plywood Stressed-skin Panels (revised 2013) 2306.1, 2314.4.3

APA PDS
Supplement 4—12 Design and Fabrication of Plywood Sandwich Panels (revised 2013) 2306.1, 2314.4.3

APA PDS
Supplement 5—16 Design and Fabrication of All-plywood Beams 2306.1, 2314.4.3

APA B840—16 303 Siding Manufacturing Specifications 2314.4.3

APA L350—07 Design/Construction Guide Diaphragms and Shearwalls 2314.4.3

APA PRP-108—18 Performance Standards and Policies for Wood Structural Panels 2314.4.3

APA V910—90 Plywood Folded Plate Laboratory Report 121 2314.4.3

APA EWCG Engineered Wood Construction Guide, Form E30 2314.4.3

APA R540—~~13~~19 Builder~~s~~ Tips: Proper Storage and Handling of Glulam Beams 2306.1

APA S475—~~16~~20 Glued Laminated Beam Design Tables 2306.1

APA S560—~~14~~20 Field Notching and Drilling of Glued Laminated Timber Beams 2306.1

APA T300—16 Glulam Connection Details 2306.1

APA X440—17 Product and Application Guide: Glulam 2306.1

APA X450—18 Glulam in Residential Building Construction Guide-~~Western Edition~~ 2306.1

APA E30—16 Engineered Wood Construction Guide 2314.4.3

**(S10107 AS)**

**APA**

**Also – revise as follows:**

APA - Engineered Wood Association

7011 South 19th

Tacoma, WA 98466

ANSI 117—2020 Standard Specification for Structural Glued Laminated Timber of Softwood Species . . . . . . . . . . . 2306.1, 2314.4.3

~~ANSI/A 190.1~~ ANSI A190.1.—~~2017~~2022 Product Standard for Structural Glued Laminated Timber. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .2303.1.3, 2306.1

ANSI/APA PRP 210—2019 Standard for Performance-Rated Engineered Wood Siding . . . . 2303.1.5, 2304.7, 2306.3, Table 2306.3(1)

ANSI/APA PRR 410—2021 Standard for Performance-Rated Engineered Wood Rim Boards . . . . . . . . . . . . . . . . . . . . . . . . . . 2303.1.13

APA PDS—20 Panel Design Specification . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .2306.1, 2314.4.3

APA PDS Supplement 1—12 Design and Fabrication of Plywood Curved Panels (revised 2013) . . . . . . . . . . . . . . . . . . .2306.1, 2314.4.3

APA PDS Supplement 2—12 Design and Fabrication of Plywood-lumber Beams (revised 2013) . . . . . . . . . . . . . . . . . . .2306.1, 2314.4.3

APA PDS Supplement 3—12 Design and Fabrication of Plywood Stressed-skin Panels (revised 2013). . . . . . . . . . . . . . .2306.1, 2314.4.3

APA PDS Supplement 4—12 Design and Fabrication of Plywood Sandwich Panels (revised 2013) . . . . . . . . . . . . . . . . .2306.1, 2314.4.3

APA PDS Supplement 5—16 Design and Fabrication of All-plywood Beams. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .2306.1, 2314.4.3

APA B840—19 303 Siding Manufacturing Specifications . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2314.4.3

APA L350—07 Design/Construction Guide Diaphragms and Shearwalls . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2314.4.3

APA PRP-108—21 Performance Standards and Policies for Wood Structural Panels . . . . . . . . . . . . . . . . . . . . . . . . . . . 2314.4.3

APA V910—90 Plywood Folded Plate Laboratory Report 121. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2314.4.3

APA E30-19 Engineered Wood Construction Guide . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2314.4.3

APA R540—19 Builders Tips: Proper Storage and Handling of Glulam Beams . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .2306.1

APA S475—20 Glued Laminated Beam Design Tables . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .2306.1

APA S560—20 Field Notching and Drilling of Glued Laminated Timber Beams . . . . . . . . . . . . . . . . . . . . . . . . . . . . .2306.1

APA T300—16 Glulam Connection Details . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .2306.1

APA X440—17 Product and Application Guide: Glulam . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .2306.1

APA X450—18 Glulam in Residential Building Construction Guide-Western Edition . . . . . . . . . . . . . . . . . . . . . . . . .2306.1

A

**(SW10438 AS)/ (S10107 AS)**

APSP

Association of Pool and Spa Professionals

2111 Eisenhower Avenue, Suite 500

Alexandria, VA 22314

Standard Referenced
reference in code
number Title section number

ANSI/APSP/ICC 3—14 American National Standard for Permanently

 Installed Residential Spas and Swim Spas 454.2.6.1

ANSI/APSP/ICC 4—12 American National Standard for Aboveground **/**Onground Residential Swimming Pools
  Includes Addenda A Approved April 4, 2013 454.2.6.1

ANSI/APSP/ICC 5-11 American National Standard for Residential

 Inground Swimming Pools 454.2.6.1

ANSI/APSP/ICC 6—13 American National Standard for Residential

 Portable Spas and Swim Spas 454.2.6.1

ANSI/APSP/ICC 7—13 American National Standard for Suction

 Entrapment Avoidance in
  Swimming Pools,

 Wading Pools, Spas, Hot Tubs, and Catch

 Basins 454.2.6.1, 454.2.6.3, 454.2.6.6

ANSI/APSP 16—2017 American National Standard for Suction Fittings
  for Use in Swimming Pools, Wading Pools, Spas,

 and Hot Tubs 454.1.6.5.12

**Revise as follows:**

**APSP (PHTA Standards)**

Pool & Hot Tub Alliance

~~Association of Pool and Spa Professionals~~

2111 Eisenhower Avenue, Suite 500

Alexandria, VA 22314

ANSI/APSP/ICC 3—2014

American National Standard for Permanently Installed Residential Spas and Swim Spas

454.2.6.1

ANSI/APSP/ICC 4—2012(R2022)

American National Standard for Aboveground /Onground Residential Swimming Pools ~~Includes Addenda A Approved April 4, 2013~~

454.2.6.1

ANSI/APSP/ICC 5-~~11~~2012(R2022)

American National Standard for Residential Inground Swimming Pools

454.2.6.1

ANSI/APSP/ICC 6—2013

American National Standard for Residential Portable Spas and Swim Spas

454.2.6.1

ANSI/~~APSP~~PHTA/ICC 7—~~13~~2020

American National Standard for Suction Entrapment Avoidance in Swimming Pools, Wading Pools, Spas, Hot Tubs, and Catch Basins

454.2.6.1, 454.2.6.3, 454.2.6.6

ANSI/APSP 16—2017

American National Standard for Suction Outlet Fitting~~s~~ Assemblies (SOFA) for Use in ~~Swimming~~ Pools, ~~Wading Pools,~~ Spas, and Hot Tubs

454.1.6.5.12

**(SW10522 AM A1)**

ASABE

American Society of Agricultural and Biological Engineers

2950 Niles Road

St. Joseph, MI 49085

Standard Referenced
reference in code
number Title section number

EP 484.3
(R2008) MON ~~2016~~DEC2017 Diaphragm Design of Metal-clad, Wood-frame Rectangular Buildings 2306.1

EP ~~486.2 OCT 2012 ED~~486.3 SEP2017

 Shallow-post and Pier Foundation Design 2306.1

EP 559.1 W/Corr.(2010)2014 Design Requirements and Bending Properties for Mechanically

  Laminated Wood Assemblies 2306.1

ASCE/SEI

American Society of Civil Engineers

Structural Engineering Institute

1801 Alexander Bell Drive

Reston, VA 20191-4400

Standard Referenced
reference in code
number Title section number

7—16with Supplement 1 Minimum Design Loads and Associated Criteria for Buildings and
  Other Structures with Supplement No. 1 202, 449.4.2.2.6, 450.4.2.2.6,

453.4.7, 453.9.1, 453.25.4.1, Table 1504.3.3, Table 1507.2.7.1, 1510.7.1,

1514.4, 1514.4.2, 1514.4.3, 1525, 1602.1, 1604.3, 1604.4, Table 1604.5, 1604.8.2,

1604.10, 1605.1, 1605.2.1, 1605.3.1, 1605.3.1.2, 1605.3.2, 1605.3.2.1, 1607.8.1, 1607.8.1.1,
1607.8.1.2, 1607.8.3, 1607.12.1, 1607.12.3.1, 1608.1, 1608.2, 1608.3, 1609.1.1, 1609.1.2,

 1609.1.2.4.1, 1609.1.2.4.2, 1609.3, 1609.5.1, 1609.5.3, 1609.8, 1611.2, 1612.4,

1613.1, Table 1613.3.3(1), Table 1613.3.3(2), 1613.3.5, 1613.3.5.1, 1613.3.5.2,

1613.4, 1613.4.1, 1613.5.1, 1613.6, 1614.1, 1616.5, 1620.1, 1620.3, 1620.6, 1621.1,

1621.2, 1622.1.1, Table 1625.4, 1626.1, Table 1626, 1709.5.2.1, 1709.8.3,

 1803.5.12, 1808.3.1, 1810.3.6.1, 1810.3.9.4, 1810.3.11.2, 1810.3.12, 1905.1.1, 1905.1.2,

1905.1.7, 1905.1.8, Table 2002.4, 2205.2.1.1, 2205.2.1.2, 2205.2.2, 2206.2.1, 2209.1, 2209.2,

2210.2, 2211.1.1.1, Table 2304.6.1, Table 2306.3(3), 2314.1, 2319.13, 2322.2.3, 2322.2.5,

2404.1, 2505.1, 2505.2, 2506.2.1, 3109.3.1, 3115.2.3, 3115.4.4

8—02 Specification for the Design of Cold-formed
  Stainless Steel Structural Members 1604.3.3, 2210.1, 2210.2, 2214.3

19—16 Structural Applications of Steel Cables for Buildings 2208.1

24—~~14~~20 Flood Resistant Design and Construction 453.4.2, 1203.4.2, 1603.1.7, 1612.4, 1612.4.1, 1612.4.2,

1612.5, 2702.1.7, 3001.2, 3101.3.2.2, 3109.2, 3109.3, 3109.3.2.1, 3109.3.3, 3109.3.4

29—~~2014~~19 Standard Calculation Methods for Structural Fire Protection 722.1

32—01 Design and Construction of Frost Protected Shallow Foundations 1809.5

49—12 Wind Tunnel Testing for Buildings and Other Structures 1609.1.1

55—16 Tensile Membrane Structures 3102.1.1

**Also – revise as follows:**

ASCE/SEI          American Society of Civil Engineers

                        Structural Engineering Institute

                        1801 Alexander Bell Drive

                        Reston, VA 20191-4400

Standard reference number        Title

7-~~16~~ 22                                    Minimum Design Loads and Associated Criteria for Buildings and Other Structures ~~with Supplement No. 1~~

ASHRAE

ASHRAE, Inc.

1791 Tullie Circle NE

Atlanta, GA 30329-2305

Standard Referenced
reference in code
number Title section number

62—01 Ventilation for Acceptable Indoor Air Quality C502.1, E306.1

ANSI/ASHRAE/
ASJHE 170—08 Ventilation of Heath Care Facilities 450.3.14, 450.3.14.4, 469.4.12.1

ASME

American Society of Mechanical Engineers

Two Park Avenue

New York, NY 10016-5990

Standard Referenced
reference in code
number Title section number

ASME/A17.1—~~2016~~2019 2019/
CSA B44—~~16~~19 Safety Code for Elevators and Escalators 469.4.9.1, 907.3.3, 911.1.6, 1607.9.1,

3001.2, 3001.1, Table 3001.2, 3001.4, 3001.6, 3002.5, 3002.10, 3003.2,

3007.1, 3008.1.3, 3008.7.1, 3010.1.3, 3010.3, 3012.1

A17.3—2015 Safety Code for Existing Elevators and Escalators 469.4.9.1, 3001.1, 3001.2,

3001.5.3, 3010.1.3, 3012.1

ASME A17.6-2010 Standard for Elevator Suspension, Compensation, and Governor Systems Safety Table 3001.2

A17.7—2007/
CSA B44—07 ~~(R2012)~~(R2019) Performance-Based Safety Code for Elevators and Escalators Table 3001.2

A18.1—~~2017~~2020 Safety Standard for Platform Lifts and Stairway Chairlifts 3001.1, Table 3001.2, 3012.1

A90.1—~~2015~~2020 Safety Standard for Belt Manlifts Table 3001.2, 3001.6

A112.19.8 Suction Fittings for Use in Swimming Pools, Wading Pools, spas, Hot Tubs,
  and Whirlpool Bathtub Appliances 454.1.6.5.3.2.3

A120.1—01 Safety Requirements for Powered Platforms for Building Maintenance 3001.6

B16.18—~~2012~~2018 Cast Copper Alloy Solder Joint Pressure Fittings 909.13.1

B16.22—~~2013~~2018 Wrought Copper and Copper Alloy Solder Joint Pressure Fittings 909.13.1

B20.1—~~2015~~2021 Safety Standard for Conveyors and Related Equipment Table 3001.2, 3001.6, 3004.3

B31.3—~~2016~~2020 Process Piping 415.11.6

18.6.1—81(2016) Wood Screws (Inch Series) 1506.6

A13.1—~~2015~~2020 Scheme for the Identification of Piping Systems 415.11.6.5

ASSE

American Society of Safety Engineers

1800 East Oakton Street

Des Plaines, IL 60018

Standard Referenced
reference in code
number Title section number

ANSI/ASSE Z359.1-~~2016~~2019

~~Requirements for the ANSI/ASSE Z359~~ The Fall Protection Code 1015.6, 1015.7

ASTC1569-03(2016): Standard Test Method for Wind Resistance of Concrete and Clay Roof Tiles (Wind Tunnel Method)

**(R9953 AS)/** **(R9508 / S14-19)**

ASTM

ASTM International

100 Barr Harbor Drive

West Conshohocken, PA 19428-2959

Standard Referenced
reference in code
number Title section number

A6/~~A6M—14~~ A6M--2017A Standard Specification for General Requirements for Rolled Structural
  Steel Bars, Plates, Shapes and Sheet 1810.3.2.3, 1810.3.5.3.1, 1810.3.5.3.3, 2214.3

A36/A36M—14 Specification for Carbon Structural Steel 1810.3.2.3

A90/A90M—13 Standard Test Method for Weight (Mass) of Coating on Iron and
  Steel Articles with Zinc or Zinc Alloy Coatings 1506.7

A153/~~A153M—09~~A153M—

2016A Specification for Zinc Coating (Hot-dip) on Iron and Steel Hardware 2304.10.5

A240/A240M—(2015b) A240M

—17 Standard Specification for Chromium-nickel Stainless Steel Plate,
  Sheet and Strip for Pressure Vessels and General Applications 1506.7, Table 1507.4.3(1)

A252—~~10~~A252—2010(2018) Specification for Welded and Seamless Steel Pipe Piles 1810.3.2.3

A283/A283M—~~13~~ 2018 Specification for Low and Intermediate Tensile Strength Carbon Steel Plates 1810.3.2.3

A361 Specification for Steel Sheet Zinc-Coated (Withdrawn) 2319.17.1.1

A416/~~A416M—15~~ **A416M— 2017A** Specification for Steel Strand, Uncoated Seven-wire for Prestressed Concrete 1810.3.2.2

A446 Specification for Steel Sheet, Zinc-coated (Galvanized) by the Hot-Dip Process,
  Structural (Physical) Quality 1917.4.3

A463/A463M—15 Standard Specification for Steel Sheet, Aluminum-coated, by the Hot-dip Process Table 1507.4.3(2)

A525—87 Specification for General Requirements for Steel Sheet, Zinc-Coated
  (Galvanized) by the Hot-Dip Process 1917.4.3

A572/A572M—~~15~~ 2018 Specification for High-strength Low-alloy Columbium-Vanadiu2m Structural Steel 1810.3.2.3

A588/A588M—15 Specification for High-strength Low-alloy Structural Steel with
  50 ksi (345 MPa) Minimum Yield Point with Atmospheric Corrosion Resistance 1810.3.2.3

A611 Standard Specification for Structural Steel (SS), Sheet, Carbon, Coil-Rolled 1917.4.3

A615/A615M—15ae1 Specification for Deformed and Plain Carbon-steel Bars for Concrete Reinforcement 1810.3.10.2

A641/A641M—14 Standard Specification for Zinc-Coated (Galvanized) Carbon Steel Wire 1506.6

A653/A653M—~~15~~2017 Specification for Steel Sheet, Zinc-coated Galvanized or Zinc-iron
   Alloy-coated Galvannealed by the Hot-dip Process Table 1507.4.3(1),

Table 1507.4.3(2), 2304.10.5.1, 2319.17.2.2.7

A690/A690M—13a(2018) Standard Specification for High-strength Low-alloy Nickel, Copper,
  Phosphorus Steel H-piles and Sheet Piling with Atmospheric Corrosion Resistance
  for Use in Marine Environments 1810.3.2.3

A706/A706M—~~15~~ 2016 Specification for Low-alloy Steel Deformed and Plain Bars
  for Concrete Reinforcement 1704.5, 2107.3

A722/A722M—~~15~~2018 Specification for High-strength Steel Bar for Prestressing Concrete 1810.3.10.2

A755/A755M—~~15~~ 2016E1 Specification for Steel Sheet, Metallic-coated by the Hot-dip
  Process and Prepainted by the Coil-coating Process for
  Exterior Exposed Building Products Table 1507.4.3(1), Table 1507.4.3(2)

A792/A792M—10(2015) Specification for Steel Sheet, 55% Aluminum-zinc Alloy-coated
  by the Hot-dip Process Table 1507.4.3(1), Table 1507.4.3(2)

A875/A875M—13 Standard Specification for Steel Sheet Zinc-5 percent,
  Aluminum Alloy-coated by the Hot-dip Process Table 1507.4.3(2)

A924/A924M—~~14~~ 2017A Standard Specification for General Requirements for Steel
  Sheet, Metallic-coated by the Hot-dip Process Table 1507.4.3(1), 2319.17.1.1, 2319.17.2.2.7

A1003/A1003M—15 Standard Specification for Sheet Steel, Carbon, Metallic, and Non-metallic Coated
  for Cold-formed Steel Framing Members 2214.3

A1064A/A1064M—16a Carbon-Steel Wire and Welded Wire Reinforcement, Plain and Deformed, for Concrete 1907.2

B42—2015A Specification for Seamless Copper Pipe, Standard Sizes 909.13.1

B43—15 Specification for Seamless Red Brass Pipe, Standard Sizes 909.13.1

B68/B68M—11 Specification for Seamless Copper Tube, Bright Annealed (Metric) 909.13.1

~~B88—14~~B88-2016 Specification for Seamless Copper Water Tube 909.13.1

B101—12 Specification for Lead-coated Copper Sheet and Strip
  for Building Construction 1404.5.3, Table 1507.4.3(1)

B117—16 Standard Practice for Operating Salt Spray (Fog) Apparatus 1506.6

B209—14 Specification for Aluminum and Aluminum Alloy Steel and Plate Table 1507.4.3(1)

ASTM—continued

B251—~~10~~2017 Specification for General Requirements for Wrought Seamless
  Copper and Copper-alloy Tube 909.13.1

B280—~~13~~2018 Specification for Seamless Copper Tube for Air Conditioning
  and Refrigeration Field Service 909.13.1

B370—12 Specification for Copper Sheet and Strip for
  Building Construction 1404.5.2, Table 1507.4.3(1)

B695—04~~(2009)~~(2016) Standard Specification for Coatings of Zinc Mechanically
  Deposited on Iron and Steel Strip for Building Construction 2304.10.5.1, 2304.10.5.3

C5—~~10~~ 2018 Specification for Quicklime for Structural Purposes Table 2507.2

C22/C22M-00(2015) Specification for Gypsum Table 2506.2

C27—98~~(13)~~ (2018) Specification for Classification of Fireclay and High-alumina Refractory Brick 2111.6

C28/C28M—10(2015) Specification for Gypsum Plasters Table 2507.2

C31/C31M—~~15~~ 2018B Practice for Making and Curing Concrete Test Specimens in the Field Table 1705.3

C33/C33M—~~13~~ 2018 Specification for Concrete Aggregates 722.3.1.4, 722.4.1.1.3

C35/C35M-1995(2014) Specification for Inorganic Aggregates for Use in Gypsum Plaster Table 2507.2

C55—~~2014A~~ 2017 Specification for Concrete Building Brick Table 722.3.2

C59/C59M—00 (2015) Specification for Gypsum Casting Plaster and Molding Plaster Table 2507.2

C61/C61M—00 (2015) Specification for Gypsum Keene’s Cement Table 2507.2

C62—~~13A~~ 2017 Standard Specification for Building Brick
  (Solid Masonry Units Made from Clay or Shale) 1807.1.6.3

C67—~~14~~ 2018 Test Methods of Sampling and Testing Brick and Structural Clay Tile 721.4.1.1.1

C73—~~14~~  2017 Specification for Calcium Silicate Brick (Sand-lime Brick) Table 722.3.2

C90—~~14~~ 2016A Specification for Loadbearing Concrete Masonry Units Table 722.3.2, 1807.1.6.3, 2109.3

C91/C91M—~~12~~ 2018 Specification for Masonry Cement Table 2507.2

C94/C94M—~~15A~~ 2017A Specification for Ready-Mixed Concrete E202, E303.2.1

C140/C140M—~~15~~ 2018 Test Method Sampling and Testing Concrete Masonry Units and Related Units 722.3.1.2

C150/C150M—~~15~~ 2018 Specification for Portland Cement 1903.1, Table 2507.2

C172/C172M—~~14A~~ 2017 Practice for Sampling Freshly Mixed Concrete Table 1705.3, E303.2.4

C199—84 ~~(2011)~~(2016) Test Method for Pier Test for Refractory Mortars 2111.6, 2111.9, 2113.12

C206—14 Specification for Finishing Hydrated Lime Table 2507.2

C208—12(2017)E1 Specification for Cellulosic Fiber Insulating Board Table 1508.2, 2303.1.6

C216—~~15~~ 2017A Specification for Facing Brick (Solid Masonry Units Made from Clay or Shale) Table 721.1(2),

1807.1.6.3

C270—14A Specification for Mortar for Unit Masonry 2103.3.2.4

C315—07(~~2011~~2016) Specification for Clay Flue Liners and Chimney Pots 2111.9, 2113.11.1, Table 2113.16(1)

C317/C317M—00(2015) Specification for Gypsum Concrete 2514.1

C330/C330M—~~14~~ 2017A Specification for Lightweight Aggregates for Structural Concrete 202

C331/C331M—~~2014~~ 2017 Specification for Lightweight Aggregates for Concrete Masonry Units 722.3.1.4, 722.4.1.1.3

C332—09 Specification for Lightweight Aggregates for Insulating Concrete 1917.4.5

C406/C406M—15 Specification for Roofing Slate 1507.7.5

C472—99(2014) Specification for Standard Test Methods for Physical Testing of
  Gypsum, Gypsum Plasters and Gypsum Concrete Table 2506.2

C473—~~15~~ 2017 Test Method for Physical Testing of Gypsum Panel Products Table 2506.2

C474—15 Test Methods for Joint Treatment Materials for Gypsum Board Construction Table 2506.2

C475/C475M—~~15~~  2017 Specification for Joint Compound and Joint Tape for Finishing Gypsum Board Table 2506.2

C476—19 Standard Specification for Grout for Masonry 2122.8.2

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete 1917.4.4

C495—99a Standard Test Method for Compressive Strength of Lightweight
  Insulating Concrete Table 1508.2,

 1917.1.1, 1917.1.2, 1917.1.3

C509—00 Elastomeric Cellular Preformed Gaskets and Sealing Material 2411.3.4

C513 Standard Test Method for Obtaining and Testing Specimens of Hardened Lightweight
  Insulating Concrete for Compressive Strength Table 1508.2

C514—04(2014) Specification for Nails for the Application of Gypsum Board Table 721.1(2), Table 721.1(3),

Table 2506.2

C516—08(~~2014~~ 2013)E1 Specifications for Vermiculite Loose Fill Thermal Insulation 722.3.1.4, 722.4.1.1.3

C547—~~15~~ 2017 Specification for Mineral Fiber Pipe Insulation Table 721.1(2), Table 721.1(3)

C549—06(2012) Specification for Perlite Loose Fill Insulation 722.3.1.4, 722.4.1.1.3

C552—~~15~~ 2017E1 Standard Specification for Cellular Glass Thermal Insulation Table 1508.2

C557—03(~~2009~~ 2017)e01 Specification for Adhesives for Fastening Gypsum Wallboard to Wood Framing Table 2506.2, 2508.4

C578—~~15~~18 Standard Specification for Rigid, Cellular Polystyrene
  Thermal Insulation Table 1508.2, 1917.4.10, 2603.10, Table 2603.12.1, Table 2603.12.2

C587—04(~~2014~~2018) Specification for Gypsum Veneer Plaster Table 2507.2

C595/C595—~~14E1~~ 2018 Specification for Blended Hydraulic Cements 1903.1, Table 2507.2

ASTM—continued

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete 1917.4.4

C631—09(2014) Specification for Bonding Compounds for Interior Gypsum Plastering Table 2507.2

C635/C635M—~~13A~~ 2018 Specification for the Manufacture, Performance and Testing of
  Metal Suspension Systems for Acoustical Tile and Lay-in Panel Ceilings 808.1.1.1, 2506.2.1

C636/C636M—13 Practice for Installation of Metal Ceiling Suspension
  Systems for Acoustical Tile and Lay-in Panels 808.1.1.1

C645—14 Specification for Nonstructural Steel Framing Members 2319.17.1.3

C652—~~15~~ 2017A Specification for Hollow Brick (Hollow Masonry Units Made from Clay or Shale) 1807.1.6.3

C726—~~12~~ 2017 Standard Specification for Mineral Roof Insulation Board Table 1508.2

C728—~~15~~ 2017A Standard Specification for Perlite Thermal Insulation Board Table 1508.2

C744—~~14~~  2016 Specification for Prefaced Concrete and Calcium Silicate Masonry Units Table 722.3.2

C754—~~15~~ 2018 Specification for Installation of Steel Framing Members
  to Receive Screw-attached Gypsum Panel Products Table 2508.1, Table 2511.1.1

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete 1917.4.4

C796—97 Standard Test Method for Foaming Agents For Use in Producing Cellular
  Concrete Using Performed Foam Table 1508.2, 1917.1.2, 1917.1.3, 1917.4.5

C836/C836M—~~15~~  2018 Specification for High-solids Content, Cold Liquid-applied
  Elastomeric Waterproofing Membrane for Use with Separate Wearing Course 1507.15.2

C840—~~13~~ 2018A Specification for Application and Finishing of Gypsum Board Table 2508.1, 2509.2

C841—03(~~2013~~ 2018) Specification for Installation of Interior Lathing and Furring Table 2508.1, Table 2511.1.1

C842—05(2015) Specification for Application of Interior Gypsum Plaster Table 2511.1.1, 2511.3, 2511.4

C843—~~99 (2012)~~ 2017 Specification for Application of Gypsum Veneer Plaster Table 2511.1.1

C844—2015 Specification for Application of Gypsum Base to Receive Gypsum Veneer Plaster Table 2508.1

C847—~~14A~~ 2018 Specification for Metal Lath Table 2507.2

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete 1917.4.4

C869—11 Specification for Foaming Agents Used in Making Preformed Foam for Cellular
  Concrete Table 1508.2, 1917.4.5

C887—13 Specification for Packaged, Dry Combined Materials for Surface Bonding Mortar 1805.2.2, 2103.2.2

C897—15 Specification for Aggregate for Job-Mixed Portland Cement-based Plaster Table 2507.2

C920—~~14A~~ 2018 Standard for Specification for Elastomeric Joint Sealants 2415.4, Table 2506.2, B303.6, E303.3.1

C926—18b Specification for Application of Portland Cement-based Plaster 2510.3,

Table 2511.1.1, 2511.3, 2511.4, 2512.1,
2512.1.2, 2512.2, 2512.6, 2512.8.2, 2512.9, 2513.7

C932—06(2013) Specification for Surface-applied Bonding Compounds for Exterior Plastering Table 2507.2

C933—~~14~~ 2018 Specification for Welded Wire Lath Table 2507.2

C946—~~10~~ 2018 Specification for Construction of Dry-stacked, Surface-bonded Walls 2103.2.2, 2109.2.2

C954—~~15~~ 2018 Specification for Steel Drill Screws for the Application of Gypsum Panel Products
  or Metal Plaster Bases to Steel Studs from 0.033 inch (0.84 mm)
  to 0.112 inch (2.84 mm) in Thickness Table 2506.2, Table 2507.2

C956—04(2015) Specification for Installation of Cast-in-place Reinforced Gypsum Concrete 2514.1

C957/C957M—~~15~~  2017 Specification for High-solids Content, Cold Liquid-applied
  Elastomeric Waterproofing Membrane with Integral Wearing Surface 1507.15.2

C1002-2018 Specification for Steel Self-piercing Tapping Screws for the Application of Gypsum Panel Products or Metal Plaster Bases to Wood Studs or Steel Studs

C1007—11a(2015) Specification for Installation of Load Bearing (Transverse and
  Axial) Steel Studs and Related Accessories Table 2508.1, Table 2511.1.1

C1029—15 Specification for Spray-applied Rigid Cellular Polyurethane Thermal Insulation 1507.14.2

C1032—~~14~~ 2018 Specification for Woven Wire Plaster Base Table 2507.2

C1036—01 Specification for Flat Glass 2411.1.2

C1047—~~2014a~~  2018 Specification for Accessories for Gypsum Wallboard and Gypsum Veneer Base Table 2506.2, Table 2507.2

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete 1917.4.4

C1063—~~19a~~  2018B Specification for Installation of Lathing and Furring to Receive
  Interior and Exterior Portland Cement-based Plaster 2510.3,

Table 2511.1.1, 2512.1.1

C1088—~~14~~ 2018 Specification for Thin Veneer Brick Units Made from Clay or Shale Table 721.1(2)

C1115—00 Dense Elastomeric Silicone Rubber Gaskets and Accessories 2411.3.4

C1157/C1157M—~~11~~  2017 Standard Performance Specification for Hydraulic Cement 1903.1, Table 2507.2

C1167—11(2017) Specification for Clay Roof Tiles 1507.3.4, 1523.6.5.2

ASTM—continued

C1177/C1177M—~~13~~  2017 Specification for Glass Mat Gypsum Substrate for
  Use as Sheathing Figure 722.5.1(2), Figure 722.5.1(3), Table 1508.2, Table 2506.2

C1178/C1178M—~~13~~  2018 Specification for Coated Mat Water-resistant Gypsum
  Backing Panel Figure 722.5.1(2), Figure 722.5.1(3), Table 2506.2, Table 2509.2

C1186—08(~~2012~~ 2016) Specification for Flat Fiber Cement Sheets 1404.10, 1405.16.1, 1405.16.2

C1225—08 (2012) Specification For Fiber-Cement Roofing Shingles, Shakes and Slates 1518.5.1

C1261—~~13~~ 2013(2017)E1 Specification for Firebox Brick for Residential Fireplaces 2111.6, 2111.9

C1278/C1278M—~~07a(2011)~~ 2017 Specification for Fiber-reinforced
  Gypsum Panels Figure 722.5.1(2), Figure 722.5.1(3), Table 1508.2, Table 2506.2

C1280—13A Specification for Application of Exterior Gypsum Panel Products for Use as Sheathing Table 2508.1, 2508.2

C1283—~~11~~ 2015 Practice for Installing Clay Flue Lining 2113.9.1, 2113.12

C1288—~~14~~ 2017 Standard Specification for Discrete Nonasbestos Fiber-cement Interior Substrate Sheets Table 2509.2

C1289—~~15~~ 2018 Standard Specification for Faced Rigid Cellular Polyisocyanurate Thermal Insulation Board Table 1508.2,

2603.10, Table 2603.12.1,
Table 2603.12.2

C1314—07 Specification for Test Method for Compressive Strength of Masonry Prisms 2122.3

C1325—~~14~~ 2018 Standard Specification for Nonasbestos Fiber-mat Reinforced Cement Backer Units Table 2509.2

C1328/C1328M—12 Specification for Plastic (Stucco Cement) Table 2507.2

C1364—~~10B~~ 2017 Standard Specification for Architectural Cast Stone 2103.1

C1396M/C1396M—~~2014A~~ 2017 Specification for Gypsum Board Figure 722.5.1(2), Figure 722.5.1(3)

C1492—03(~~2009~~ 2016) Standard Specification for Concrete Roof Tile 1507.3.5

C1600/C1600M—~~11~~ 2017 Standard Specification for Rapid Hardening Hydraulic Cement Table 2507.2

C1629/C1629M—~~15~~ 2018A Standard Classification for Abuse-resistant Nondecorated
  Interior Gypsum Panel Products and Fiber-reinforced Cement Panels 403.2.3.1, 403.2.3.2, 403.2.3.4

C1658/C1658M—~~13~~ 2018 Standard Specification for Glass Mat
  Gypsum Panels Figure 722.5.1(2), Figure 722.5.1(3), Table 2506.2

C1670—~~16~~ 2018 Standard Specification for Adhered Manufactured Stone Masonry Veneer Units 2103.1

C1766—~~13~~ 2015 Standard Specification for Factory-laminated Gypsum Panel Products Table 2506.2

D25—~~12~~ 2012(2017) Specification for Round Timber Piles 1810.3.2.4, 2303.1.12

D41/D41M—~~2011~~  2011(2016) Specification for Asphalt Primer Used in Roofing,
  Dampproofing and Waterproofing 1514.2.3.1,

1517.6.2.4, 1519.6, 1521.6, 1521.14.1

, Table 1507.10.2

D43/D43M—2000(~~2012~~ 2018)~~E1~~ Specification for Coal Tar Primer Used in Roofing, Dampproofing
  and Waterproofing 1514.2.3.1, 1517.6.2.4, 1519.6, 1521.6, 1521.14.2, Table 1507.10.2

D56—~~05(2010)~~ 2016A Test Method for Flash Point By Tag Closed Cup Tester 202

D86—~~15~~  2017 Test Method for Distillation of Petroleum Products at Atmospheric Pressure 202

D92—12b Standard Test Method for Flash and Fire Points by Cleveland Open Cup Tester 1519.2.2

D93—~~15~~ 2018 Test Method for Flash Point By Pensky-Martens Closed Cup Tester 202

D225—07 Specification for Asphalt Shingles (Organic Felt) Surfaced with Mineral Granules 1507.2.5

D226/D226M—~~09~~  2017 Specification for Asphalt-saturated Organic Felt
  Used in Roofing and Waterproofing 1404.2, 1505.2, 1507.1.1, 1507.1.1.1, Table 1507.1.1,

1507.2.3, 1507.3.3, 1507.5.3, 1507.6.3, 1507.7.3, 1507.8.3,

1507.9.3, Table 1507.10.2, 1507.17.3, 1518.4

D227/D227M—
03~~(2011~~ 2018)E1 Specification for Coal-tar-saturated Organic Felt Used in Roofing and Waterproofing Table 1507.10.2

D256—03 Standard Test Methods for Determining the Izod Pendulum Impact Resistance of Plastics 2615.2

D312/D312M—~~15~~ 2016M Specification for Asphalt Used in Roofing Table 1507.10.2, 1519.3, Table 1519.3A,

1519.4, 1521.14.1

D412—98a (2002)e1 Standard Test Methods for Vulcanized Rubber and Thermoplastic
  Elastomers—Tension 2415.4

D422—63 (2007) E2 Test Method for Particle-size Analysis of Soils 1803.5.3

D448—2012(2017) Standard Classification for Sizes of Aggregate for Road and Bridge Construction 1507.12.3,

1507.13.3, E403.3

D450/D450M—~~0~~17(~~2013~~2018)~~E1~~ Specification for Coal-tar Pitch Used in Roofing, Dampproofing and
  Waterproofing Table 1507.10.2, Table 1519.3B

D624—00e1 Standard Test Method for Tear Strength of Conventional Vulcanized Rubber
  and Thermoplastic Elastomers 2415.4

D635—14 Test Method for Rate of Burning and/or Extent and
  Time of Burning of Plastics in a Horizontal Position 2606.4

D638—03 Test Method for Tensile Properties of Plastics 2614.2, 2615.2

D1079—02 Standard Terminology Relating to Roofing, Waterproofing, and Bituminous Materials 1513.1

D1143/D1143M—07(2013)E1 Test Method for Deep Foundations Under Static Axial Compressive Load 1810.3.3.1.2

D1227—13 Specification for Emulsified Asphalt Used as a Protective Coating for Roofing Table 1507.10.2, 1507.15.2

ASTM—continued

D1557—2012 E1 Test Method for Laboratory Compaction Characteristics
  of Soil Using Modified Effort [56,000 ft-lb/ft3 (2,700 KN m/m3)] J107.5, J111, 1804.5, 1804.6

D1621 Standard Test Method for Compressive Properties of Rigid Cellular Plastics 1523.6.5.2.17.1

D1622 Standard Test Method for Apparent Density of Rigid Cellular Plastics 1523.6.5.2.17.2

D1623 Standard Test Method for Tensile and Tensile Adhesion Properties of Rigid
  Cellular Plastics 1523.6.5.2.17.3

D1761—06 Test Method for Mechanical Fasteners in Wood 2314.4.4

D1863/D1863M—05(~~2011~~2018)E1 Specification for Mineral Aggregate Used on Built-up Roofs 1504.8, Table 1507.10.2, 1519.12.1

D1929—16 Standard Test Method for Determining Ignition Temperature of Plastics 402.6.4.4, 406.7.2,

1409.11.2.1, 2606.4

D1970/D1970M—~~2015a~~ 2017A Specification for Self-adhering Polymer Modified
  Bituminous Sheet Materials Used as Steep Roof
  Underlayment for Ice Dam Protection 1507.1.1, Table 1507.1.1, 1507.1.1.1, 1507.1.1.2,

1507.1.1.3, 1507.2.4, 1502.2.8.1, 1507.2.9.2

D2126 Standard Test Method for Response of Rigid Cellular Plastics to Thermal
  and Humid Aging 1523.6.5.2.17.4

D2178/D2178M—15A Specification for Asphalt Glass Felt Used in Roofing and Waterproofing Table 1507.10.2

D2240—03 Standard Test Method for Rubber Property—Durometer Hardness 2415.4

D2487—~~2011~~ 2017 Practice for Classification of Soils for Engineering
  Purposes (Unified Soil Classification System) Table 1610.1, 1803.5.1

D2565—99(2008) Standard Practice for Xenon Arc Exposure of Plastics Intended for Outdoor
  Applications 2615.2

D2626/D2626M—
04(2012)E1 Specification for Asphalt Saturated and Coated Organic Felt Base Sheet Used in Roofing 1507.3.3,

Table 1507.10.2, 1518.4

D2822/
D2822M-05(2011)~~E1~~ Specification for Asphalt Roof Cement, Asbestos Containing Table 1507.10.2

D2823/D2823M—
05(2011)E1 Specification for Asphalt Roof Coatings, Asbestos Containing Table 1507.10.2

D2824/D2824M—~~2013~~2018 Standard Specification for Aluminum-Pigmented Asphalt Roof Coating,
  Nonfibered, and Fibered without Asbestos Table 1507.10.2

D2842 Standard Test Method for Water Absorption of Rigid Cellular Plastics 1523.6.5.2.17.6

D2843—16 Standard Test Method for Density of Smoke from the Burning or Decomposition of Plastics 2606.4

D2856 Standard Test Method for Open-cell Content of Rigid Cellular Plastics
  by the Air-Pycnometer. 1523.6.5.2.17.5

D2859—16 Standard Test Method for Ignition Characteristics of Finished
  Textile Floor Covering Materials 804.4.1, 804.4.2

D2898—10(2017) Test Methods for Accelerated Weathering of Fire-retardant-treated
  Wood for Fire Testing 1505.1, 1516.1, 2303.2.4, 2303.2.6, 2314.4.4

D3018 Standard Specification for Class A Asphalt Shingles Surfaced with Mineral Granules 1523.6.5.1

~~D3019—08~~ D3019/D3019M

—2017 Specification for Lap Cement Used with Asphalt Roll Roofing,
  Nonfibered, Asbestos Fibered and Nonasbestos Fibered Table 1507.10.2

D3161/D3161M—16 2016A Test Method for Wind Resistance of Steep Slope Roofing Products
  (Fan Induced Method) 1504.3.3, Table 1504.3.3, 1507.2.7.1, Table 1507.2.7.1, 1507.17.8

D3200—74 (~~2012~~ 2017) Standard Specification and Test Method for Establishing Recommended
  Design Stresses for Round Timber Construction Poles 2303.1.12

D3201/D3201M—2013 Test Method for Hygroscopic Properties of Fire-retardant-treated
  Wood and Wood-based Products 2303.2.7, 2314.4.4

D3278—1996 (2011) Test Methods for Flash Point of Liquids by Small Scale Closed-cup Apparatus 202

D3462/D3462M—~~10A~~ 2016 Specification for Asphalt Shingles Made from Glass Felt and Surfaced with
  Mineral Granules 1507.2.5, 1523.6.5.1

D3468/D3468—99 (2013)E1 Specification for Liquid-applied Neoprene and
  Chlorosulfonated Polyethylene Used in Roofing and Waterproofing 1507.15.2

D3498—03 Standard Specifications for Adhesives for Field-Gluing Plywood to Lumber Framing
  for Floor Systems 2314.4.4, 2322.1.5

D3679—17 Specification for Rigid Poly (Vinyl Chloride) (PVC) Siding 1404.9, 1405.14

D3689/D3698M—2013E1 Test Methods for Deep Foundations Under Static Axial Tensile Load 1810.3.3.1.5

D3737—~~2012~~ 2018el Practice for Establishing Allowable Properties for Structural Glued Laminated Timber (Glulam) 2303.1.3

D3746/D3746M—85 (2015)E1 Test Method for Impact Resistance of Bituminous Roofing Systems 1504.7, 1515.2.4

D3747—79 (2007) Specification for Emulsified Asphalt Adhesive for Adhering Roof Insulation Table 1507.10.2

ASTM—continued

D3787—89 Test Method for Bursting Strength of Textiles-Constant-Rate-of-Traverse (CRT)
  Ball Burst Test 454.2.17.1.15

D3909/

D3909M—14 Specification for Asphalt Roll Roofing (Glass Felt) Surfaced with Mineral Granules 1507.2.9.2, 1507.6.5,

Table 1507.10.2

D3957—09 (2015) Standard Practices for Establishing Stress Grades for Structural Members Used in Log Buildings 2303.1.11

D4022/D4022M—
2007(2012)E1 Specification for Coal Tar Roof Cement, Asbestos Containing Table 1507.10.2

D4086 Standard Practice for Visual Evaluation of Metamerism 454.1.2.4, 454.1.11.3

D4272—15 Test Method for Total Energy Impact of Plastic Films by Dart Drop 1504.7, 1515.2.4

D4318—~~10E1~~ 2017E1 Test Methods for Liquid Limit, Plastic Limit and Plasticity Index of Soils 1803.5.3

D4402 Viscosity Determinations of Unfilled Asphalt Using the Brookfield Thermoset Apparatus 1519.2.3

D4434/D4434M—~~12~~ 2015 Specification for Poly (Vinyl Chloride) Sheet Roofing 1507.13.2

D4479/D4479M—
07(~~2012~~ 2018)~~E1~~ Specification for Asphalt Roof Coatings-Asbestos-free Table 1507.10.2

D4533(2015) Standard Test Method for Trapezoid Tearing Strength of Geo Textiles 1507.1.1.1

D4586/D4586M—
07(~~2012~~ 2018)~~E1~~ Specification for Asphalt Roof Cement-Asbestos-free Table 1507.10.2

D4601/D4601M—
04(2012)E1 Specification for Asphalt-coated Glass Fiber Base Sheet Used in Roofing Table 1507.10.2

D4637/D4637M—~~14e1~~ 2015 Specification for EPDM Sheet Used in Single-ply Roof Membrane 1507.12.2

D4829—11 Test Method for Expansion Index of Soils 1803.5.3

D4869/D4869M—2016A Specification for Asphalt-saturated (Organic Felt)
  Underlayment Used in Steep Slope Roofing 1507.1.1, Table 1507.1.1, 1507.1.1.1,

1507.1.1.2, 1507.1.1.3, 1507.2.3, 1507.5.3,

1507.6.3, 1507.7.3, 1507.8.3, 1507.9.3, 1507.17.3

D4897/D4897M—~~01(2009)~~ 2016A Specification for Asphalt-coated Glass Fiber Venting Base Sheet Used in Roofing Table 1507.10.2

D4945—~~12~~ 2017 Test Method for High-strain Dynamic Testing of Deep Foundations 1810.3.3.1.2

D4990—97a (2013) Specification for Coal Tar Glass Felt Used in Roofing and Waterproofing Table 1507.10.2

D5019—07a Specification for Reinforced Nonvulcanized Polymeric Sheet Used in Roofing Membrane 1507.12.2

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete 1917.4.4

D5055—~~13E1~~ 19el Specification for Establishing and Monitoring Structural
  Capacities of Prefabricated Wood I-joists 2303.1.2

D5456—~~14B~~ 21el Specification for Evaluation of Structural Composite Lumber Products 2303.1.10

D5516—~~09~~ 2018 Test Method of Evaluating the Flexural Properties of Fire-retardant-treated
  Softwood Plywood Exposed to the Elevated Temperatures 2303.2.5.1

D5643/D5643M—
06(~~2012~~ 2018)~~E1~~  Specification for Coal Tar Roof Cement, Asbestos-free Table 1507.10.2

D5664—~~10~~ 2017 Test Methods for Evaluating the Effects of Fire-retardant Treatment and
  Elevated Temperatures on Strength Properties of Fire-retardant-treated Lumber 2303.2.5.2

D5665/D5665M—20~~14E1~~17 Specification for Thermoplastic Fabrics Used in Cold-applied
  Roofing and Waterproofing Table 1507.10.2

D5726—98 (2013) Specification for Thermoplastic Fabrics Used in Hot-applied
  Roofing and Waterproofing Table 1507.10.2

D5957—98 Standard Guide for Flood Testing Horizontal Waterproofing Installation 1519.16.6

D6083/D6063M—~~18~~  21 Specification for Liquid Applied Acrylic Coating Used in Roofing Table 1507.10.2, Table 1507.14.3,

1507.15.2, 1523.6.2.1.1, 1523.6.3.1, 1523.6.5.2.12.2

D6162/D6162M—~~2000A
(2015)E1~~ 2016 Specification for Styrene-butadiene-styrene (SBS) Modified Bituminous
  Sheet Materials Using a Combination of Polyester and Glass Fiber Reinforcements 1507.11.2

D6163/D6163M—~~2000~~
~~(2015)E1~~ 2016 Specification for Styrene-butadiene-styrene (SBS) Modified
  Bituminous Sheet Materials Using Glass Fiber Reinforcements 1507.11.2

D6164/D6164M—~~11~~2016 Specification for Styrene-butadiene-styrene (SBS) Modified
  Bituminous Sheet Metal Materials Using Polyester Reinforcements 1507.11.2

D6222/D6222M—~~11~~ 2016 Specification for Atactic Polypropylene (APP) Modified
  Bituminous Sheet Materials Using Polyester Reinforcements 1507.11.2

D6223/D6223M—
~~02(2009)E1~~ 2016 Specification for Atactic Polypropylene (APP) Modified Bituminous Sheet
  Materials Using a Combination of Polyester and Glass Fiber Reinforcements 1507.11.2

D6298/D6298M—~~13~~ 2016 Specification for Fiberglass Reinforced Styrene-butadiene-styrene
  (SBS) Modified Bituminous Sheets with a Factory Applied Metal Surface 1507.11.2

ASTM—continued

D6305—08(2015)E1 Practice for Calculating Bending Strength Design Adjustment
  Factors for Fire-retardant-treated Plywood Roof Sheathing 2303.2.5.1

D6380/D6380—03(~~2013~~2018)~~E1~~ Standard Specification for Asphalt Roll Roofing (Organic) Felt 1507.2.9.2, 1507.3.3, 1507.6.5

D6464—03a(~~2009~~ 2017)~~e1~~ Standard Specification for Expandable Foam Adhesives for Fastening Gypsum
  Wallboard to Wood Framing 2508.4, Table 2506.2

D6509/D6509M—~~09(2015)~~ 2016 Standard Specification for Atactic Polypropylene (APP)
  Modified Bituminous Base Sheet Materials Using Glass Fiber Reinforcements 1507.11.2

D6694/D6694M—08(2013)E1 Standard Specification for Liquid-applied Silicone Coating
  Used in Spray Polyurethane Foam Roofing Systems Table 1507.14.3, 1507.15.2

D6754/D6745M—15 Standard Specification for Ketone Ethylene Ester Based Sheet Roofing 1507.13.2

D6757—~~2016~~ 2018 Specification for Inorganic Underlayment for Use with
  Steep Slope Roofing 1507.1.1, Table 1507.1.1, 1507.2.3, 1507.17.3

D6841—~~08~~ 2016 Standard Practice for Calculating Design Value Treatment
  Adjustment Factors for Fire-retardant-treated Lumber 2303.2.5.2

D6878/D6878M—~~13~~ 2017 Standard Specification for Thermoplastic Polyolefin Based Sheet Roofing 1507.13.2

D6947/D6947M—07~~(2013~~ 2016~~)E1~~ Standard Specification for Liquid Applied Moisture Cured
  Polyurethane Coating Used in Spray Polyurethane Foam Roofing System Table 1507.14.3, 1507.15.2

D7032—~~14~~  2017 Standard Specification for Establishing Performance Ratings for Wood,
  Plastic Composite Deck Boards and Guardrail Systems (Guards or Rails) 2612.2, 2612.2.1,

2612.4, 2612.5.1

D7147—11(2018) Specification for Testing and Establishing Allowable
  Loads of Joist Hangers 2303.5.1, 2303.5.2, 2304.10.3

D7158/D7158M—19ae1 Standard Test Method for Wind Resistance of Asphalt Shingles (Uplift Force/
  Uplift Resistance Method) 1504.1.1, 1507.1.1, Table 1507.1.1, 1507.2.7.1

D7254—17 Standard Specification for Polypropylene (PP) Siding 1404.12

D7655/D7655M—12(2017) Standard Classification for Size of Aggregate Used as Ballast for Roof Membrane Systems 1507.12.3,

1507.13.3

D7672—~~14~~ 19E1 Standard Specification for Evaluating Structural Capacities of Rim Board Products and Assemblies 2303.1.13

E84—~~2016~~ 2018B Test Methods for Surface Burning Characteristics of Building Materials 202, 402.6.4.4, 406.7.2,

452.2.16.3, 703.5.2, 720.1, 720.4, 803.1.1, 803.1.4, 803.10, 803.11,
806.7, 1403.5, 1404.12.1, 1407.9, 1407.10.1, 1409.9, 1409.10.1, 1510.6.2,
1510.6.3, 2303.2, 2314.4.4, 2603.3, 2603.4.1.13, 2603.5.5, 2603.7.1, 2603.7.2,
 2603.7.3, 2604.2.4, 2606.3.5.4, 2606.4, 2612.3, 2614.3, 3105.6

E90—09(2016) Test Method for Laboratory Measurement of Airborne Sound
  Transmission Loss of Building Partitions and Elements 1207.2, 1207.2.1

E96/E96M—~~2015~~ 2016 Test Method for Water Vapor Transmission of Materials 202, 449.3.6.4.2, 451.3.6.3.3,

1523.6.5.2.17.7, B302.1

E108—~~16~~ 2017 Standard Test Methods for Fire Tests of Roof Coverings 453.12.1, 1505.1, 1513.1, 1516.1,

2603.6, 2610.2, 2610.3

E119—~~2016~~ 2018B Standard Test Methods for Fire Tests of Building Construction and Materials 703.2, 703.2.1, 703.2.3,

703.2.5, 703.3, 703.4, 703.6, 704.12, 705.7, 705.8.5,
707.6, 712.1.13.2, 714.3.1, 714.4.1, 715.1, 715.4, 716.2, Table 716.3,
Table 716.5, 716.5.6, 716.5.8.1.1, Table 716.6, 716.6.7.1, 717.3.1,
 717.5.2, 717.5.3, 717.6.1, 716.6.2.1, Table 721.1(1), 2103.1, 2603.5.1

E136—~~16~~2019 Stand Test Method for Assessing Combustibility of ~~Behavior of~~ Materials Using ~~in~~ a Vertical Tube Furnace at 750°C 703.5.1

E283—04(2012) Standard Test Method for Determining Rate of Air Leakage Through Exterior Windows
  Curtain Walls, and Doors Under Specified Pressure Difference Across the Specimen 202

E330/E330M—02 or 14 Test Method for Structural Performance of Exterior Windows, Curtain Walls and
  Doors by Uniform Static Air Pressure Difference 1709.5.2, 1709.5.2.1, 1709.8, 2415.4, 2415.7.1

E331—00 (~~2009~~ 2016) Test Method for Water Penetration of Exterior Windows, Skylights,
  Doors and Curtain Walls by Uniform Static Air Pressure Difference 1403.2, 2415.4

E492—09(2016)E1 Test Method for Laboratory Measurement of Impact Sound Transmission Through
  Floor-ceiling Assemblies Using the Tapping Machine 1207.3

E648—~~14c~~ 2017A Standard Test Method for Critical Radiant Flux of Floor-covering Systems
  Using a Radiant Heat Energy Source 406.8.3, 424.2, 804.2, 804.3

E648—17A Standard Test Method for Critical Radiant Flux of Floor-covering Systems
  Using a Radiant Heat Energy Source 406.1.4, 424.2, 804

E681—2009(2015) Test Methods for Concentration Limits of Flammability of Chemical Vapors and Gases 202

E736/E736M—~~00(2015)E1~~ 2017 Test Method for Cohesion/Adhesion of Sprayed Fire-resistive
  Materials Applied to Structural Members 704.13.3.2

E814—2013A(2017) Standard Test Method of Fire Tests of Through-penetration
  Firestops 202, 714.3.1.2, 714.3.2, 714.4.1.2

ASTM—continued

E970—~~2014~~ 2017 Standard Test Method for Critical Radiant Flux of Exposed Attic
  Floor Insulation Using a Radiant Heat Energy Source 720.3.1

E1300—04e01, 07e01,
09e, 12AE1 or 16 ~~12AE1~~ in ICC Practice for Determining Load Resistance of Glass in Buildings 1709.5.1, 2404.1, 2404.2, 2404.3.1,

2404.3.2, 2404.3.3, 2404.3.4, 2404.3.5, 2411.2.1.1, 2411.2.1.2, 2411.3.1.2

E1347 Standard Test Method for Color and Color-Difference Measurement by
  Tristimulus Colorimetry 454.1.2.4, 454.1.11.3

E1354—~~2016~~ 2017 Standard Test Method for Heat and Visible Smoke Release Rates for
  Materials and Products Using an Oxygen Consumption Calorimeter 424.2, 1403.5

E1477 Standard Test Method for Luminous Reflectance Factor of Acoustical Materials by
  Use of Integrating-Sphere Reflectometers 454.1.2.4

E1592—05(~~2012~~ 2017) Test Method for Structural Performance of Sheet Metal Roof and Siding Systems
  by Uniform Static Air Pressure Difference 1504.3.2

E1602—03(~~2010~~ 2017)~~E1~~ Guide for Construction of Solid Fuel-burning Masonry Heaters 2112.2

E1886—12 or 2013a Test Method for Performance of Exterior Windows, Curtain Walls, Doors and
  Storm Impact Protective Systems Impacted by Missiles and Exposed to Cyclic
  Pressure Differentials 1609.1.2, 1709.5.1

E1966—2015 Standard Test Method for Fire-resistant Joint Systems 202, 715.3

E1996—17, or
2012a, or 2014a Specification for Performance of Exterior Windows, Curtain Walls, Doors and Impact
  Protective Systems Impacted by Windborne Debris in Hurricanes 449.4.2.5.1, 450.4.2.5.1,

1609.1.2, 1609.1.2.2, 1709.5.1

E2072—14 Standard Specification for Photoluminescent (Phosphorescent) Safety Markings 1025.3, 1025.4

E2140—01 Standard Test Method for Water Penetration of Metal Roof Panel Systems by
  Static Water Pressure Head Table 1515.2, 1523.6.5.2.4.1.1, TAS 110 Table 15

E2178—13 Standard Test Method for Air Permeance of Building Materials 202, 1507.10.2

E2203—02 Dense Thermoplastic Elastomers Used for Compression Seals, Gaskets, Setting
  Blocks, Spacers and Accessories 2411.3.4

E2273—~~03(2011)~~ 2018 Standard Test Method for Determining the Drainage Efficiency of
  Exterior Insulation and Finish Systems (EIFS) Clad Wall Assemblies 1408.4.1

E2307—15BE1 Standard Test Method for Determining Fire Resistance of
  Perimeter Fire Barriers Using the Intermediate-scale, Multistory Test Apparatus 715.4

E2322—03 (Reapproved 2015) Standard Test Method for Conducting Transverse and Concentrated Load Tests on
  Panels Used in Floor and Roof Construction 3115.4.2

E2353—~~14~~ 2016 Standard Test Methods for Performance of Glazing in Permanent Railing Systems,
  Guards and Balustrades 2407.1.2

E2397/E2397M—2015 Standard Practice for Determination of Dead Loads and Live Loads Associated
  with Vegetative Green Roof Systems 1607.12.3.1

E2404—~~15a~~ 2017 Standard Practice for Specimen Preparation and Mounting of Textile, Paper or
  Vinyl Wall or Ceiling Coverings to Assess Surface Burning Characteristics 803.1.4

E2556/E2556M—10(2016) Standard Specification for Vapor Permeable Flexible Sheet Water-Resistive Barriers
  Intended for Mechanical Attachment 2510.6

E2568—~~09e1~~ 2017A Standard Specification for PB Exterior Insulation and Finish Systems 1408.2

E2570/E2570—07(2014)E1 Standard Test Method for Evaluating Water-resistive Barrier (WRB)
  Coatings Used Under Exterior Insulation and Finish Systems (EIFS) for
  EIFS with Drainage 1408.4.1.1

E2573—~~12~~ 2017 Standard Practice for Specimen Preparation and Mounting of Site-fabricated
  Stretch Systems to Assess Surface Burning Characteristics 803.10

E2599—~~15~~ 2018 Standard Practice for Specimen Preparation and Mounting of Reflective Insulation
  Materials and Vinyl Stretch Ceiling Materials for Building Applications to
  Assess Surface Burning Characteristics 2614.3

E2634—~~11(2015)~~ 2018 Standard Specification for Flat Wall Insulating Concrete Form (ICF) Systems 1903.4

E2751/E2751M—~~13~~ 2017A Standard Practice for Design and Performance of Supported Laminated Glass Walkways 2409.1

F547—~~(2012)~~  2017 Terminology of Nails for Use with Wood and Wood-based Materials Table 2506.2

F1346—91 (2010) Performance Specification for Safety Covers and Labeling Requirements for
  All Covers for Swimming Pools, Spas and Hot Tubs 454.1.1, 454.1.3.1.9,

 454.2.2, 454.2.17

F1487 Standard Consumer Safety Performance Specification for Playground
  Equipment for Public Use 453.4.5, 453.10.5.2

F1667—~~15~~ 2018 Specification for Driven Fasteners: Nails, Spikes and Staples Table 721.1(2), Table 721.1(3),

1506.5, 1507.2.6, 2303.6, Table 2506.2

F2006—10 or 17 Standard/Safety Specification for Window Fall Prevention Devices for
  Nonemergency Escape (Egress) and Rescue (Ingress) Windows 1015.8

ASTM—continued

F2090—17 Specification for Window Fall Prevention Devices with Emergency
  Escape (Egress) Release Mechanisms 1015.8, 1015.8.1

F2200—~~2014~~ 2017 Standard Specification for Automated Vehicular Gate Construction 3110.3

F2208—2014 Standard Safety Specification for Residential Pool Alarms 454.2.17.1.9

F2376—17a Standard Practice for Classification, Design, Manufacture, Construction, and
  Operation of Water Slide Systems 454.1.9.2.1.1

F3125/F3125M—15 Standard Specification for High Strength Structural Bolts, Steel and
  Alloy Steel, Heat Treated, 120 ksi (830 MPa) and 150 ksi (1040 MPa) Minimum
  Tensile Strength, Inch and Metric Dimensions 2214.3

G53—96 Practice for Operating Light-and Water-Exposure Apparatus (Fluorescent
  UV-Condensation Type) for Exposure of Nonmetallic Materials 454.2.17.1.15.2

G60—01 Standard Practice for Conducting Cyclic Humidity Tests 2319.17.2.2.8, 2603.12.2

G85 Standard Practice for Modified Salt Spray (Fog) Testing 1517.5.1, 1517.5.2, 1523.6.5.2.10,

1523.6.5.2.11

G152—13 Practice for Operating Open Flame Carbon Arc Light Apparatus for
  Exposure of Nonmetallic Materials 1504.6

G153 Standard Practice for Operating Enclosed Carbon Arc Light Apparatus f  Exposure of Nonmetallic Materials 1504.6

G154—~~12A~~  16A Practice for Operating Fluorescent Light Apparatus for UV Exposure of Nonmetallic Materials 1504.6

G155—13 Practice for Operating Xenon Arc Light Apparatus for Exposure of
  Nonmetallic Materials 1504.6, 2615.2

**(S10107 AS)/(R10513 AS)**

**Also – revise as follows:**

**ASTM**

ASTM International

100 Barr Harbor Drive

West Conshohocken, PA  19428-2959

**Add new standard(s) as follows:**

**ASTM**

E2925-17: Standard Specification for Manufactured Polymeric Drainage and Ventilation Materials Used to Provide a Rainscreen Function

**(S9634 / S196-19 AM)**

**Add new standard(s) as follows:**

**ASTM**

C1372-17: Standard Specification for Dry-Cast Segmental Retaining Wall Units

**(S9574 / S115-19 AS)**

*Update the following, all other existing AAMA Standards remain the same:*

E283—04(2012) or E283/283M-19

Standard Test Method for Determining Rate of Air Leakage Through Exterior Windows Curtain Walls, and Doors Under Specified Pressure Difference Across the Specimen                                                                              202

E330/E330M—~~02 or~~14 or 14 (21)

Test Method for Structural Performance of Exterior Windows, Curtain Walls and Doors by Uniform Static Air Pressure Difference

1709.5.2, 1709.5.2.1, 1709.8, 2415.4, 2415.7.1

E331-00 (2009 or 2016)

Test Method for Water Penetration of Exterior Windows, Skylights, Doors and Curtain Walls by Uniform Static Air Pressure Difference

1403.2, 2415.4

E1886--~~12 or~~2013a or 2019

Test Method for Performance of Exterior Windows, Curtain Walls, Doors and Storm Impact Protective Systems Impacted by Missile(s) and Exposed to Cyclic Pressure Differentials                                      1609.1.2, 1709.5.1

E1996-~~-17 or 2012a or~~ 2014a, 2017 or 2020

Standard Specification for Performance of Exterior Windows, Curtain Walls, Doors and Impact Protective Systems Impacted by Windborne Debris in Hurricanes                    449.4.2.5.1, 450.4.2.5.1, 1609.1.2, 1609.1.2.2, 1709.5.1

F2006—~~10 or~~ 17 or 2021

Standard/Safety Specification for Window Fall Prevention Devices for Nonemergency Escape (Egress) and Rescue (Ingress) Windows

1015.8

F2090--17 or 2021

Specification for Window Fall Prevention Devices with Emergency Escape (Egress) Release Mechanisms

1015.8, 1015.8.1

**(S10435 AM A2)**

ASTM C1570-03(2016): Standard Test Method for Wind Resistance of Concrete and Clay Roof Tiles (Air Permeability Method)

**(R9953 AS)/** **(R9508 / S14-19)**

**Add new standard(s) as follows:**

**ASTM**

E336-17a: Standard Test Method f or Measurement of Airborne Sound Attenuation between Rooms in Buildings

**(S9435 / G123-18 AM)**

**Add new standard(s) as follows:**

**ASTM**

E1007-16: Test Method f or Field Measurement of Tapping Machine Impact Sound Transmission Through Floor Ceiling Assemblies and Associated Support Structures

**(S9436 / G126-18 AM)**

**Add new standard(s) as follows:**

**ASTM**

E2652-16: Standard Test Method for Behavior of Materials in a Tube Furnace with a Cone-shaped Airflow Stabilizer at 750oC

**(F9235 / FS3-18 AMPC1)**

**ASTM F2286-16 Standard Design and Performance Specification for Removable Mesh Fencing for Swimming Pools, Hot Tubs, and Spas                                   454.2.17.1.15**

(SW10438 AS)

**ASTM**

ASTM International

100 Barr Harbor Drive

West Conshohocken, PA 19428-2959

D3737—18e1 Practice for Establishing Allowable Properties for Structural Glued Laminated Timber (Glulam). .2303.1.3

D5055—19e1 Specification for Establishing and Monitoring Structural

Capacities of Prefabricated Wood I-joists . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2303.1.2

D5456—21e1 Specification for Evaluation of Structural Composite Lumber Products. . . . . . . . . . . . . . . . . . . . . 2303.1.10

D7672—19 Standard Specification for Evaluating Structural Capacities of Rim Board Products and Assemblies . .2303.1.13

**(S10107 AS)**

D6878/D6878M—~~13~~ 21 Standard Specification for Thermoplastic Polyolefin Based Sheet Roofing . . . . . . . . . . . . . . . . . .1507.13.2

**(R10119 AM with A1)**

ASTM ~~D6083-18~~ D6083/D6083M-21        Specification for Liquid-Applied Acrylic Coating Used in Roofing

**(R10513 AS)**

ASTM D8257                                         Standard Specification for Mechnically Attached Polymeric Roof Underlayment Used in Steep Slope Roofing

**(R10145 AS)**

ASTM International

100 Barr Harbor Drive P.O. Box C700

West Conshohocken, PA 19428-2959

Standard

reference

number                                                     Title

|  |
| --- |
|  |

        C1902                                         Standard Specification for Cellular Glass Insulation Used in Building and Roof Applications

(R10479 AS)

AWC

American Wood Council

222 Catoctin SE, Suite 201

Leesburg, VA 20175

Standard Referenced
reference in code
number Title section number

AWC WCD No. 4—2003 Wood Construction Data—Plank and Beam Framing for Residential Buildings 2306.1.2, 2314.4.7

ANSI/AWC WFCM—2018 Wood Frame Construction Manual for One- and Two-Family Dwellings 1609.1.1, 1609.1.1.1,

2301.2, 2309.1, 2314.4.7

ANSI/AWC NDS—2018 National Design Specification (NDS) for
  Wood Construction with 2015 NDS Supplement 202, 722.1, Table 1604.3, 1809.12,

1810.3.2.4, Table 1810.3.2.6, 1905.1.8,
2304.13, 2306.1, Table 2306.2(1), Table 2306.2(2),

Table 2306.3(1), Table 2306.3(2), 2307.1, 2314.4.7

AWC STJR—~~2015~~ 2021 Span Tables for Joists and Rafters 2306.1.1, 2314.4.7

ANSI/AWC PWF—~~2015~~ 2021 Permanent Wood Foundation Design Specification 1805.2, 1807.1.4, 2304.10.5.2, 2314.4.7

ANSI/AWC SDPWS—~~2015~~ 2021 Special Design Provisions for Wind and Seismic 202, 2305.1, 2305.2, 2305.3, 2306.1, 2306.2,

2306.3, Table 2306.3(1), Table 2306.3(3), 2307.1, 2314.4.7

AWPA

American Wood Protection Association

P.O. Box 361784

Birmingham, AL 35236-1784

Standard Referenced
reference in code
number Title section number

C1—03 All Timber Products-Preservative Treatment by Pressure Processes 1505.6

M4—2015 Standard for the Care of Preservative-treated Wood Products 1810.3.2.4.1, 2303.1.9, 2314.4.5

U1—~~16~~ 20 USE CATEGORY SYSTEM: User Specification for Treated Wood
  Except Commodity Specification H 1403.6, Table 1507.9.6, 1807.1.4, 1807.3.1,

1809.12, 1810.3.2.4.1, 2303.1.9, 2304.12.1,
2304.12.4, 2304.12.3, 2304.12.5, 2314.4.5

AWS

American Welding Society

8669 NW 36 Street, #130

Doral, FL 33166

Standard Referenced
reference in code
number Title section number

B2.1—B2.1M—~~2018~~ 2014-AMD1 Specification for Welding Procedure and Performance Qualification 2214.3

D1.1—D1.1M—2020 Structural Welding Code—Steel 2214.3

D1.2 Structural Welding Code—Aluminum 2003.3

D1.3—D1.3M—2018 Structural Welding Code—Sheet Steel 2214.3

D1.4—D1.4M—~~2017~~ 2018-ADMD1 Structural Welding Code—Reinforcing Steel 2214.3

D9.1—D9.1M—2018 Sheet Metal Welding Code 2214.3

**(S9988 AS)**

D1.4—D1.4M—~~2017~~ 2018-AMD1 Structural Welding Code—Reinforcing Steel 2214.3

B2.1—B2.1M—~~2018~~ 2014-AMD1 Specification for Welding Procedure and Performance Qualification 2214.3

(S9988 AS)

BHMA

Builders Hardware Manufacturers’ Association

355 Lexington Avenue, 17th Floor

New York, NY 10017-6603

Standard Referenced
reference in code
number Title section number

A156.10—~~2011~~ 2017 Power Operated Pedestrian Doors 1010.1.4.2

A156.19—~~2013~~ 2020 Standard for Power Assist and Low Energy Operated Doors 1010.1.4.2

A156.27—~~11~~ 2019 Power and Manual Operated Revolving Pedestrian Doors 1010.1.4.1

A156.38—~~2014~~ 2020 Low Energy Power Operated Sliding and Folding Doors 1010.1.4.2

**Add new standard(s) as follows:**

BHMA

A156.41-2013: Door Controls-Closers

**(F9155 / E54-18 AM)**

CEN

European Committee for Standardization (CEN)

Central Secretariat

Rue de Stassart 36

B-10 50 Brussels

Standard Referenced
reference in code
number Title section number

EN 1081—98 Resilient Floor Coverings—Determination of the Electrical Resistance 406.7.1

BS EN 15250—2007 Slow Heat Release Appliances Fired By Solid Fuel Requirements and Test Methods 2112.2, 2112.5

CGSB

Canadian General Standards Board

Place du Portage 111, 6B1

11 Laurier Street

Gatineau, Quebec, Canada KIA 1G6

Standard Referenced
reference in code
number Title section number

37-GP-52M (1984) Roofing and Waterproofing Membrane, Sheet Applied, Elastomeric 1504.7, 1507.12.2

37-GP-56M (1980) Membrane, Modified, Bituminous, Prefabricated and
  Reinforced for Roofing—with December 1985 Amendment 1507.11.2

CAN/CGSB 37.54—95 Polyvinyl Chloride Roofing and Waterproofing Membrane 1507.13.2

CISCA

Ceilings and Interior Systems Construction Association

1010 Jorie Blvd., Suite 30

Oak Brook, IL 60523

Standard Referenced
reference in code
number Title section number

CISCA—2007 Recommended Test Procedures for Access Floors 3115.4.2, 3115.4.3

CPA

Composite Panel Association

19465 Deerfield Avenue, Suite 306

Leesburg, VA 20176

Standard Referenced
reference in code
number Title section number

ANSI A135.4—2012 Basic Hardboard 1404.3.1, 2303.1.7, 2314.4.1

ANSI A135.5—2012 Prefinished Hardboard Paneling 2303.1.7, 2304.7

ANSI A135.6—2012 Engineered Wood Siding 1404.3.2, 2303.1.7, 2314.4.1

A208.1—2016 Particleboard 2303.1 8, 2303.1. 8.1

CPSC

Consumer Product Safety Commission

4330 East West Highway

Bethesda, MD 20814-4408

Standard Referenced
reference in code
number Title section number

16 CFR Part 1201 (2002) Safety Standard for Architectural Glazing Material 2406.2, Table 2406.2(1),

2406.3.1, 2407.1, 2407.1.4.1, 2408.2.1,
2408.3, 2409.2, 2409.3.1, 2409.4.1

16 CFR Part 1209 (2002) Interim Safety Standard for Cellulose Insulation 720.6

16 CFR Part 1404 (2002) Cellulose Insulation 720.6

16 CFR Part 1500 (2009) Hazardous Substances and Articles; Administration and Enforcement Regulations 202

16 CFR Part 1500.44(2009) Method for Determining Extremely Flammable and Flammable Solids 202

16 CFR Part 1507 (2002) Fireworks Devices 202

16 CFR Part 1630 (2007) Standard for the Surface Flammability of Carpets and Rugs 804.4.1, 804.4.2

Pub. No. 362 Safety Barrier Guidelines for Home Pools 454.1.3.1.9

CSA

Canadian Standards Association

8501 East Pleasant Valley

Cleveland, OH 44131-5516

Standard Referenced
reference in code
number Title section number

AAMA/WDMA/CSA
101/I.S.2/A440—08, 11 or 17or19 Specifications for Windows, Doors and Unit Skylights 1010.1.7, 1709.5.1, 2405.5, 2411.3.2.1

ASME A17.7-2007/CSA B44.7-07 Performance-based Safety Code for Elevators and Escalators

CSSB

Cedar Shake and Shingle Bureau

P. O. Box 1178

Sumas, WA 98295-1178

Standard Referenced
reference in code
number Title section number

CSSB—97 Grading and Packing Rules for Western Red Cedar Shakes and
  Western Red Shingles of the Cedar Shake and Shingle Bureau Table 1507.8.5, Table 1507.9.6

 New Roof Construction Manual (2015) 1507.8

DASMA

Door and Access Systems Manufacturers Association International

1300 Summer Avenue

Cleveland, OH 44115-2851

Standard Referenced
reference in code
number Title section number

ANSI/DASMA 107—2017 Room Fire Test Standard for Garage Doors Using Foam Plastic Insulation 2603.4.1.9

108—05, 12 or 17 Standard Method for Testing Sectional Garage Doors, Rolling Doors
  and Flexible Doors: Determination of Structural Performance
  Under Uniform Static Air Pressure Difference 1709.5.2.1

115—05, 12 or 17 Standard Method for Testing Sectional Garage Doors, Rolling Doors
  and Flexible Doors: Determination of Structural
  Performance Under Missile Impact and Cyclic Wind Pressure 1609.1.2

DECO

Document Engineering Co., Inc.

5210 Stagg Street

Van Nuys, CA 9140

5

Standard Referenced
reference in code
number Title section number

ANSI Z358.1—04 Emergency Eyewash and Shower Equipment 450.3.11.7

DOC/NIST

U.S. Department of Commerce

National Institute of Standards and Technology

100 Bureau Drive Stop 3460

Gaithersburg, MD 20899

Standard Referenced
reference in code
number Title section number

CS236 Mat-Formed Particleboard 2314.4.6

PS-1—~~09~~ 19 Structural Plywood 2303.1.5, 2304.7, Table 2304.8(4),

2304.8(5), Table 2306.2(1), Table 2306.2(2), 2314.4.6

PS-2—~~10~~ 18 Performance Standard for ~~Wood-based~~ Wood Structural~~-use~~ Panels 2303.1.5, 2304.7, 2304.8(5),

Table 2306.2(1), Table 2306.2(2), 2314.4.6

PS 20—05 American Softwood Lumber Standard 202, 1810.3.2.4, 2303.1.1, 2314.4.6

~~PS 56 Structural Glued Laminated Timber~~ 2314.4.6

**(S10107 AS)**

|  |
| --- |
|  **DOC/NIST**U.S. Department of CommerceNational Institute of Standards and Technology100 Bureau Drive Stop 3460Gaithersburg, MD 20899CS236 Mat-Formed Particleboard . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2314.4.6PPS 1—19 Structural Plywood. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2303.1.5, 2304.7, Table 2304.8(4),2304.8(5), Table 2306.2(1), Table 2306.2(2), 2314.4.6PPS 2—18 Performance Standard for Wood Structural Panels . . . . . . . . . . . . . 2303.1.5, 2304.7, 2304.8(5),Table 2306.2(1), Table 2306.2(2), 2314.4.6PS 20—05 American Softwood Lumber Standard. . . . . . . . . . . . . . . . . . . . . . . . . . .202, 1810.3.2.4, 2303.1.1, 2314.4.6~~PS 56 Structural Glued Laminated Timber . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2314.4.6~~ |
|   |

**(S10107 AS)**

DOL/OSHA

U.S. Department of Labor

Occupational Safety and Health Administration

Frances Perkins Building

200 Constitution Avenue NW

Washington, DC 20210

Standard Referenced
reference in code
number Title section number

29 CFR
Part 1910.1000 (2015) Air Contaminants 202

29 CFR 1910.1200 OSHA Hazard Communication Standard 202, 453.6.2

DOTn

U.S. Department of Transportation

c/o Superintendent of Documents

1200 New Jersey Avenue, SE

Washington, DC 20402-9325

Standard Referenced
reference in code
number Title section number

14 CFR Part 150 (2005) The Aviation Safety and Noise Abatement Act of 1979 3114.1

49 CFR Parts 100–185—2015 Hazardous Materials Regulations 202

49 CFR Part 172—2015 Hazardous Materials Tables, Special Provisions, Hazardous Materials
  Communications, Emergency Response Information and Training Requirements 202

49 CFR Parts 173.137
(2009) Shippers—General Requirements for Shipments and Packaging—
  Class 8—Assignment of Packing Group 202

49 CFR—Parts 173–178—(2015) Specification of Transportation of Explosive and Other
  Dangerous Articles, UN 0335, UN 0336 Shipping Containers 202

FDOE

Florida Office of Educational Facilities

1014 Turlington Building

325 West Gaines Street

Tallahassee, FL 32399-0400

Standard Referenced
reference in code
number Title section number

SREF Size of Space and Occupant Design Criteria 453.4.1, 453.8.2

SREF Life Cycle Cost Guidelines for Materials and Building Systems for Florida’s
  Public Educational Facilities 453.8.7

FEMA

Federal Emergency Management Agency

Federal Center Plaza

500 C Street S.W.

Washington, DC 20472

Standard Referenced
reference in code
number Title section number

FEMA-TB-11—01 Crawlspace Construction for Buildings Located in Special Flood Hazard Areas 1805.1.2.1

FGI

The Facility Guidelines Institute

9750 Fall Ridge Trail

St. Louis, MO 63127

Standard Referenced
reference in code
number Title section number

GHCF—18 Guidelines for Design and Construction of Hospitals

 449.2.2,

449.3.2, 449.3.3, 449.3.4, 449.3.5,

449.3.6, 449.3.7, 449.3.9, 449.3.11,

449.3.13, 469.2.1.2

GHCF—18 Guidelines for Design and Construction of Outpatient Facilities 451.2.2, 451.3.3, 451.3.3.1, 451.3.4,

451.3.5, 451.3.6, 451.3.8, 451.3.10, 451.3.13, 469.2.1.2

GHCF—18 Guidelines for Design and Construction of Residential Health, Care, and
  Support Facilities (First Printing 2018)

 450.2.2, 450.3.2, 450.3.3.1, 450.3.3.2, 450.3.3.3, 450.3.3.4,

450.3.3.5, 450.3.3.6, 450.3.4, 450.3.4.3, 450.3.4.4, 450.3.5, 450.3.6,
450.3.7, 450.3.8, 450.3.9, 450.3.11, 450.3.14, 450.3.15

**Revise as follows:**

FGI The Facility Guidelines Institute

9750 Fall Ridge Trail

St. Louis, MO 63127

Standard referenced number   Title

GHCF—~~18~~ 22 Guidelines for Design and Construction of Hospitals

GHCF—~~18~~ 22 Guidelines for Design and Construction of Outpatient Facilities

GHCF—~~18~~22 Guidelines for Design and Construction of Residential Health, Care, and

Support Facilities ~~(First Printing 2018)~~

(SP10484 AS)

FINA

Federation Internationale de Natation Amateur

Av. de l’ Avant-Poste 4

1005 Lausanne

SWITZERLAND

Standard Referenced
reference in code
number Title section number

CHG-22 FINA Handbook 1998—2000 454.1.2.2.1

FINA Handbook 2005—2009 454.1.2.7

Florida Codes

Florida Building Commission

Building Codes and Standards Office

Department of Business and Professional Regulation

2601 Blair Stone Road

Tallahassee, FL 32399

Standard Referenced
reference in code
number Title section number

FBC-A–Eight Edition (2023) Accessibility 101.4.8, 202, 315.6, 412.3.6, 413.3.6, 419.9, 453.10.2.7.7,

453.10.2.8.7, 453.27.4, 454.1.3.1.2, 457.1.4.1.1, 457.1.4.4.1, 457.1.4.4.2, 466.7.1.1,

467.2.2.2, 467.3.1.4, 467.9.2.1.3, 907.1.4, 907.9, 1003.3.4, 1003.5.1, 1004.6, 1009.1,

1010.1, 1010.1.9.8.1, 1010.7.1, 1011.6, 1011.7.1, 1011.17, 1012.1, 1012.2, 1012.3, 1012.6, 1012.6.1,

 1012.6.3, 1012.6.4, 1012.10, 1013.4, 1014.3, 1014.6, 1023.9, 1101.1.1, 3001.3, 3006.11

FBC-B– Eight Edition (2023) Building 101.4.9, 102.1.1, 102.2.2, 102.6.1, 117.1, 449.3.3.2, 449.3.5.1, 449.3.11.5,

449.4.2.2.5, 449.4.2.5.4, 449.4.2.6.1.1, 450.4.2.6.1.1, 451.3.10.12,

 453.5.5.1,

453.5.5.2, 453.13.7.1, 454.1.4.1, 454.1.4.2.3, 454.1.6.5.16.4.1, 454.1.6.5.16.5.1, 454.1.9.8.5,

454.1.11.7, 454.2.1.2, 454.2.16, 455.3.5, 456.3.5, 457.1.4.1.4, 460.6, 467.2.4, 467.6.1, 1523.2,

1523.5.1, 1524.1, 1609.1.2.4.1, 1625.4, 1905.1.2, 1905.1.5, 3115.2.4, 3115.4.1, 3115.4.4,

B201, B305.2, B306.2, B307.2.1, C406.2.1, C502.1, C602.1.5, E104.2, E201, E305.2, E306

FBC-EC– Eight Edition (2023) Energy Conservation 101.4.6, 201.3, 202, 1203.1, Table 1203.3, 1203.4.2, 1301.1.1, 1405.3.1

FBC-EB– Eight Edition (2023) Existing Building 101.4.7, 102.2, 102.6, 202, 449.1.3, 450.1.3, 451.1.3,

467.1.3, Table 504.3, Table 504.4, Table 506.2, 1011.5.2,

1507.1.1.1, 1511.1.1, 2701.1, 3109.1.1

FBC-FG– Eight Edition (2023) Fuel Gas 101.4.1, 201.3, 406.1.9, 415.9.2, 454.2.1.2, 454.2.15, 455.3.7, 456.3.6.1,

456.3.6.2, 2113.11.1.2, 2113.15, 2702.2.5, 2801.1, B201, E201

FBC-M– Eight Edition (2023) Mechanical 101.4.2, 201.3, 406.1.9, 409.3, 412.6.6, 414.1.2, 414.3, 415.9.1, 415.9.1.7, 415.9.2,

415.9.3, 415.11.11, 416.2.2, 416.3, 417.1, 419.8, 421.5, 426.1.4, 453.15.5, 454.2.1.2,

460.6.2, 460.7.2, 460.10.2, 603.1, 603.1.1, 603.1.2, 712.1.6, 717.2.2, 717.5.3, 717.5.4, 717.5.5,

717.6.1, 717.6.2, 717.6.3, 718.5, 720.1, 720.7, 903.2.11.4, 904.2.2, 904.12, 907.3.1, 909.1,

909.10.2, 909.13.1, 910.4.7, 1006.2.2.3, 1011.16, 1020.5.1, 1203.1, 1203.2.1, 1203.5.2,

1203.5.2.1, 1203.6, 1209.3, 2304.5, 2702.2.5, 2801.1, 3111.2, B201, C502.1, E201

Florida Codes—continued

FBC-P– Eight Edition (2023) Plumbing 101.4.3, 110.3, 201.3, 415.9.3, 449.3.9.1, 451.3.8.1, 452.2.15.1,

454.1.11.2, 454.2.1.2, 454.2.3, 454.2.8.1, 454.2.13.2, 455.3.2.1, 455.4.2, 456.3.1.1, 456.3.2.1,

457.1.4.1.2, 460.6.1, 603.1.2, 718.5, 903.3.5, 904.11.1.4, 912.6, 1206.3.3, 1503.4, 1503.4.1, 1503.4.2.1,

1514.4, 1514.4.2, 1514.4.3, 1524.1, 1805.4.3, 2901.1, Table P2902.1, 3111.2, 3305.1, B201, E201

FBC-R– Eight Edition (2023) Residential 101.2, 102.6.1, 105.15, 117.1, 305.2.3, 308.3.4, 308.4.2, 308.6.4,

310, 310.5.1, 310.5.2, 310.6, 1907.2, K111.1

FFPC– Eight Edition (2023) Florida Fire Prevention Code 101.4.5, 102.6, 102.6.2, 201.3, 202, 307.1, Table 307.1(1),

Table 307.1(2), 307.1.1, 403.4.5, 404.2, 406.7, 406.8, 407.2.5, 407.4, 410.3.6, 411.1, 412, 412.6.1,

413, 414.1.1, 414.1.2, 414.1.2.1, 414.2, 414.2.5, Table 414.2.5(1), Table 414.2.5(2), 414.3, 414.5,

414.5.1, Table 414.5.1, 414.5.2, 414.5.3, 414.6, 415, 415.6, 415.6.1, 415.6.1.1, 415.6.1.4, Table 415.6.2, 415.8.2,

415.9, 415.9.1, 415.9.1.3, 415.9.1.4, 415.9.1.6, 415.9.1.7, 415.9.1.8, 415.9.2, 415.9.3, 415.10, 415.11,

415.11.1.7, 415.11.4, 415.11.7.2, 415.11.9.3, 415.11.10.1, 416, 416.4, 422.3.1, 422.3.2, 426.1, 426.1.4, 451.2.1,

453.1, 453.2.1, 453.3.2,

 453.3.3, 453.3.5, 453.3.6, 453.4, 453.5.1, 453.5.13, 453.6.1, 453.7.7.1, 453.8.1,

453.8.1.3, 453.8.4, 453.8.5, 453.9.1, 453.10.6, 453.12.2, 453.13.1, 453.14.2, 453.14.2.1, 453.20.4, 453.21.1,

453.22.1, 453.26.1, 453.27.1, 453.27.9.1, 453.27.10.1, 453.27.15.3, 454.2.1.2, 455.4.3, 456.3.4, 457.1.3.1.1,

457.1.4.1.1, 457.1.4.2.13, 457.1.4.13.2, 457.2.2.1.1, 459.2, 459.2.3, 463.4, 467.3.1, 467.9.1, Table 504.3a,

Table 504.4a,b, Table 506.2a,b, 507.4, 507.8.1.1.1, 507.8.1.1.2, 507.8.1.1.3, Table 509, 705.8.1, 707.1, 901.2,

901.3, 901.5, 901.6.2, 901.6.3, 903.2.7.1, 903.2.11.3.1, Table 903.2.11.6, 903.2.12, 903.3.1.2.2, 903.3.1.2.3, 903.5,

904.2.2, 904.11.3, 905.1, 905.3.6, 905.3.7, 906.1, 906.4, 907.1.1, 907.2.5, 907.2.6, 907.2.13.2, 907.2.15, 907.2.16,

907.2.23, 907.2.24, 907.5.2.2, 907.6.6, 907.6.6.2, 907.8, 909.6.3, 909.12.1, 909.19, 909.20, 910.2.2, 910.5, 912.4.3,

916.2, 916.7, 916.10, 916.11, 917.1, 1001.3, 1001.4, 1001.9.7, 1203.5.2, 1203.6, 1507.16, 1507.18, Table 1604.5,

2603.4.1.12, 2701.1, 2702.1.3, 2702.2.3, 2702.2.7, 2702.2.10, 2702.2.13, 2702.2.14, 2702.4,

3003.3, 3007.9.1, 3008.1.3, 3102.1, 3103.1, 3111.2, 3111.3, 3111.3.4, 3111.3.5, 3302.3, 3303.7, 3309.2, 3601.2, B201, E201

61C-5 Rule 61C, Florida Administrative Code (Bureau of Elevator Safety Regulations) 3001.1

64E Rule 64E, Florida Administrative Code (Sewage Disposal) 454.1.1, 454.1.2.1, 454.1.10.3,

457.1.3.2.12, 457.1.4.13.2, 457.1.4.13.6, 457.2.3, 465.1, 465.4.7,

 465.5.1, 465.13.1.1, 2901.1

FS Florida Statutes 102.2, 102.2.1, 105.1.3, 105.1.4, 105.3, 105.3.1.2, 105.3.5, 105.5, 105.6,

105.8, 105.9, 105.14, 105.16, 105.17, 107.1, 107.3, 107.3.4.2, 107.6, 110.8.2,

110.8.3, 110.8.4.4, 110.8.5, 110.8.6, 117, 202, 307.1.1, 449.1.1, 449.1.4, 449.2, 449.3,

 450.1, 450.1.4,

 450.2, 451.1.1,451.1.4, 451.2, 451.2.1, 452.1, 453.1, 453.2.2, 453.3.1,

453.3.2, 453.3.3, 453.3.6, 453.4.3, 453.5.3, 453.8.7, 453.10.2.8.7, 453.10.7,

 453.13.8.1, 453.16.8,

453.25.6, 453.25.6.1, 453.25.6.2, 453.27.4, 453.27.9, 454.1.1, 454.1.11.1, 454.1.11.9, 455.1, 455.2,

455.3.1, 455.3.4, 455.4.3, 456.1,

 456.2, 456.3.4, 457.1.1, 457.1.2, 457.2, 458.1, 458.2.2, 459.1,

 461.1, 463.1, 463.5.2, 464.1, 464.2, 464.3, 464.4.1, 464.4.6.5, 465.1, 467.1,

 903.2.11.3.1, 1816.1.7,

 2901.1, 3001.1, 3001.2, 3001.6, 3010.1.1, 3010.1.3, 3109.2, Appendix B, Appendix C, C501, E102

FBC-TPHVHZ— Florida Building Code, Test Protocols for High Velocity Hurricane Zones

 RAS 109 1507.14, 1521.18, 1523.6.2.1

 RAS 111 1503.2.1, 1504.5, 1507.2.9, 1507.2.9.1, 1507.3.3.1, 1511.6, 1514.2, 1514.2.1,

1514.2.2, 1514.2.3, 1514.2.4, 1514.2.5.2, 1514.3, 1514.4.1,

1515.2.3.2, 1517.6.1, 1517.6.2.1, 1517.6.2.5, 1518.5.3, 1518.6.2, 1518.7.3.4,

1518.9.5, 1519.8, 1519.10, 1519.13, 1519.16.5, 1523.6.5.2.14, 1525

 RAS 113 1518.8.1.1

 RAS 115 1507.2, 1518.7, 1523.6.5.2.6.3

 RAS 117 1519.7, 1519.11, 1520.4, 1520.5, 1521.7.1, 1521.14.3

RAS 118 1518.8.1, 1507.3.2, 1507.3.3, 1507.3.3.1, 1507.3.8, 1507.3.9

 RAS 119 1518.8.1, 1507.3.2, 1507.3.3, 1507.3.3.1, 1507.3.8, 1507.3.9

 RAS 120 1518.8.1, 1507.3.2, 1507.3.3, 1507.3.3.1, 1507.3.8, 1507.3.9

 RAS 127 1518.8.5, 1518.8.6, 1523.6.5.2, 1523.6.5.2.2.2, 1523.6.5.2.2.3, 1523.6.5.2.3.2,

1523.6.5.2.3.3, 1523.6.5.2.6.2, 1525

 RAS 128 1525

 RAS 130 1507.8, 1507.9, 1518.10

 RAS 133 1518.9.2

 RAS 150 1519.1, 1525

 TAS 100 1523.6.5, 1523.6.5.1, 1523.6.5.2, 1523.6.5.2.4, 1523.6.5.2.4.1,

1523.6.5.2.5, 1523.6.5.2.6, 1523.6.5.2.7

 TAS 100A 1523.6.5.2.13

 TAS 101 1523.6.5.2.2, 1523.6.5.2.2.2, 1523.6.5.2.2.3

 TAS 102 1523.6.5.2.3, 1523.6.5.2.3.2, 1523.6.5.2.3.3, 1523.6.5.2.6.2, 1523.6.5.2.6.3

 TAS 102A 1523.6.5.2.3, 1523.6.5.2.3.2, 1523.6.5.2.3.3, 1523.6.5.2.6.2, 1523.6.5.2.6.3

 TAS 103 1523.6.5.2.1

 TAS 104 1523.6.5.2.1

 TAS 105 1513.1, 1519.7.1, 1521.7, 1521.11

 TAS 106 1512.4.2.4, 1523.6.5.2.2.4, 1523.6.5.2.3.4, 1523.6.5.2.6.4

 TAS 107 1504.3.3, 1507.2.7.1, 1507.17.8, 1518.11.3,

1523.6.5.1

Florida Codes—continued

 TAS 108 1523.6.5.2.2.1, 1523.6.5.2.2.2, 1523.6.5.2.2.3, 1523.6.5.2.3.1,

1523.6.5.2.3.2, 1523.6.5.2.3.3, 1523.6.5.2.6.1, 1523.6.5.2.6.2, 1523.6.5.2.6.3

 TAS 110 1515.1.3, 1515.1.4, 1515.2.5, 1520.1, 1520.4, 1523.1.1, 1523.6.2, 1523.6.2.1, 1523.6.3,

1523.6.5.2.4.1, 1523.6.5.2.6, 1523.6.5.2.7, 1523.6.5.2.8, 1523.6.5.2.9,

1523.6.5.2.12, 1523.6.5.2.13.1, 1523.6.5.2.14, 1523.6.5.2.15, 1523.6.5.2.16, 1523.6.5.2.17

 TAS 111A 1523.6.5.2.14

 TAS 111B 1523.6.5.2.14

 TAS 111C 1523.6.5.2.14

 TAS 112 1523.6.5.2

 TAS 114 1506.5, 1513.1, 1515.1.1, 1515.2.4,

1517.5.1, 1519.5.1, 1517.5.2

, 1520.4, 1523.6.2, 1523.6.2.1, 1523.6.3,

1523.6.5.2.9, 1523.6.5.2.10, 1523.6.5.2.11, 1506.6, 1506.7

 TAS 116 1513.1, 1523.6.5.2.2.1, 1523.6.5.2.3.1, 1523.6.5.2.6.1

 TAS 117 1523.6.5.2.9

 TAS 121 1523.6.5.2.12

 TAS 123 1518.8.1.1, 1523.6.5.2.15, 1523.6.5.2.17

 TAS 123A 1523.6.5.2.16

 TAS 124 1521.10, 1523.6.4

 TAS 125 1504.3.2,

1518.9.1, 1523.6.5.2.4.1

 TAS 126 1521.12

 TAS 135 1523.6.5.2.6

 TAS 201 449.4.2.5.1, 450.4.2.5.1, 1609.1.2, 1618.4.6.4,

1626.2.1, 1626.3, 1626.5.1, 1626.5.2, 1709.5.1, 2411.3.2.4

 TAS 202 449.4.2.5.1, 450.4.2.5.1

, 1010.1.7, 1405.1, 1626.5.1,

1626.5.3, 1709.5.1, 1709.5.2, 1709.5.2.1, 1709.8, 2411.3.2.1, 2411.3.2.1.1

 TAS 203 449.4.2.5.1, 450.4.2.5.1,

 1626.2.1, 1626.3.1, 1626.5.1, 1626.5.3, 1709.5.1, 2411.3.2.4

 TAS 301 1515.1.3

FM

Factory Mutual Global Research

Standards Laboratories Department

1151 Boston-Providence Turnpike

Norwood, MA 02062

Standard Referenced
reference in code
number Title section number

4430 (2012) Approval Standard for Heat and Smoke Vents 910.3.1

4470—2016 Approval Standard for Single-Ply Polymer-Modified Bitumen Sheet, Built-Up Roof (BUR)
  And Liquid Applied Roof Assemblies for use in Class 1 and
  Noncombustible Roof Deck Construction 1504.7, 1515.1.1, 1515.2.4

4471 (1992) Approval Standard for Class I Panel Roofs 1515.1.1, Table 1515.2, 1523.6.5.2.4.1

4474 (2011) American National Standard for Evaluating the Simulated Wind Uplift Resistance of
  Roof Assemblies Using Static Positive and/or Negative Differential Pressures 1504.3.1, 1504.3.3

4880—~~2015~~ 2017 Approval American National Standard for ~~Class 1 Rating of Building Panels or~~ Evaluating the Fire performance Insulated Building Panel Assemblies and Interior Finish Materials 2603.9

FRSA

Florida Roofing Sheet Metal and Air Conditioning Contractors Association

P.O. Box 4850

Winter Park, FL 32793

Standard Referenced
reference in code
number Title section number

FRSA/TRI
September 2018(09—18) Florida High Wind Concrete and Clay Roof Tile
  Installation Manual, Sixth Edition Revised 1507.3.2, 1507.3.3, 1507.3.3.1,

1507.3.7, 1507.3.8, 1507.3.9

**Revise as follows:**

**FRSA**

**Florida Roofing and Sheet Metal ~~and Air Conditioning~~ Contractors Association.**

**P.O. Box 4850**

**Winter Park, FL32793**

**FRSA/TRI Alliance**

**Florida High Wind Concrete and Clay Roof Tile Installation Manual, ~~Sixth~~ Seventh Edition ~~Revised~~**

**~~September~~ December 20~~18~~ 23 (~~09~~ 12—~~18~~ 22)**

**1507.3.2, 1507.3.3, 1507.3.3.1, 1507.3.7, 1507.3.8, 1507.3.9**

**(R9950 AS)**

FS

Federal Specification

941 Jefferson Davis Highway, Suite 104

Arlington, VA 22202

Standard Referenced
reference in code
number Title section number

TTC 555B Test Specification for Wind Driven Rain Infiltration Resistance 1523.6.2.1.1, 1523.6.3.1

GA

Gypsum Association

6525 Belcrest Road, Suite 480

Hyattsville, MD 20782

Standard Referenced
reference in code
number Title section number

GA 216—~~2016~~ 2018 Application and Finishing of Gypsum Panel Products Table 2508.1, 2509.2
GA 600—~~2015~~ 2018 Fire-Resistance and Sound Control Design Manual, ~~21st~~ 22nd Edition Table 721.1(1), Table 721.1(2), Table 721.1(3)

GSA

General Services Administration

1800 F Street, NW

Washington, DC 20405

Standard Referenced
reference in code
number Title section number

DD-G-451c (1977) Standard for Glass, Flat and Corrugated, for Glazing Mirrors

and Other Uses 2411.1.2

HPVA

Hardwood Plywood Veneer Association

1825 Michael Faraday Drive

Reston, VA 20190

Standard Referenced
reference in code
number Title section number

ANSI/HPVA HP-1—2016 American National Standard for Hardwood and Decorative Plywood 2303.3, 2304.7

ICC

International Code Council, Inc.

500 New Jersey Ave, NW

6th Floor

Washington, DC 20001

Standard Referenced
reference in code
number Title section number

ICC A117.1—09 Accessible and Usable Buildings and Facilities 202, 907.5.2.3.3, 1009.8.2, 1009.9,

1009.11, 1010.1.9.7, 1012.1, 1012.6.5,
1012.10, 1013.4, 1023.9, 1101.2, 1111.2,
1111.3, 1111.4, 1111.4.2

ICC 300—17 ICC Standard on Bleachers, Folding and Telescopic Seating and Grandstands 1029.1.1, 1029.17

Table 1607.1

ICC 400—17 Standard on Design and Construction of Log Structures 2301.2

ICC 500—14 ICC/NSSA Standard on the Design and Construction of
  Storm Shelters 202, 423.1, 423.1.1, 423.2, 423.3, 423.4,

453.9.1, 453.10.6, 453.25.4, 1604.5.1

ICC 600—14 Standard for Residential Construction in High-wind Regions 1609.1.1, 1609.1.1.1

SBCCI SSTD 11—97 Test Standard for Determining Wind Resistance of Concrete or Clay Roof Tiles 1504.2.1.1, 1504.2.1.2

Revise as follows:

**ICC**

1100-2018: Standard for Spray-applied Foam Plastic Insulation

**(F9324 / FS155-18 AS)**

**ICC**

International Code Council, Inc.500 New Jersey Ave NW 6th Floor

Washington DC 20001US

ICC A117.1-~~09~~ 2017:

Accessible and Usable Buildings and Facilities

**(S9437 / G127-18 AS)**

IEEE

Institute of Electrical and Electronics Engineers

2001 L Street, NW, Suite 700

Washington, DC 20036-491

0

Standard Referenced
reference in code
number Title section number

IEEE Appropriate standards for the type of equipment being protected 457.1.4.1.5, 449.3.15.5, 450.3.19.4

IESNA

Illuminating Engineering Society of North America

120 Wall Street, 17th Floor

New York, NY 10005-4001

Standard Referenced
reference in code
number Title section number

ANSI/IESNA RP-28-07 Lighting and the Visual Environment for Senior Living 450.3.15.3

ANSI/IESNA TM-15-11
Addendum A Backlight, Uplight, and Glare (BUG) Ratings Table 453.10.3.7(2)

ISO

International Organization for Standardization

ISO Central Secretariat

1 ch, de la Voie-Creuse, Case Postale 56

CH-1211 Geneva 20, Switzerland

Standard Referenced
reference in code
number Title section number

ISO 8115—86 Cotton Bales—Dimensions and Density Table 307.1(1), Table 415.11.1.1.1

ISO 8336—09 Fiber-Cement Flat Sheets - Product Specification and Test Methods 1404.10, 1405.16.1,

1405.16.2, Table 2509.2

MHI

Material Handling Institute

8720 Red Oak Blvd. Suite 201

Charlotte, NC 28217

Standard Referenced
reference in code
number Title section number

ANSI MH29.1—08 Safety Requirements for Industrial Scissors Lifts Table 3001.2

MIA

Marble Institute of America

28901 Clemens Road, Suite 100

Cleveland, OH 44145

Standard Referenced
reference in code
number Title section number

MIA (1998) Appropriate standards for marble selection, cutting and design 460.6.4, 460.7.1.3, 460.9.2

NAAMM

National Association of Architectural Metal Manufacturers

800 Roosevelt Road, Bldg. C, Suite 312

Glen Ellyn, IL 60137

Standard Referenced
reference in code
number Title section number

FP 1001—~~17~~ 18 Guide Specifications for Design of Metal Flag Poles 1609.1.1

NAAMM MBG 531—2017 Metal Grating Manual

 2214.3

NCMA

National Concrete Masonry Association

13750 Sunrise Valley

Herndon, VA 22071-4662

Standard Referenced
reference in code
number Title section number

TEK 5—84 (~~1996~~2005) Details for Concrete Masonry Fire Walls Table 721.1(2)

NFPA

National Fire Protection Association

1 Batterymarch Park

Quincy, MA 02169-7471

Standard Referenced
reference in code
number Title section number

10—~~18~~ 21 Standard for Portable Fire Extinguishers 453.15.3, 906.2, 906.3.2,

906.3.4, Table 906.3(1), Table 906.3(2)

11—16 Standard for Low **Low-, Medium, and High** Expansion Foam 904.7

12—~~15~~18 Standard on Carbon Dioxide Extinguishing Systems 904.8, 904.12

12A—~~15~~ 18 Standard on Halon 1301 Fire Extinguishing Systems 904.9

13—~~16~~ 19 Installation of Sprinkler Systems 461.1, 712.1.3.1, 903.3.1.1,

903.3.2, 903.3.8.2, 903.3.8.5, 904.12, 905.3.4, 907.6.4, 1019.3

13D—~~16~~ 19 Standard for the Installation of Sprinkler Systems in One- and Two-family
  Dwellings and Manufactured Homes 903.2.11.3, 903.3.1.3

13R—~~16~~ 19 Standard for the Installation of Sprinkler Systems in
  Low Rise Residential Occupancies 903.2.11.3, 903.3.1.2, 903.3.5.2, 903.4

14—~~16~~ 19 Standard for the Installation of Standpipe and Hose System 905.2, 905.3.4, 905.4.2, 905.6.2,

905.8, 3002.10

16—~~15~~ 19 Standard for the Installation of Foam-water Sprinkler and Foam-water Spray Systems 904.7, 904.12

17—~~17~~ 20 Standard for Dry Chemical Extinguishing Systems 904.6, 904.12

17A—~~17~~ 20 Standard for Wet Chemical Extinguishing Systems 904.5, 904.12

20—~~16~~ 19 Standard for the Installation of Stationary Pumps for Fire Protection 412.3.4.1, 449.3.10,

450.3.13.1, 451.3.9.1, 904.10, 913.1, 913.2.1, 913.5

30—~~18~~ 21 Flammable and Combustible Liquids Code 415.6, 468.3.6.5, 507.8.1.1.1, 507.8.1.1.2

30A—~~18~~ 21 Code for Motor Fuel-Dispensing Facilities and Repair Garages 406.1.9.2

31—~~15~~ 20 Standard for the Installation of Oil-burning Equipment 2113.15

32—16 Standard for ~~Dry Cleaning Plants~~ Dry cleaning Facilities 415.9.3

40—~~16~~ 19 Standard for the Storage and Handling of Cellulose Nitrate Film 409.1

45-19 Standard on Fire Protection for Laboratories Using Chemicals (2015 Edition)

55-19 Compressed Gases and Cryogenic Fluids Code

58—~~17~~ 20 Liquefied Petroleum Gas Code 415.9.2

61—~~17~~ 20 Standard for the Prevention of Fires and Dust Explosions in Agricultural and Food Product Facilities 426.1

70—~~17~~ 20 National Electrical Code (NEC) 108.3, 406.1.7, 406.1.9, 415.11.1.8, 449.4.2.9.1, 450.4.2.9.1,

450.4.2.9.6.4, 453.17.8, 453.25.5, 453.25.5.2, 454.1.10.4.2,

457.1.4.1.5, 464.4.2.2.1, 469.4.14.1, 469.4.14.7.1, 469.4.14,

 453.17.8,

Table 509, 904.3.1,

 907.6.1, 909.12.2, 909.16.3, 910.4.6, 1205.4.1,

 2701.1, 2702.1.3, H106.1, H106.2, H115, K101, K111.1

72—~~16~~ 19 National Fire Alarm and Signaling Code 407.4.4.3, 407.4.4.5, 407.4.4.5.1, 449.3.12.2, 450.3.16.2,

453.7.7, 466.7.1.1, 466.7.1.2, 466.7.2, 466.10.5.1, 466.10.5.2,

469.4.14.10.1, 901.6, 903.4.1, 904.3.5, 907.1.2, 907.2, 907.2.6, 907.2.11,

907.2.13.2, 907.3, 907.3.3, 907.3.4, 907.5.2.1.2, 907.5.2.2, 907.5.2.2.5,

907.6, 907.6.1, 907.6.2, 907.6.6, 907.7, 907.7.1, 907.7.2, 907.2.9.3,

911.1.6, 2702.2.4, 3002.10, 3005.5, 3007.7

74—89 Standards for the Installation, Maintenance and Use of Household Fire Warning Equipment 461.1

80—~~16~~ 19 Standard for Fire Doors and Other Opening Protectives 410.3.5, 509.4.2, 716.1, 716.5.7,

716.5.8.1, 716.5.9.2, 716.6.4, 717.4.1.2, 1010.1.4.3

82—~~14~~ 19 Standard on Incinerators and Waste and Linen Handling Systems and Equipment 713.13

85—~~15~~ 19 Boiler and Combustion System Hazards Code 426.1

91—04 Exhaust Systems for Air Conveying of Vapors, Gases, Mists, and
  Noncombustible Particulate Solids 468.3.6.5

92—~~15~~ 18 Standard for Smoke Control Systems 909.7, 909.8

96—2017 Standard for Ventilation Control and Fire Protection of Commercial
  Cooking Operations 466.6.2

99—~~18~~21 Health Care Facilities Code 407.10, 425.1, 422.6, 449.3.11.10, 449.3.13, 449.3.13.7,

449.3.14.1, 449.4.2.9.1, 450.3.12, 450.3.14.3, 450.3.17, 450.3.18.1,

450.4.2.9.1, 451.3.13.1, 451.3.15, 469.4.11.1.1, 469.4.11.1.2,

469.4.14.1, 469.4.14.7.1, 469.4.14.9.3

101—~~18~~  21 Life Safety Code 449.2.1, 449.3.14.4, 450.3.18.4, 451.3.13.5, 453.6.1, 453.14.2.1,

453.27.9.1, 453.27.10.1, 457.1.3.1.1, 457.1.4.1.1, 457.1.4.2.13,

457.1.4.13.2, 457.2.2.1.1, 457.1.4.13.2, 467.3.2.2, 469.3.1, 469.3.2,

469.4.14.10.1

, 903.2.11.3.1, 1029.6.2

105—~~16~~ 19 Standard for Smoke Door Assemblies and Other Opening Protectives 405.4.2, 710.5.2.2,

716.5.3.1, 717.4.1.2, 909.20.4.1, 2702.1.3

110—~~16~~ 19 Standard for Emergency and Standby Power Systems 449.3.14.1, 449.3.14.3, 449.3.14.7,

449.3.14.10, 450.3.18.1, 450.3.18.3, 451.3.13.1,

451.3.13.3, 467.2.8.1, 469.4.14.9.2, 2702.1.2

111—~~16~~ 19 Standard on Stored Electrical Energy Emergency and Standby Power Systems 469.4.14.9.2, 2702.1.3

113-19 Standard on Stored Electrical Energy Emergency and Standby Power Systems

120—~~15~~ 20 Standard for Fire Prevention and Control in Coal Mines 426.1

170—18 Standard for Fire Safety and Emergency Symbols 1025.2.6.1

211—~~16~~ 19 Standard for Chimneys, Fireplaces, Vents and Solid Fuel-burning Appliances 2112.5

221—~~18~~21 Standard for High Challenge Fire Walls, Fire Walls, and Fire Barrier Walls 706.2

252—17 Standard Methods of Fire Tests of Door Assemblies Table 716.3, 716.3.1, 716.4,

716.5.1, 716.5.3, 716.5.4, 716.5.5.1, 716.5.8.1.1

253—~~15~~ 19 Standard Method of Test for Critical Radiant Flux of Floor Covering Systems
  Using a Radiant Heat Energy Source 406.1.4, 406.8.3, 424.2, 804.2, 804.3

257—17 Standard for Fire Test for Window and Glass Block Assemblies Table 716.3, 716.4, 716.5.3.2, 716.6,

716.6.1, 716.6.2, 716.6.7.3

259—18 Standard Test Method for Potential Heat of Building Materials 2603.4.1.10, 2603.5.3

265—~~2015~~ 2019 Standard Methods of Fire Tests for Evaluating Room Fire Growth
 Contribution of Textile or Expanded Vinyl Wall Coverings on Full Height Panels and Walls 803.1.3, 803.1.3.1

268—2017 Standard Test Method for Determining Ignitability of Exterior
  Wall Assemblies Using a Radiant Heat Energy Source 1406.2.1.1, 1406.2.1.1.1, 1406.2.1.1.2,

2603.5.7, D105.1, D106

275—17 Standard Method of Fire Tests for the Evaluation of Thermal Barriers 1407.10.2, 1409.10.2, 2603.4

276—~~15~~ 19 Standard Method of Fire Tests for Determining the Heat Release Rate of
  Roofing Assemblies With Combustible Above-Deck Roofing Components 1508.1, 2603.3, 2603.4.1.5

285—12 Standard Fire Test Method for the Evaluation of Fire Propagation Characteristics of
  Exterior Nonload-bearing Wall Assemblies Containing Combustible Components 718.2.6, 1403.5,

1407.10.4, 1409.10.4,
1510.6.2, 2603.5.5

286—~~15~~  19 Standard Methods of Fire Test for Evaluating Contribution of
  Wall and Ceiling Interior Finish to Room Fire Growth 402.6.4.4, 803.1.2, 803.1.2.1, 803.11,

1407.10.3, 2603.7, 2603.9, 2604.2.4, 2614.4

288—17 Standard Methods of Fire Tests of Horizontal Fire Door Assemblies
  Installed in Horizontal in Fire-resistance-rated Floor Systems 712.1.13.1

289—~~13~~ 19 Standard Method of Fire Test for Individual Fuel Packages 402.6.2, 402.6.4.5, 424.2, 806.4

409—16 Standard for Aircraft Hangars 412.4.6, Table 412.4.6, 412.4.6.1, 412.6.5

418—16 Standard for Heliports 412.8.4

484—~~18~~ 19 Standard for Combustible Metals 426.1

NFPA—continued

652-19 Standard on the Fundamentals of Combustile Dust

654—~~17~~  20 Standard for the Prevention of Fire & Dust Explosions from the Manufacturing,
  Processing and Handling of Combustible Particulate Solids 426.1

655—17 Standard for the Prevention of Sulfur Fires and Explosions 426.1

664—~~17~~ 20 Standard for the Prevention of Fires and Explosions in Wood Processing and
  Woodworking Facilities 426.1

701—~~15~~ 19 Standard Method of Fire Tests for Flame-Propagation of Textiles and Films 410.3.6, 424.2, 801.4, 806.1,

806.3, 806.4, 3102.3, 3102.3.1,
3102.6.1.1, 3105.3.4.1, 3105.4, 3105.6, D102.2.8, D106, H106.1.1, H115

704—17 Standard System for the Identification of the Hazards of
  Materials for Emergency Response 202, 415.5.2

750—~~15~~ 19 Standard on Water Mist Fire Protection Systems 202, 904.11.1.1

780—17 Standard for the Installation of Lightning Protection Systems 449.3.15.1, 450.3.19.1, 453.17.7

1124—17 Code for the Manufacture, Transportation and Storage of Fireworks and
  Pyrotechnic Articles 415.6.1.1

2001—~~15~~ 20 Standard on Clean Agent Fire Extinguishing Systems 904.10

2010-20 Standard for Fixed Aerosol Fire-extinguishing Systems

C618-12a Standard Specification for Coal Fly Ash and Raw or Calcined Natural Pozzolan
  for Use in Concrete 1917.4.4

C869—11 Specification for Foaming Agents Used in Making Preformed Foam for Cellular
  Concrete Table 1508.2, 1917.4.5

Ann Arbor, MI 48113-0140, USA

Standard Referenced
reference in code
number Title section number

NSF 50—11 Equipment for Pools, Spas, Hot Tubs, and Other Recreational
  Water Facilities 454.1.1, 454.1.2.1, 454.1.6.5.1, 454.1.6.5.16,

 454.1.6.5.16.4.2,

454.1.6.5.16.5.2, 454.1.9.2.5.2, 454.1.9.8.6.1, 454.1.10.3, 454.1.11.9

NSF 60—05 Drinking Water Treatment Chemicals—Health Effects 454.1.2.1, 454.1.6.5.18, 454.1.11.19

**NFPA**

Also – revise as follows:

68—13: Standard on Explosion Protection by Deflagration Venting

**(F9815/F168-18 AS)**

NFPA 275—17 Standard Method of Fire Tests for the Evaluation of Thermal Barriers

508.4.4.1, 509.4.1, 1407.10.2, 1409.10.2, 2603.4

**(S10353 AS)**

PCI

Precast Prestressed Concrete Institute

200 West Adams Street, Suite 2100

Chicago, IL 60606-6938

Standard Referenced
reference in code
number Title section number

MNL 124—~~11~~  18 ~~Design~~Specification for Fire Resistance of Precast Prestressed Concrete 722.2.3.1

MNL 128—~~01~~ 19 ~~Recommended Practice~~ Specification for Glass Fiber Reinforced Concrete Panels 1903.3

**Update standard(s) as follows:**

PCI

Precast Prestressed Concrete Institute 200 West Adams Street, Suite 2100 Chicago IL 60606-6938

US

~~MNL~~ PCI 124-~~11~~18:

~~Design~~ Specification for Fire Resistance of Precast Prestressed Concrete

**(F9282 / FS77-18 AS)**

PTI

Post-Tensioning Institute

38800 Country Club Drive

Farmington Hills, MI 48331

Standard Referenced
reference in code
number Title section number

PTI DC—10.5-~~12~~ 19 Standard Requirements for Design and Analysis of Shallow Post-Tensioned Concrete
  Foundations on Expansive and Stable Soils 1808.6.2

RCSC

Research Council on Structural Connections

c/o Stanley D. Lindsey & Assoc. Ltd.

2244 Metro Center Blvd., Suite 208

Nashville, TN 37228-1320

Standard Referenced
reference in code
number Title section number

RCSC—14 Specification for Structural Joints Using High Strength Bolts 2214.3

RCSC-20~~14~~, Specification for Structural Joints Using High-Strength Bolts, 2020             2214.3

**(S10135 AS)**

RMI

Rack Manufacturers Institute

8720 Red Oak Boulevard, Suite 201

Charlotte, NC 28217

Standard Referenced
reference in code
number Title section number

ANSI/MH16.1—12 Specification for Design, Testing and Utilization of Industrial Steel Storage Racks 2209.1

ANSI/MH16.3—16 Specification for the Design, Testing, and Utilization of Industrial Steel
  Cantilevered Storage Racks 2209.2

SBCA

Structural Building Components Association

6300 Enterprise Lane

Madison, WI 53719

Standard Referenced
reference in code
number Title section number

ANSI/FS 100-12(R2018) Standard Requirements for Wind Pressure Resistance of Foam Plastic Insulating
  Sheathing Used in Exterior Wall Covering Assemblies 2603.10

SDI

Steel Deck Institute

P. O. Box 25

Fox River Grove, IL 60021

Standard Referenced
reference in code
number Title section number

ANSI/SDI NC—2017 Standard for Noncomposite Steel Floor Deck 2210.1.1.1, 2214.3

ANSI/SDI RD—2017 Standard for Steel Roof Deck 2210.1.1.2, 2214.3

DDM—04 Diaphragm Design Manual 2214.3, 2222.4

ANSI/SDI C—2017 Standard for Composite Steel Floor Deck Slabs 2210.1.1.3, 2214.3

Update standards as follows:

SDI

DDM04-15~~DDM--04~~, Diaphragm Design Manual, 4th Edition, 2015, with Addendum 1 (2015) and Addendum 2 (2016)             2214.3, 2222.4

**(S10133 AS)**

SJI

Steel Joist Institute

234 W. Cheves Street

Florence, SC 29501

Standard Referenced
reference in code
number Title section number

SJI-100—15 Standard Specification for K-Series, LH-Series, and DLH-Series Open Web
  Steel Joists and for Joist Girders, 2015 1604.3.3, 2203.2, 2207.1

SJI-200—15 Standard Specification for Composite Steel Joists, CJ-series 1604.3.3, 2203.2, 2207.1

SJI—07 Structural Design of Steel Joist Roofs to Resist Ponding Loads, Technical Digest No. 3 2214.3

SJI—15 Vibration of Steel Joist-Concrete Slab Floors, Technical Digest No. 5 2214.3

SJI—12 Design of Steel Joist Roofs to Resist Uplift Loads, Technical Digest No. 6 2214.3

SJI—08 Welding of Open Web Steel Joist and Joist Girders, Technical Digest No. 8 2214.3

SJI—08 Handling and Erection of Steel Joists and Joist Girders, Technical Digest No. 9 2214.3

SJI—17 44th Edition Standard Specifications Load Tables and Weight Tables for Steel
  Joists and Joist Girders 2214.3

SJI—18 90 Years of Open Web Steel Joist Construction 2214.3

SJI-07 Design of Lateral Load Resisting Frames Using Steel Joists and
  Joist Girders, Technical Digest No. 11 2214.3

|  |
| --- |
| Update standards as follows:SJISteel Joist Institute140 W. Evans~~234 W. Cheves~~StreetFlorence, SC 29501SJI-100—15Standard Specification for K-Series, LH-Series, and DLH-Series Open Web Steel Joists and for Joist Girders, 20151604.3.3, 2203.2, 2207.1SJI-200—15Standard Specification for Composite Steel Joists, CJ-series, 20151604.3.3, 2203.2, 2207.1SJI—18~~07~~Structural Design of Steel Joist Roofs to Resist Ponding Loads, Technical Digest No. 3, 20182214.3SJI—15Vibration of Steel Joist-Concrete ~~Slab~~Floors, Technical Digest No. 5, 20152214.3SJI—12Design of Steel Joist Roofs to Resist Uplift Loads, Technical Digest No. 6, 20122214.3SJI—20~~08~~Welding of Open Web Steel Joist and Joist Girders, Technical Digest No. 8, 20202214.3SJI—08Handling and Erection of Steel Joists and Joist Girders, Technical Digest No. 9, 20082214.3SJI—20~~17~~45~~44~~th Edition Standard Specifications Load Tables and Weight Tables for Steel Joists and Joist Girders, 20202214.3SJI—1890 Years of Open Web Steel Joist Construction, 20182214.3SJI-21~~07~~Design of Lateral Load Resisting Frames Using Steel Joists and Joist Girders, Technical Digest No. 11, 20212214.3 |

**(S10416 AS)**

SPRI

Single-Ply Roofing Institute

411 Waverly Oaks Road, Suite 331B

Waltham, MA 02452

Standard Referenced
reference in code
number Title section number

ANSI/SPRI/
FM4435-ES-1—~~11~~ 17 Wind Design Standard for Edge Systems Used with Low Slope Roofing Systems 1504.5

ANSI/SPRI RP-4—~~13~~ 18 Wind Design Guide for Ballasted Single-ply Roofing Systems 1504.4

ANSI/SPRI VF-1 -17 External Fire Design Standard for Vegetative Roofs

**(R10119 AS)**

**Update standards as follows:**

**SPRI**

GT-1-2016: Test Standard for Gutter Systems

**(R9511 / S17-19 AMPC2)**

ANSI/SPRI/FM4435-ES-1—~~11~~17

Wind Design Standard for Edge Systems Used with Low Slope Roofing Systems

**(R10119 AM with A1)**

STI

Steel Tube Institute

2516 Waukegan Road, Suite 172

Glenview, IL 60025

Standard Referenced
reference in code
number Title section number

C1670—16 Standard Specification for Adhered Manufactured Stone Masonry Veneer Units 2103.1

FMA/WDMA 250—10 Standard Practice for the Installation of Non-Frontal Flange Windows with

HSS Design Manual, Volume 3 Connections at HSS Members, 2016 2214.3

HSS Design Manual, Volume 4 Truss & Bracing Connections, 2017 2214.3

Update standards as follows:

STI

Steel Tube Institute

2516 Waukegan Road, Suite 172

Glenview, IL 60025

STI, 2021. HSS Design Manual, Volume 1: Section Properties & Design Information, Steel Tube Institute, 2021

~~HSS Design Manual, Volume 1 Section Properties & Design Information, 2015~~

2214.3

STI, 2021. HSS Design Manual, Volume 2A: Member Design 2016, Steel Tube Institute, 2021

2214.3

STI, 2021. HSS Design Manual, Volume 2B: Member Design 2016, Steel Tube Institute, 2021

~~HSS Design Manual, Volume 2 Member Design, 2016~~

2214.3

STI, 2021. HSS Design Manual, Volume 3: Connections at HSS Members 2016, Steel Tube Institute, 2021

~~HSS Design Manual, Volume 3 Connections at HSS Members, 2016~~

2214.3

STI, 2021. HSS Design Manual, Volume 4: Truss & Bracing Connections 2016, Steel Tube Institute, 2021

~~HSS Design Manual, Volume 4 Truss & Bracing Connections, 2017~~

2214.3

(S10420 AS)

TECO

Timber Company, Inc.

2402 Daniels Street

Madison, WI 53704

Standard Referenced
reference in code
number Title section number

TECO PRP-133 Performance Standards and Policies for Structural Use Panels 2314.4.8

TIA

Telecommunications Industry Association

1320 N. Courthouse Road

Arlington, VA 22201-3834

Standard Referenced
reference in code
number Title section number

ANSI/TIA 222-H—2017 Structural Standard~~s~~  for Antenna Supporting Structures and Antennas
  and Small Wind Turbine Support Structures 1609.1.1, 3108.1, 3108.2

TMS

The Masonry Society

105 South Sunset Street, Suite Q

Longmont, CO 80501

Standard Referenced
reference in code
number Title section number

216—2013 Standard Method for Determining Fire Resistance of Concrete
  and Masonry Construction Assemblies Table 721.1(2), 722.1

302—~~2012~~ 2018 Standard Method for Determining the Sound Transmission Class Rating for Masonry Walls 1207.2.1

402—2016 Building Code for Masonry Structures 1405.6, 1405.10, 1604.3.4, 1807.1.6.3.2,

1808.9, 2101.2, 2105.1, 2106.1, 2107.1, 2107.2, 2107.3,
2107.4, 2107.6, 2108.1, 2108.4, 2109.1, 2109.4, 2110.1, 2114.2,

2122.1, 2122.4, 2122.5, 2122.7, 2122.8.2, 2122.8.4, 2122.10

403—2017 Direct Design Handbook for Masonry Structures 2101.2

TMS 404—16 Standard for the Design of Architectural Cast Stone 2101.2

TMS 504—16 Standard for the Fabrication of Architectural Cast Stone 2103.1

TMS 604—16 Standard for the Installation of Architectural Cast Stone 2104

602—2016 Specification for Masonry Structures 1405.6.1, 1807.1.6.3, 2103.1,

2103.2.1, 2103.3, 2103.4, 2104.1, 2105.1, 2108.1, 2121.1.6, 2122.1, 2122.2.3,

2122.3, 2122.4, 2122.7.4, 2122.8.1, 2122.8.2, 2122.8.3, 2122.8.4, 2122.8.6, 2122.8.8

TPI

Truss Plate Institute

218 N. Lee Street, Suite 312

Alexandria, VA 22314

Standard Referenced
reference in code
number Title section number

TPI 1—2014 National Design Standard for Metal-plate-connected Wood Truss Construction 2303.4.6, 2306.1,

2319.17.2.1.1, 2319.17.2.2.8

UL

UL LLC

333 Pfingsten Road

Northbrook, IL 60062-2096

Standard Referenced
reference in code
number Title section number

9—2009 Fire Tests of Window Assemblies—with Revisions through February 2015 Table 716.3, 716.3.2,

716.4, 716.5.3.2, 716.6, 716.6.1, 716.6.2, 716.6.7.3

10A—2009 Tin Clad Fire Doors—with Revisions through ~~December 2013~~ July 2018 716.5

10B—2008 Fire Tests of Door Assemblies—with Revisions through February 2015 716.3.1, Table 716.3,

716.5.2, 716.5.4, 716.5.5.1, 716.5.8.1.1

10C—~~2009~~ 2016 Positive Pressure Fire Tests of Door Assemblies~~—with Revisions through February 2015~~  Table 716.3,

716.3.1, 716.5.1, 716.5.3, 716.5.4, 716.5.5.1, 716.5.8.1.1, 1010.1.10.1

14B—2008 Sliding Hardware for Standard Horizontally mounted Tin Clad Fire Doors—
  with Revisions through ~~May 2013~~ July 2017 716.5

14C—06 Swinging Hardware for Standard Tin Clad Fire Doors Mounted Singly and in Pairs—
  with Revisions through ~~May 2013~~ July 2017 716.5

55A—04 Materials for Built-Up Roof Coverings 1507.10.2

103—2010 Factory-built Chimneys, for Residential Type and Building Heating Appliances—
  with Revisions through ~~July 2012~~ July 2017 718.2.5.1

127—2011 Factory-built Fireplaces—with Revisions through ~~May 2015~~ May 2016 718.2.5.1, 2111.12

181—05 Standard for Factory-Made Air Ducts and Air Connectors 449.3.6.4, 451.3.6.3, 451.3.6.3.4

199E—04 Outline of Investigation for Fire Testing of Sprinklers and
  Water Spray Nozzles for Protection of Deep Fat Fryers 904.12.4.1

217—~~06~~ 15 Single and Multiple Station Smoke Alarms—with Revisions through ~~October 2015~~ November 2016 907.2.11

263—11 Standard for Fire Tests of Building Construction and Materials—with Revisions through
  ~~June 2015~~ March 2018 703.2, 703.2.1, 703.2.3, 703.2.5, 703.3, 703.4, 703.6,

704.12, 705.7, 705.8.5, 707.6, 712.1.13, 714.4.1.1, 714.5.1, 715.1, 716.2,

Table 716.3, 716.5.6, 716.5.8.1.1, Table 716.6, 716.7.1, 717.3.1, 717.5.2,

717.5.3, 717.6.1, 717.6.2.1, Table 721.1(1), 2103.1, 2603.5.1

268—~~09~~ 2016 Smoke Detectors for Fire Alarm Systems-with revisions through July 2016 407.8, 907.2.6.2, 907.2.11.7

294—~~1999~~ 2018 Access Control System Units—with Revisions through ~~February 2015~~ October 2018 1010.1.9.7, 1010.1.9.8,

1010.1.9.9, 1010.1.9.10

300—05(R2010) Fire Testing of Fire Extinguishing Systems for Protection of
  Commercial Cooking Equipment—with Revisions through December 2014 904.12

300A—06 Outline of Investigation for Extinguishing System Units for Residential Range
  Top Cooking Surfaces 407.2.6, 904.13

305—2012 Panic Hardware—with Revisions through ~~August 2014~~ March 2017 1010.1.10.1

325—~~02~~ 2017 Door, Drapery, Gate, Louver and Window Operations and Systems—
  with Revisions through ~~May 2015~~ 406.1.1, 3110.4

555—2006 Fire Dampers—with Revisions through ~~May 2014~~ October 2016 717.3

555C—~~2006~~ 2014 Ceiling Dampers—with Revisions through ~~December 2014~~ May 2017 717.3

555S—~~99~~  2014 Smoke Dampers—with Revisions through ~~February 2014~~ October 2016 717.3.1

580—2006 Test for Uplift Resistance of Roof Assemblies—with Revisions through
  ~~October 2013~~ October 2018 1504.3.1, 1504.3.2, 1504.3.3, 2222.4.6

641—2010 Type L Low-temperature Venting Systems—with Revisions through ~~June 2013~~ April 2018 2113.11.1.4

710B—2011 Recirculating Systems—with Revisions through August 2014 904.12

723—~~2008~~ 2018 Standard for Test for Surface Burning Characteristics of
 Building Materials~~—with Revisions through August 2013~~ 202, 402.6.4.4, 406.7.2,

703.5.2, 720.1, 720.4, 803.1.1, 803.1.4, 803.10, 803.11, 806.7,
1403.5, 1404.12.1, 1407.9, 1407.10.1,1409.9, 1409.10.1, 1510.6.2,
1510.6.3, 2303.2, 2603.3, 2603.4.1.13, 2603.5.4, 2603.5.5, 2606.3.5.4,
2603.7.1, 2604.2.4, 2606.4, 2612.3, 2614.3, 3105.3.4.1, D102.2.8, D106

790—04 Standard Test Methods for Fire Tests of Roof Coverings—
  with Revisions through ~~July 2014~~ October 2018 1505.1, 1513.1, 1516.1, 2603.6, 2610.2, 2610.3

793—08 Standards for Automatically Operated Roof Vents for Smoke and Heat—
  with Revisions through ~~September 2011~~ March 2017 910.3.1

864—~~03~~ 2014 Standards for Control Units and Accessories for Fire Alarm Systems—
  with Revisions through ~~December 2014~~ March 2018 909.12

924—~~06~~ 2016 Standard for Safety Emergency Lighting and Power Equipment—
  with Revisions through ~~April 2014~~ May 2018 1013.5

1040—96 Fire Test of Insulated Wall Construction—
  with Revisions through ~~October 2012~~ April 2017 1407.10.3, 1409.10.3, 2603.9

1069—07 Hospital Signaling and Nurse Call Equipment, 7th Edition 449.3.13.1, 450.3.17, 451.3.11.1, 467.8.3.6

UL—continued

1256—02 Fire Test of Roof Deck Construction—
  with Revisions through ~~January 2007~~ August 2018 1508.1, 2603.3, 2603.4.1.5

1479—~~03~~ 2015 Fire Tests of Through-penetration Firestops~~—~~  ~~with Revisions through June 2015~~ 202, 714.4.1.2, 714.5.1.2, 714.5.4

1482—2011 Solid-Fuel-type Room Heaters—with Revisions through August 2015 2112.2, 2112.5

1703—02 Flat-Plate Photovoltaic Modules and Panels—
  with Revisions through ~~October 2015~~ September 2018 1505.8, 1505.9, 1507.17.6, 1510.7.4, 1518.11.1, 3111.3.1

1715—97 Fire Test of Interior Finish Material—
  with Revisions through ~~January 2013~~ April 2017 1407.10.3, 1409.10.2, 1409.10.3, 2603.4, 2603.9, 2614.4

1741-2010 Inverters, Converters, Controllers and Interconnection System Equipment for Use with Distributed Energy Resources—with Revisions through February 2018

1777—2007 Chimney Liners—with Revisions through ~~October 2015~~ April 2014 2113.11.1, 2113.19

1784—~~01~~ 2015 Air Leakage Tests of Door Assemblies—  ~~with Revisions through February 2015~~ 405.4.3, 710.5.2.2, 710.5.2.2.1, 716.5.3.1, 716.5.7.1,

716.5.7.3, 3006.3, 3007.6.3, 3008.6.3

1897—~~12~~ 2015 Uplift Tests for Roof Covering Systems—~~with Revisions through September 2015~~ 1504.3.1

1975—06 Fire Test of Foamed Plastics Used for Decorative Purposes 402.6.2, 402.6.4.5, 424.2

1994—~~04~~ 2015 Luminous Egress Path Marking Systems—
  ~~with Revisions through May 2015~~ 411.7, 1008.2.1, 1025.2.1, 1025.2.3, 1025.2.4, 1025.2.5

2017—2008 Standards for General-purpose Signaling Devices and Systems—
  with Revisions through May 2011 454.2.17.1.9

2034—~~2008~~ 2017 Standard for Single- and Multiple-Station Carbon Monoxide Alarm—
  with Revisions through ~~March 2015~~ September 2018 202

2075—2013 Standard for Gas and Vapor Detectors and Sensors –with revisions through December 2017 202

2079—~~04~~ 2015 Tests for Fire Resistance of Building Joint Systems—
  ~~with Revisions through August 2015~~ 202, 715.3, 715.6

2196—~~2001~~ 2017 ~~Tests~~ Standard for Fire ~~Resistive Cables—with Revisions through March 2012~~ Test for Circuit Integrity of Fire –Resistive Power, Instrumentation, Control and Date Cables 909.20.6.1, 913.2.2,

2702.3, 3007.8.1, 3008.8.2

2200—2012 Stationary Engine Generator Assemblies—with Revisions through ~~July~~ October 2015 2702.1.1

2202—09 (2012) Standard for Electric Vehicle (EV) Charging System ~~Equipment~~ Equipment-with revisions through February 2018, ~~2013~~ 406.1.7

2594—~~13~~ 2016 Standard for Electric Vehicle Supply Equipment, 2013 406.1.7

2703-2014 Mounting Systems, Mounting Devices, Clamping/Retention Devices and Ground Lugs for Use with Flat-plate Photovoltaic Modules and Panels -with revisions through December 2019

**Add new standard(s) follows:**

UL

UL LLC 333 Pfingsten Road Northbrook IL 60062-2096

723S-2006:

Drop-Out Ceilings Installed Beneath Automatic Sprinklers

**(F9325 / FS158-18 AS)**

UL 723—~~2008~~2018 Standard for Test for Surface Burning Characteristics of Building Materials—with Revisions through August 2013

202, 402.6.4.4, 406.7.2, 602.4.1.1, 602.4.2.1, 602.4.3.1, 703.5.2, 720.1, 720.4, 803.1.1, 803.1.4, 803.10, 803.11, 806.7, 1403.5, 1404.12.1, 1407.9, 1407.10.1,1409.9, 1409.10.1, 1510.6.2, 1510.6.3, 2303.2, 2603.3, 2603.4.1.13, 2603.5.4, 2603.5.5, 2604.2.4, 2606.4, 2612.3, 2614.3, 3105.3.4.1, D102.2.8, D106

**(S10353 AS)**

ULC

Underwriters Laboratories of Canada

7 Underwriters Road

Toronto, Ontario, Canada M1R3B4

Standard Referenced
reference in code
number Title section number

CAN/ULC S 102.2—20~~10~~18 Standard Method of Test for Surface Burning Characteristics of Flooring,
  Floor Coverings and Miscellaneous Materials and Assemblies—~~with 2000 Revisions~~ 720.2, 720.3,

720.4

USC

United States Code

c/o Superintendent of Documents

U.S. Government Printing Office

732 North Capitol Street NW

Washington, DC 20401

Standard Referenced
reference in code
number Title section number

18 USC Part 1, Ch.40 Importation, Manufacture, Distribution and Storage of Explosive Materials 202

WCLIB

West Coast Lumber Inspection Bureau

P. O. Box 23145

Portland, OR 97281

Standard Referenced
reference in code
number Title section number

AITC 104—03 Typical Construction Details 2306.1

AITC 110—01 Standard Appearance Grades for Structural Glued Laminated Timber 2306.1

AITC 113—10 Standard for Dimensions of Structural Glued Laminated Timber 2306.1

AITC 117—10 Standard Specifications for Structural Glued Laminated Timber of Softwood Species 2306.1

AITC 119—96 Standard Specifications for Structural Glued Laminated Timber of Hardwood Species 2306.1

AITC 200—09 Manufacturing Quality Control Systems Manual for Structural Glued Laminated Timber 2306.1

WDMA

Window and Door Manufacturers Association

2025 M Street, NW Suite 800

Washington, DC 20036-3309

Standard Referenced
reference in code
number Title section number

AAMA/WDMA/CSA
101/I.S.2/A440—08 or 11 or 17 Specifications for Windows, Doors and Unit Skylights 1010.1.7, 1709.5.1, 2405.5, 2411.3.2

WDMA I.S.11-2018, Industry Standard Analytical Method for Design Pressure (DP) Ratings of Fenestration Products..............1709.5.1

(S10417 AS)

FMA/AAMA/WDMA 2710-20, Guidelines for the Full Frame Replacement of Windows without Removal of External Brick Veneer............1405.4

**(S10391 AM)**

WRI

Wire Reinforcement Institute, Inc.

942 Main Street, Suite 300

Hartford, CT 06103

Standard Referenced
reference in code
number Title section number

WRI/CRSI—81 Design of Slab-on-ground Foundations—with 1996 Update 1808.6.2

**(S9124 / ADM47-16 AS)**