|  |  |  |  |
| --- | --- | --- | --- |
| **MECHANICAL**  **TAC ACTION/Votes**  **Local Technical amendments**  **to the**  **2023 8th Edition Florida Building Code** | | | |
|  |  |  |  |
| JURISDICTION | DOCUMENT with TECHNICAL AMENDMENT | SUMMARY OF TECHNICAL AMENDMENT | TAC ACTION/VOTE |
|  |  |  |  |
| Broward County  Pg 1 | FBC  Mechanical  307.2.1/Exception | Local Amendment regarding condensate disposal. | Locke Motion to Deny  2nd Cochelle  Vote: 8 Yes – 0 No |
|  |  |  |  |
| Broward County  Pg. 2 | FBC  Mechanical  908.3.1 | Local Amendment regarding location of cooling tower loccations. | Locke Motion to Deny  2nd Cochelle  Vote: 8 Yes – 0 No |
|  |  |  |  |
| Broward County  Pg. 3 | FBC  Mechanical  908.8/Exception | Local Amendment regarding existing cooling tower exemptions and new cooling tower and evaporative condenser shall be operated with conductivity controllers and make up and blowdown meters and shall achieve a min of 8 cycles. | Locke Motion to Deny  2nd Cochelle  Vote: 8 Yes – 0 No |
|  |  |  |  |
| Pinellas County Construction Industry Licensing Board  (PCCILB)  Pg 5 | FBC  Mechanical  M1411.3 | Local Amendment regarding insulation of condensate drain lines. | Locke Motion to Deny  2nd Cochelle  Vote: 8 Yes – 0 No |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |